Offline HP Array Configuration Utility Image
Version 9.10.22.0
4/20/2012


Description
-----------

   The Offline HP Array Configuration Utility provides an ISO image that can be
   burned to a CD/DVD, or flashed to a USB memory key using the HP USB Key Utility 
   for Windows
   (http://h20000.www2.hp.com/bizsupport/TechSupport/SoftwareDescription.jsp?lang=en&cc=US&swItem=MTX-eee9b3632ced47478f9ef85d43&mode=5)
   



Support
-------
Supported Controllers

  Smart Array products:
     Smart Array 5312 Controller
     Smart Array 5302 Controller
     Smart Array 5304 Controller
     Smart Array 532 Controller
     Smart Array 5i Controller  
     Smart Array 641 Controller
     Smart Array 642 Controller
     Smart Array 6400 Controller
     Smart Array 6400 EM Controller
     Smart Array 6i Controller
     Smart Array P600 Controller
     Smart Array P400 Controller
     Smart Array P400i Controller
     Smart Array E200 Controller
     Smart Array E200i Controller
     Smart Array P800 Controller
     Smart Array E500 Controller
     Smart Array P700m Controller
     Smart Array P410i Controller
     Smart Array P411 Controller
     Smart Array P212 Controller
     Smart Array P712m Controller
     Smart Array B110i SATA RAID
     Smart Array P812 Controller
     Smart Array P220i Controller
     Smart Array P222 Controller
     Smart Array P420 Controller
     Smart Array P420i Controller
     Smart Array P421 Controller
     Dynamic Smart Array B320i RAID
     Dynamic Smart Array B120i RAID

  MSA products:
     MSA500 Controller
     MSA500 G2 Controller
     MSA1000 Controller     
     MSA1500 CS Controller
     MSA20 Controller  

  

 For additional support information go to:
 http://www.hp.com/products1/serverconnectivity/support_matrices.html#linux


Installing & Running the Offline HP Array Configuration Utility 
--------------------------------------------------------------

Burn/write the ISO image to the desired media (CD/DVD/USB Key).  Insert the media
into the server and boot the server.  Verify that your system can boot from the
desired media. 

A menu with the three boot options (ACU, ACUCLI, HPACUSCRIPTING) is shown.  
The user can manually select which utility to start; or if no selection is made, 
ACU is automatically started.

This image is a bootable environment that immediately starts ACU to allow
configuration of storage.

This ISO image can also be mounted as a CD image through ILO2.  It is highly
recommended that your server have the latest BIOS firmware and latest ILO2 
firmware installed.

This utility provides the following boot options:
   *   The web based Array Configuration Utility (ACU)
   *   The command line Array Configuration Utility (ACUCLI)
   *   The command line Array Configuration Scripting Utility (HPACUSCRIPTING)



Feedback
--------

  For support for Offline HP Array Configuration Utility or Smart Array controllers, 
  please visit the web at http://support.hp.com.

  For feedback or suggestions on the Offline HP Array Configuration Utility, 
  please send comments to acu@hp.com. Please note that support cannot be provided through this address.


