<map id="G" name="G">
<area shape="rect" id="node27" href="$structlmacdesc.html" title="Descriptor filled by the LMAC." alt="" coords="1285,1909,1384,2046"/>
<area shape="rect" id="node2" href="$structco__list.html" title="structure of a list" alt="" coords="1061,853,1125,955"/>
<area shape="rect" id="node4" href="$structco__list__hdr.html" title="structure of a list element header" alt="" coords="1092,200,1185,285"/>
<area shape="rect" id="node13" href="$structtxdesc.html" title="LMAC Tx Descriptor." alt="" coords="1015,2209,1097,2346"/>
<area shape="rect" id="node45" href="$structbfr__mem__node.html" title="Structure representing a piece of BFR memory." alt="" coords="1588,1144,1711,1333"/>
<area shape="rect" id="node7" href="$structtx__policy__tbl.html" title="Policy Table Structure used to store Policy Table Information used by MAC HW to prepare..." alt="" coords="327,809,457,999"/>
<area shape="rect" id="node21" href="$structtxl__buffer__control.html" title="Control descriptor containing information about the transmission rates to use, the..." alt="" coords="157,1470,307,1642"/>
<area shape="rect" id="node9" href="$structtx__hd.html" title="Definition of a TX header descriptor." alt="" coords="1200,688,1363,1120"/>
<area shape="rect" id="node39" href="$structtx__hw__desc.html" title="Definition of a TX confirmation descriptor." alt="" coords="1308,1496,1412,1616"/>
<area shape="rect" id="node11" href="$structba__ssc__bitmap.html" title="Structure of generic BA SSC + bitmap." alt="" coords="644,853,764,955"/>
<area shape="rect" id="node29" href="$structtxl__buffer__tag.html" title="Buffer header structure." alt="" coords="1268,2421,1401,2680"/>
<area shape="rect" id="node15" href="$structhostdesc.html" title="Descriptor filled by the Host." alt="" coords="5,336,160,664"/>
<area shape="rect" id="node17" href="$structmac__addr.html" title="MAC address structure." alt="" coords="197,5,283,91"/>
<area shape="rect" id="node52" href="$structmac__hdr__ctrl.html" title="Structure of a long control frame MAC header." alt="" coords="277,174,387,311"/>
<area shape="rect" id="node19" href="$structumacdesc.html" title="Descriptor filled by the UMAC." alt="" coords="512,1822,645,2133"/>
<area shape="rect" id="node24" href="$structtx__compressed__policy__tbl.html" title="Compressed Policy Table Structure used to store Policy Table Information used by..." alt="" coords="108,853,303,955"/>
<area shape="rect" id="node32" href="$structdma__desc.html" title="Element in the pool of TX DMA bridge descriptors." alt="" coords="1525,827,1616,981"/>
<area shape="rect" id="node34" href="$structtx__pbd.html" title="Definition of a TX payload buffer descriptor." alt="" coords="1601,2200,1721,2355"/>
<area shape="rect" id="node43" href="$structtx__cfm__tag.html" title="Structure indicating the status and other information about the transmission." alt="" coords="1387,809,1501,999"/>
<area shape="rect" id="node50" href="$structbar__frame.html" title="Structure of a Block Acknowledgment Request frame." alt="" coords="481,844,620,964"/>
<area shape="rect" id="node55" href="$structba__ssc__bitmap__256.html" title="Structure of BA SSC + 256&#45;bit bitmap." alt="" coords="788,853,940,955"/>
</map>
