# rx_cntrl_pm_mon Struct Reference
[RXU]

Structure used for Duplicate Filtering of packet received on unregistered STA. More...

`#include <rxu_cntrl.h>`

Collaboration diagram for rx_cntrl_pm_mon:
[legend]

## Data Fields
struct mac_addr | addr
| Source address that we monitor.
uint8_t | pm_state
| PM state of the device we monitor.
bool | mon
| Flag indicating if the monitoring is enabled or not.

## Detailed Description

Structure used for Duplicate Filtering of packet received on unregistered STA.

Definition at line 300 of file rxu_cntrl.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/rxu/rxu_cntrl.h