# rxu_mgt_ind Struct Reference

Parameters of the RXU_MGT_IND message. More...

`#include <rxu_task.h>`

## Data Fields
uint16_t | length
| Length of the frame.
uint16_t | framectrl
| Frame control field of the frame.
uint16_t | center_freq
| Center frequency on which we received the packet.
uint8_t | band
| PHY band.
uint8_t | sta_idx
| Index of the station that sent the frame. 0xFF if unknown.
uint8_t | inst_nbr
| Index of the VIF that received the frame. 0xFF if unknown.
int8_t | rssi
| RSSI of the received frame.
uint32_t | payload []
| Frame payload.

## Detailed Description

Parameters of the RXU_MGT_IND message.

Definition at line 35 of file rxu_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/rxu/rxu_task.h