# MAC
[MACSW]

Common MAC types, defines and utils functions. More...

Collaboration diagram for MAC:

## Data Structures
struct | mac_frame
| MAC Frame structure. More...
struct | key_info_tag
| Structure containing the information about a key. More...
struct | mac_htoprnelmt
| MAC HT operation element. More...
struct | mac_mu_edca_param_set
| MU EDCA Parameter Set Element. More...
struct | mac_edca_param_set
| EDCA Parameter Set Element. More...
struct | mac_hdr_ctrl_short
| Structure of a short control frame MAC header. More...
struct | mac_hdr_ctrl
| Structure of a long control frame MAC header. More...
struct | mac_hdr
| Structure of a Data/Management frame MAC header. More...
struct | mac_hdr_qos
| Structure of a QoS Data frame MAC header. More...
struct | mac_hdr_qos_htc
| Structure of a QoS Data + HTC frame MAC header. More...
struct | mac_hdr_long
| Structure of a 4-address Data frame MAC header. More...
struct | mac_hdr_long_qos
| Structure of a 4-address QoS Data frame MAC header. More...
struct | mac_eth_hdr
| Structure of Ethernet Header. More...
struct | bcn_frame
| Structure of a Beacon or ProbeRsp frame. More...
struct | preq_frame
| Structure of a Probe Request frame. More...
struct | bar_frame
| Structure of a Block Acknowledgment Request frame. More...
struct | ba_base
| Base structure of a Block Acknowledgment frame. More...
struct | ba_ssc_bitmap
| Structure of generic BA SSC + bitmap. More...
struct | ba_ssc_bitmap_32
| Structure of BA SSC + 32-bit bitmap. More...
struct | ba_ssc_bitmap_64
| Structure of BA SSC + 64-bit bitmap. More...
struct | ba_ssc_bitmap_128
| Structure of BA SSC + 128-bit bitmap. More...
struct | ba_ssc_bitmap_256
| Structure of BA SSC + 256-bit bitmap. More...
struct | ba_msta_aid_tid_info
| Multi-STA AID/TID info field. More...
struct | ba_comp_frame
| Structure of a Compressed Block Acknowledgment frame. More...
struct | amsdu_hdr
| Structure of A-MSDU Header. More...
struct | he_basic_trigger_user_info
| Structure of the User Info part of the HE Basic Trigger frame. More...
struct | he_user_info_base
| Base part of the User Info field present in the HE trigger frames. More...
struct | he_trigger_base
| Base structure of a HE Trigger frame. More...
struct | mac_addr
| MAC address structure. More...
struct | mac_ssid
| SSID. More...
struct | mac_chan_def
| Primary Channel definition. More...
struct | mac_chan_op
| Operating Channel. More...
struct | mac_scan_result
| Scan result element, parsed from beacon or probe response frames. More...
struct | mac_rateset
| Structure containing the legacy rateset of a station. More...
struct | mac_sec_key
| Structure defining a security key. More...
struct | mac_htcapability
| MAC HT capability information element. More...
struct | mac_vhtcapability
| MAC VHT capability information element. More...
struct | mac_he_mcs_nss_supp
| Structure listing the per-NSS, per-BW supported MCS combinations. More...
struct | mac_hecapability
| MAC HE capability information element. More...
## Defines
#define | TU_DURATION 1024
| duration of a Time Unit in microseconds
#define | MAC_BASIC_RATE 0x80
| Mask to test if it's a basic rate - BIT(7).
#define | WORD_ALIGN 3
| Mask for extracting/checking word alignment.
#define | MAC_ADDR_CMP(addr1_ptr, addr2_ptr)
| Compare two MAC addresses.
#define | MAC_ADDR_CMP_PACKED(__a1, __a2) (memcmp(__a1, __a2, MAC_ADDR_LEN) == 0)
| Compare two MAC addresses whose alignment is not known.
#define | MAC_ADDR_CPY(addr1_ptr, addr2_ptr)
| Copy a MAC address.
#define | MAC_SSID_CMP(ssid1_ptr, ssid2_ptr)
| Compare two SSID.
#define | MAC_ADDR_GROUP(mac_addr_ptr) ((*((uint8_t *)(mac_addr_ptr))) & 1)
| Check if MAC address is a group address: test the multicast bit.
#define | MAC_FRAME_LEN 512
| Maximum size of the frame body for frames that are internally carried.
#define | MAC_DEFAULT_KEY_COUNT 4
| Max number of default keys for given VIF.
#define | MAC_DEFAULT_MFP_KEY_COUNT 6
| Max number of MFP key for given VIF.
#define | MAC_QOS_INFO_STA_UAPSD_ENABLED_VO CO_BIT(0)
| UAPSD enabled on VO.
#define | MAC_QOS_INFO_STA_UAPSD_ENABLED_VI CO_BIT(1)
| UAPSD enabled on VI.
#define | MAC_QOS_INFO_STA_UAPSD_ENABLED_BK CO_BIT(2)
| UAPSD enabled on BK.
#define | MAC_QOS_INFO_STA_UAPSD_ENABLED_BE CO_BIT(3)
| UAPSD enabled on BE.
#define | MAC_QOS_INFO_STA_UAPSD_ENABLED_ALL 0x0F
| UAPSD enabled on all access categories.
#define | MAC_QOS_INFO_AP_UAPSD_ENABLED CO_BIT(7)
| UAPSD enabled in AP.
#define | MAC_PROT_NONERP_PRESENT_BIT CO_BIT(0)
| Non-ERP stations are present.
#define | MAC_PROT_USE_PROTECTION_BIT CO_BIT(1)
| ERP protection shall be used.
#define | MAC_PROT_BARKER_PREAMB_BIT CO_BIT(2)
| Barker preamble protection shall be used.
#define | MAC_PROT_ERP_STATUS_MASK
| ERP protection status mask.
#define | HE_MAC_CAPA_VAL_GET(he_cap, field)
| Get the value of a bit field in the HE MAC capability element.
#define | HE_MAC_CAPA_VAL_SET(he_cap, field, val)
| Set the value of a bit field in the HE MAC capability element.
#define | HE_MAC_CAPA_BIT_IS_SET(he_cap, bit)
| Test if a bit in the HE MAC capability element is set.
#define | HE_MAC_CAPA_BIT_SET(he_cap, bit)
| Set a bit in the HE MAC capability element.
#define | HE_MAC_CAPA_BIT_CLR(he_cap, bit)
| Clear a bit in the HE MAC capability element.
#define | HE_PHY_CAPA_VAL_GET(he_cap, field)
| Get the value of a bit field in the HE PHY capability element.
#define | HE_PHY_CAPA_VAL_SET(he_cap, field, val)
| Set the value of a bit field in the HE PHY capability element.
#define | HE_PHY_CAPA_BIT_IS_SET(he_cap, bit)
| Test if a bit in the HE PHY capability element is set.
#define | HE_PHY_CAPA_BIT_SET(he_cap, bit)
| Set a bit in the HE PHY capability element.
#define | HE_PHY_CAPA_BIT_CLR(he_cap, bit)
| Clear a bit in the HE PHY capability element.
#define | MAC_ADDR_LEN 6
| MAC address length in bytes.
#define | MAC_SSID_LEN 32
| SSID maximum length.
#define | MAC_DOMAINCHANNEL_24G_MAX 14
| max number of channels in the 2.4 GHZ band
#define | MAC_DOMAINCHANNEL_5G_MAX 28
| max number of channels in the 5 GHZ band
#define | MAC_RATESET_LEN 12
| MAC rateset maximum length.
#define | MAC_SEC_KEY_LEN 32
| MAC Security Key maximum length.
#define | MAX_MCS_LEN 16
| MCS bitfield maximum size (in bytes).
#define | MAC_HE_MAC_CAPA_LEN 6
| Length (in bytes) of the MAC HE capability field.
#define | MAC_HE_PHY_CAPA_LEN 11
| Length (in bytes) of the PHY HE capability field.
#define | MAC_HE_PPE_THRES_MAX_LEN 25
| Maximum length (in bytes) of the PPE threshold data.
#define | __PACKED __attribute__ ((__packed__))
| Pack a structure field.
## Enumerations
enum | mac_vif_type { VIF_STA, VIF_IBSS, VIF_AP, VIF_MESH_POINT, VIF_MONITOR, VIF_UNKNOWN }
| Interface types. More...
enum | mac_bss_type { INFRASTRUCTURE_MODE = 1, INDEPENDENT_BSS_MODE, ANY_BSS_MODE }
| BSS type.
enum | mac_chan_band { PHY_BAND_2G4, PHY_BAND_5G, PHY_BAND_MAX }
| Channel Band. More...
enum | mac_chan_bandwidth { PHY_CHNL_BW_20, PHY_CHNL_BW_40, PHY_CHNL_BW_80, PHY_CHNL_BW_160, PHY_CHNL_BW_80P80, PHY_CHNL_BW_OTHER }
| Operating Channel Bandwidth. More...
enum | mac_chan_flags { CHAN_NO_IR = CO_BIT(0), CHAN_DISABLED = CO_BIT(1), CHAN_RADAR = CO_BIT(2) }
| Channel Flag. More...
enum | mac_cipher_suite { MAC_CIPHER_WEP40 = 0, MAC_CIPHER_TKIP = 1, MAC_CIPHER_CCMP = 2, MAC_CIPHER_WEP104 = 3, MAC_CIPHER_WPI_SMS4 = 4, MAC_CIPHER_BIP_CMAC_128 = 5, MAC_CIPHER_GCMP_128, MAC_CIPHER_GCMP_256, MAC_CIPHER_CCMP_256, MAC_CIPHER_BIP_GMAC_128, MAC_CIPHER_BIP_GMAC_256, MAC_CIPHER_BIP_CMAC_256, MAC_CIPHER_INVALID = 0xFF }
| Cipher suites (order is important as it is used by MACHW). More...
enum | mac_akm_suite { MAC_AKM_NONE, MAC_AKM_PRE_RSN, MAC_AKM_8021X, MAC_AKM_PSK, MAC_AKM_FT_8021X, MAC_AKM_FT_PSK, MAC_AKM_8021X_SHA256, MAC_AKM_PSK_SHA256, MAC_AKM_TDLS, MAC_AKM_SAE, MAC_AKM_FT_OVER_SAE, MAC_AKM_8021X_SUITE_B, MAC_AKM_8021X_SUITE_B_192, MAC_AKM_FILS_SHA256, MAC_AKM_FILS_SHA384, MAC_AKM_FT_FILS_SHA256, MAC_AKM_FT_FILS_SHA384, MAC_AKM_OWE, MAC_AKM_WAPI_CERT, MAC_AKM_WAPI_PSK }
| Authentication and Key Management suite. More...
enum | mac_legacy_rates { MAC_RATE_1MBPS = 2, MAC_RATE_2MBPS = 4, MAC_RATE_5_5MBPS = 11, MAC_RATE_6MBPS = 12, MAC_RATE_9MBPS = 18, MAC_RATE_11MBPS = 22, MAC_RATE_12MBPS = 24, MAC_RATE_18MBPS = 36, MAC_RATE_24MBPS = 48, MAC_RATE_36MBPS = 72, MAC_RATE_48MBPS = 96, MAC_RATE_54MBPS = 108 }
| Legacy rate 802.11 definitions. More...
enum | mac_bss_membership { MAC_BSS_MEMBERSHIP_HT_PHY = 127, MAC_BSS_MEMBERSHIP_VHT_PHY = 126 }
| BSS Membership Selector definitions. More...
enum | mac_ac { AC_BK = 0, AC_BE, AC_VI, AC_VO, AC_MAX }
| Access Category enumeration. More...
enum | mac_tid { TID_0, TID_1, TID_2, TID_3, TID_4, TID_5, TID_6, TID_7, TID_MGT, TID_MAX }
| Traffic ID enumeration. More...
enum | mac_sta_flags { STA_QOS_CAPA = CO_BIT(0), STA_HT_CAPA = CO_BIT(1), STA_VHT_CAPA = CO_BIT(2), STA_MFP_CAPA = CO_BIT(3), STA_OPMOD_NOTIF = CO_BIT(4), STA_HE_CAPA = CO_BIT(5) }
| Station flags. More...
enum | mac_connection_flags { CONTROL_PORT_HOST = CO_BIT(0), CONTROL_PORT_NO_ENC = CO_BIT(1), DISABLE_HT = CO_BIT(2), WPA_WPA2_IN_USE = CO_BIT(3), MFP_IN_USE = CO_BIT(4) }
| Connection flags. More...
## Functions
uint32_t | mac_paid_gid_sta_compute (struct mac_addr const *mac_addr)
| Compute the PAID/GID to be put in the THD for frames that need to be sent to an AP or a Mesh peer.
uint32_t | mac_paid_gid_ap_compute (struct mac_addr const *mac_addr, uint16_t aid)
| Compute the PAID/GID to be put in the THD for frames that need to be sent to a STA connected to an AP or a TDLS peer.
enum mac_akm_suite | mac_akm_suite_value (uint32_t akm_suite)
| Convert IEE802.11 AKM suite into enum mac_akm_suite.
enum mac_cipher_suite | mac_cipher_suite_value (uint32_t cipher_suite)
| Convert IEE802.11 Cipher suite into enum mac_cipher_suite.
__INLINE bool | mac_nontxed_bssid_get (uint8_t bssid_index, uint8_t max_bssid_ind, struct mac_addr const *ref_bssid, struct mac_addr *bssid)
| Get the value of the nonTransmitted BSSID, based on the reference BSSID, the nonTransmitted BSSID index and the Maximum BSSID indicator.
__INLINE void | mac_ref_bssid_get (uint8_t bssid_index, uint8_t max_bssid_ind, struct mac_addr const *bssid, struct mac_addr *ref_bssid)
| Get the value of the refernec BSSID, based on the nonTransmitted BSSID, the nonTransmitted BSSID index and the Maximum BSSID indicator.
static uint32_t | mac_ie_find (uint32_t addr, uint16_t buflen, uint8_t ie_id, uint16_t *len)
| Find an information element in the variable part of a management frame body.
static uint32_t | mac_ext_ie_find (uint32_t addr, uint16_t buflen, uint8_t ext_ie_id, uint16_t *len)
| Find an extended information element in the variable part of a management frame body.
static uint32_t | mac_vsie_find (uint32_t addr, uint16_t buflen, uint8_t const *oui, uint8_t ouilen, uint16_t *len)
| Find a vendor specific information element in the variable part of a management frame body.
uint32_t | mac_ie_rates_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the Supported Rates element in a frame buffer.
uint32_t | mac_ie_ext_rates_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the Extended Supported Rates element in a frame buffer.
uint32_t | mac_ie_ssid_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the SSID element in a frame buffer.
uint32_t | mac_ie_country_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the Country element in a frame buffer.
uint32_t | mac_ie_rsn_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the RSN element in a frame buffer.
uint32_t | mac_ie_wpa_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the WPA element in a frame buffer.
uint32_t | mac_ie_wapi_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the WAPI element in a frame buffer.
uint32_t | mac_ie_mesh_id_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the Mesh ID element in a frame buffer.
uint32_t | mac_ie_mesh_peer_mgmt_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the Mesh Peering Management element in a frame buffer.
uint32_t | mac_ie_mesh_awake_win_find (uint32_t buffer, uint16_t buflen)
| Search for the Mesh Awake Window element in a frame buffer.
uint32_t | mac_ie_mesh_conf_find (uint32_t buffer, uint16_t buflen)
| Search for the Mesh Configuration element in a frame buffer.
uint32_t | mac_ie_tim_find (uint32_t buffer, uint16_t buflen)
| Search for the TIM element in a frame buffer.
uint32_t | mac_ie_csa_find (uint32_t buffer, uint16_t buflen)
| Search for the Channel Switch Announcement element in a frame buffer.
uint32_t | mac_ie_ecsa_find (uint32_t buffer, uint16_t buflen)
| Search for the Extended Channel Switch Announcement element in a frame buffer.
uint32_t | mac_ie_sec_chnl_offset_find (uint32_t buffer, uint16_t buflen, bool *valid_len)
| Search for the Secondary Channel Offset element in a frame buffer.
uint32_t | mac_ie_wide_bw_chnl_find (uint32_t buffer, uint16_t buflen, bool *valid_len)
| Search for the Wide Bandwidth Channel sub-element in a frame buffer.
uint32_t | mac_ie_ds_find (uint32_t buffer, uint16_t buflen)
| Search for the DS element in a frame buffer.
uint32_t | mac_ie_mgmt_mic_find (uint32_t buffer, uint16_t buflen)
| Search for the Management MIC element in a frame buffer.
uint32_t | mac_ie_qos_capa_find (uint32_t buffer, uint16_t buflen)
| Search for the QoS Capability element in a frame buffer.
uint32_t | mac_ie_erp_find (uint32_t buffer, uint16_t buflen)
| Search for the ERP element in a frame buffer.
uint32_t | mac_ie_op_mode_notif_find (uint32_t buffer, uint16_t buflen)
| Search for the Operating Mode Notification element in a frame buffer.
uint32_t | mac_ie_power_constraint_find (uint32_t buffer, uint16_t buflen)
| Search for the Power Constraint element in a frame buffer.
uint32_t | mac_ie_mde_find (uint32_t buffer, uint16_t buflen)
| Search for the MDE element in a frame buffer.
uint32_t | mac_ie_wmm_param_find (uint32_t buffer, uint16_t buflen)
| Search for the WMM parameter element in a frame buffer.
uint32_t | mac_ie_ht_capa_find (uint32_t buffer, uint16_t buflen)
| Search for the HT capability element in a frame buffer.
uint32_t | mac_ie_multi_bssid_find (uint32_t buffer, uint16_t buflen)
| Search for the Multiple BSSID element in a frame buffer.
uint32_t | mac_ie_sub_non_txed_bssid_find (uint32_t buffer, uint16_t buflen)
| Search for the nonTransmitted BSSID profile sub-element in a frame buffer.
uint32_t | mac_ie_non_txed_bssid_capa_find (uint32_t buffer, uint16_t buflen)
| Search for the nonTransmitted BSSID capability element in a frame buffer.
uint32_t | mac_ie_multi_bssid_index_find (uint32_t buffer, uint16_t buflen)
| Search for the nonTransmitted BSSID index element in a frame buffer.
uint32_t | mac_ie_vht_capa_find (uint32_t buffer, uint16_t buflen)
| Search for the VHT capability element in a frame buffer.
uint32_t | mac_ie_he_capa_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the HE capability element in a frame buffer.
uint32_t | mac_ie_ht_oper_find (uint32_t buffer, uint16_t buflen)
| Search for the HT operation element in a frame buffer.
uint32_t | mac_ie_vht_oper_find (uint32_t buffer, uint16_t buflen)
| Search for the VHT operation element in a frame buffer.
uint32_t | mac_ie_he_oper_find (uint32_t buffer, uint16_t buflen, uint8_t *ie_len)
| Search for the HE operation element in a frame buffer.
uint32_t | mac_ie_mu_edca_find (uint32_t buffer, uint16_t buflen)
| Search for the MU EDCA element in a frame buffer.
uint32_t | mac_ie_uora_find (uint32_t buffer, uint16_t buflen)
| Search for the UORA element in a frame buffer.
__INLINE uint16_t | mac_ie_len (uint32_t addr)
| Compute the total length of an information element.
## Variables
const uint8_t | mac_tid2ac [TID_MAX]
| Array converting a TID to its associated AC.
const uint8_t | mac_ac2uapsd [AC_MAX]
| Array converting an AC to its corresponding bit in the QoS Information field.
const uint8_t | mac_aci2ac [AC_MAX]
| Array converting an ACI to its corresponding AC. See Table 9-136 in 802.11-2016.
const uint8_t | mac_ac2aci [AC_MAX]
| Array converting an AC to its corresponding ACI. See Table 9-136 in 802.11-2016.
const uint8_t | mac_id2rate [MAC_RATESET_LEN]
| Array converting a MAC HW rate id into its corresponding standard rate value.
struct mac_addr | mac_addr_bcst = {{0xFFFF, 0xFFFF, 0xFFFF}}
| Constant value corresponding to the Broadcast MAC address.
const uint8_t | mac_tid2ac []
| Array converting a TID to its associated AC.
const uint8_t | mac_ac2uapsd []
| Array converting an AC to its corresponding bit in the QoS Information field.
const uint8_t | mac_aci2ac []
| Array converting an ACI to its corresponding AC. See Table 9-136 in 802.11-2016.
const uint8_t | mac_ac2aci []
| Array converting an AC to its corresponding ACI. See Table 9-136 in 802.11-2016.
const uint8_t | mac_id2rate []
| Array converting a MAC HW rate id into its corresponding standard rate value.
struct mac_addr | mac_addr_bcst
| Constant value corresponding to the Broadcast MAC address.
struct mac_hdr_ctrl_short | __PACKED
| Structure of a short control frame MAC header.
## Information Element offsets, lengths and other definitions
enum | mac_ht_oper_prot_val { MAC_HT_OPER_PROT_NO_PROT = 0, MAC_HT_OPER_PROT_NONMEMBER, MAC_HT_OPER_PROT_20MHZ, MAC_HT_OPER_PROP_NON_HT_MIXED }
| 802.11 information element definition
#define | MAC_LEN_OFT 1
| 802.11 information element definition
#define | MAC_SSID_ID_OFT 0
| 802.11 information element definition
#define | MAC_SSID_LEN_OFT 1
| 802.11 information element definition
#define | MAC_SSID_SSID_OFT 2
| 802.11 information element definition
#define | MAC_SSID_MAX_LEN (MAC_SSID_LEN + 2)
| 802.11 information element definition
#define | MAC_RATES_ID_OFT 0
| 802.11 information element definition
#define | MAC_RATES_LEN_OFT 1
| 802.11 information element definition
#define | MAC_RATES_RATES_OFT 2
| 802.11 information element definition
#define | MAC_RATES_ELMT_MAX_LEN 8
| 802.11 information element definition
#define | MAC_RATES_MAX_LEN 10
| 802.11 information element definition
#define | MAC_RATES_MIN_LEN 3
| 802.11 information element definition
#define | MAC_FH_ID_OFT 0
| 802.11 information element definition
#define | MAC_FH_LEN_OFT 1
| 802.11 information element definition
#define | MAC_FH_DWELL_OFT 2
| 802.11 information element definition
#define | MAC_FH_HOP_SET_OFT 4
| 802.11 information element definition
#define | MAC_FH_HOP_PAT_OFT 5
| 802.11 information element definition
#define | MAC_FH_HOP_IDX_OFT 6
| 802.11 information element definition
#define | MAC_FH_PARAM_LEN 7
| 802.11 information element definition
#define | MAC_DS_ID_OFT 0
| 802.11 information element definition
#define | MAC_DS_LEN_OFT 1
| 802.11 information element definition
#define | MAC_DS_CHANNEL_OFT 2
| 802.11 information element definition
#define | MAC_DS_PARAM_LEN 3
| 802.11 information element definition
#define | MAC_CF_ID_OFT 0
| 802.11 information element definition
#define | MAC_CF_LEN_OFT 1
| 802.11 information element definition
#define | MAC_CF_COUNT_OFT 2
| 802.11 information element definition
#define | MAC_CF_PERIOD_OFT 3
| 802.11 information element definition
#define | MAC_CF_MAX_DUR_OFT 4
| 802.11 information element definition
#define | MAC_CF_REM_DUR_OFT 6
| 802.11 information element definition
#define | MAC_CF_PARAM_LEN 8
| 802.11 information element definition
#define | MAC_TIM_ID_OFT 0
| 802.11 information element definition
#define | MAC_TIM_LEN_OFT 1
| 802.11 information element definition
#define | MAC_TIM_CNT_OFT 2
| 802.11 information element definition
#define | MAC_TIM_PERIOD_OFT 3
| 802.11 information element definition
#define | MAC_TIM_BMPC_OFT 4
| 802.11 information element definition
#define | MAC_TIM_BMP_OFT 5
| 802.11 information element definition
#define | MAC_TIM_MIN_LEN 6
| 802.11 information element definition
#define | MAC_TIM_MAX_LEN (5 + MAC_TIM_SIZE)
| 802.11 information element definition
#define | MAC_TIM_BCMC_PRESENT CO_BIT(0)
| 802.11 information element definition
#define | MAC_IBSS_ID_OFT 0
| 802.11 information element definition
#define | MAC_IBSS_LEN_OFT 1
| 802.11 information element definition
#define | MAC_IBSSATIM_OFT 2
| 802.11 information element definition
#define | MAC_IBSS_PARAM_LEN 4
| 802.11 information element definition
#define | MAC_COUNTRY_ID_OFT 0
| 802.11 information element definition
#define | MAC_COUNTRY_LEN_OFT 1
| 802.11 information element definition
#define | MAC_COUNTRY_MIN_LEN 8
| 802.11 information element definition
#define | MAC_COUNTRY_STRING_OFT 2
| 802.11 information element definition
#define | MAC_COUNTRY_STRING_LEN 3
| 802.11 information element definition
#define | MAC_COUNTRY_FIRST_CHAN_OFT 0
| 802.11 information element definition
#define | MAC_COUNTRY_NB_CHAN_OFT 1
| 802.11 information element definition
#define | MAC_COUNTRY_PWR_LEVEL_OFT 2
| 802.11 information element definition
#define | MAC_COUNTRY_TRIPLET_LEN 3
| 802.11 information element definition
#define | MAC_CHALLENGE_ID_OFT 0
| 802.11 information element definition
#define | MAC_CHALLENGE_LEN_OFT 1
| 802.11 information element definition
#define | MAC_CHALLENGE_TEXT_OFT 2
| 802.11 information element definition
#define | MAC_ERP_ID_OFT 0
| 802.11 information element definition
#define | MAC_ERP_LEN_OFT 1
| 802.11 information element definition
#define | MAC_ERP_PARAM_OFT 2
| 802.11 information element definition
#define | MAC_ERP_LEN 3
| 802.11 information element definition
#define | MAC_ERP_NON_ERP_PRESENT CO_BIT(0)
| 802.11 information element definition
#define | MAC_ERP_USE_PROTECTION CO_BIT(1)
| 802.11 information element definition
#define | MAC_ERP_BARKER_PREAMBLE_MODE CO_BIT(2)
| 802.11 information element definition
#define | MAC_ERP_IE_PRESENT CO_BIT(7)
| 802.11 information element definition
#define | MAC_RSNIE_ID_OFT 0
| 802.11 information element definition
#define | MAC_RSNIE_LEN_OFT 1
| 802.11 information element definition
#define | MAC_RSNIE_INFO_OFT 2
| 802.11 information element definition
#define | MAC_RSNIE_VERSION_OFT 2
| 802.11 information element definition
#define | MAC_RSNIE_GROUP_CIPHER_OFT 4
| 802.11 information element definition
#define | MAC_RSNIE_PAIRWISE_CIPHER_SUITE_CNT_OFT 8
| 802.11 information element definition
#define | MAC_RSNIE_PAIRWISE_CIPHER_SUITE_LIST_OFT 10
| 802.11 information element definition
#define | MAC_RSNIE_PAIRWISE_CIPHER_SIZE 4
| 802.11 information element definition
#define | MAC_RSNIE_KEY_MANAGEMENT_SUITE_CNT_OFT 14
| 802.11 information element definition
#define | MAC_RSNIE_KEY_MANAGEMENT_SUITE_LIST_OFT 16
| 802.11 information element definition
#define | MAC_RSNIE_KEY_MANAGEMENT_SIZE 4
| 802.11 information element definition
#define | MAC_RSNIE_RSN_CAPABILITIES_OFT 20
| 802.11 information element definition
#define | MAC_RSNIE_RSN_PMKID_COUNT_OFT 22
| 802.11 information element definition
#define | MAC_RSNIE_RSN_PMKID_COUNT_LIST_OFT 24
| 802.11 information element definition
#define | MAC_RSNIE_RSN_PMKID_SIZE 16
| 802.11 information element definition
#define | MAC_RSNIE_MIN_LEN 20
| 802.11 information element definition
#define | MAC_WPA_ID_OFT 0
| 802.11 information element definition
#define | MAC_WPA_LEN_OFT 1
| 802.11 information element definition
#define | MAC_WPA_INFO_OFT 2
| 802.11 information element definition
#define | MAC_WPA_VERSION_OFT 6
| 802.11 information element definition
#define | MAC_WPA_GROUP_CIPHER_OFT 8
| 802.11 information element definition
#define | MAC_WPA_PAIRWISE_CIPHER_SUITE_CNT_OFT 12
| 802.11 information element definition
#define | MAC_WPA_PAIRWISE_CIPHER_SUITE_LIST_OFT 14
| 802.11 information element definition
#define | MAC_WPA_CIPHER_SIZE 4
| 802.11 information element definition
#define | MAC_WPA_KEY_MANAGEMENT_SUITE_CNT_OFT 18
| 802.11 information element definition
#define | MAC_WPA_KEY_MANAGEMENT_SUITE_LIST_OFT 20
| 802.11 information element definition
#define | MAC_WPA_KEY_MANAGEMENT_SIZE 4
| 802.11 information element definition
#define | MAC_WPA_CAPABILITIES_OFT 24
| 802.11 information element definition
#define | MAC_WPA_MIN_LEN 24
| 802.11 information element definition
#define | MAC_WAPI_ID_OFT 0
| 802.11 information element definition
#define | MAC_WAPI_LEN_OFT 1
| 802.11 information element definition
#define | MAC_WAPI_INFO_OFT 2
| 802.11 information element definition
#define | MAC_WAPI_VERSION_OFT 2
| 802.11 information element definition
#define | MAC_WAPI_AKM_SUITE_CNT_OFT 4
| 802.11 information element definition
#define | MAC_WAPI_AKM_SUITE_LIST_OFT 6
| 802.11 information element definition
#define | MAC_WAPI_AKM_SUITE_SIZE 4
| 802.11 information element definition
#define | MAC_WAPI_PAIRWISE_CIPHER_SUITE_CNT_OFT 10
| 802.11 information element definition
#define | MAC_WAPI_PAIRWISE_CIPHER_SUITE_LIST_OFT 12
| 802.11 information element definition
#define | MAC_WAPI_CIPHER_SUITE_SIZE 4
| 802.11 information element definition
#define | MAC_WAPI_GROUP_CIPHER_SUITE_OFT 16
| 802.11 information element definition
#define | MAC_WAPI_CAPABILITY_OFT 20
| 802.11 information element definition
#define | MAC_WAPI_BKID_CNT_OFT 22
| 802.11 information element definition
#define | MAC_WAPI_BKID_LIST_OFT 24
| 802.11 information element definition
#define | MAC_WAPI_MIN_LEN 22
| 802.11 information element definition
#define | MAC_BSS_LOAD_ID_OFT 0
| 802.11 information element definition
#define | MAC_BSS_LOAD_LEN_OFT 1
| 802.11 information element definition
#define | MAC_BSS_LOAD_STA_CNT_OFT 2
| 802.11 information element definition
#define | MAC_BSS_LOAD_CH_UTILIZATION_OFT 4
| 802.11 information element definition
#define | MAC_BSS_LOAD_AVAIL_ADM_CAPA 5
| 802.11 information element definition
#define | MAC_BSS_LOAD_LEN 7
| 802.11 information element definition
#define | MAC_EDCA_PARAM_ID_OFT 0
| 802.11 information element definition
#define | MAC_EDCA_PARAM_LEN_OFT 1
| 802.11 information element definition
#define | MAC_EDCA_PARAM_QOS_INFO_OFT 2
| 802.11 information element definition
#define | MAC_EDCA_PARAM_RESERVED_OFT 3
| 802.11 information element definition
#define | MAC_EDCA_PARAM_BE_PARAM_OFT 4
| 802.11 information element definition
#define | MAC_EDCA_PARAM_BK_PARAM_OFT 8
| 802.11 information element definition
#define | MAC_EDCA_PARAM_VI_PARAM_OFT 12
| 802.11 information element definition
#define | MAC_EDCA_PARAM_VO_PARAM_OFT 16
| 802.11 information element definition
#define | MAC_EDCA_PARAM_LEN 20
| 802.11 information element definition
#define | MAC_QOS_CAPA_ID_OFT 0
| 802.11 information element definition
#define | MAC_QOS_CAPA_LEN_OFT 1
| 802.11 information element definition
#define | MAC_QOS_CAPA_INFO_OFT 2
| 802.11 information element definition
#define | MAC_QOS_CAPA_LEN 3
| 802.11 information element definition
#define | MAC_MULTI_BSSID_ID_OFT 0
| 802.11 information element definition
#define | MAC_MULTI_BSSID_LEN_OFT 1
| 802.11 information element definition
#define | MAC_MULTI_BSSID_MAX_INDICATOR_OFT 2
| 802.11 information element definition
#define | MAC_MULTI_BSSID_SUB_IES_OFT 3
| 802.11 information element definition
#define | MAC_MULTI_BSSID_ELMT_MIN_LEN 4
| 802.11 information element definition
#define | MAC_MULTI_BSSID_MIN_LEN 6
| 802.11 information element definition
#define | MAC_NON_TXED_BSSID_CAPA_ID_OFT 0
| 802.11 information element definition
#define | MAC_NON_TXED_BSSID_CAPA_LEN_OFT 1
| 802.11 information element definition
#define | MAC_NON_TXED_BSSID_CAPA_OFT 2
| 802.11 information element definition
#define | MAC_NON_TXED_BSSID_CAPA_LEN 4
| 802.11 information element definition
#define | MAC_MULTI_BSSID_INDEX_ID_OFT 0
| 802.11 information element definition
#define | MAC_MULTI_BSSID_INDEX_LEN_OFT 1
| 802.11 information element definition
#define | MAC_MULTI_BSSID_INDEX_OFT 2
| 802.11 information element definition
#define | MAC_MULTI_BSSID_DTIM_PERIOD_OFT 3
| 802.11 information element definition
#define | MAC_MULTI_BSSID_DTIM_COUNT_OFT 4
| 802.11 information element definition
#define | MAC_MULTI_BSSID_INDEX_MIN_LEN 3
| 802.11 information element definition
#define | MAC_HT_CAPA_ID_OFT 0
| 802.11 information element definition
#define | MAC_HT_CAPA_LEN_OFT 1
| 802.11 information element definition
#define | MAC_HT_CAPA_INFO_OFT 2
| 802.11 information element definition
#define | MAC_HT_CAPA_AMPDU_PARAM_OFT 4
| 802.11 information element definition
#define | MAC_HT_CAPA_SUPPORTED_MCS_SET_OFT 5
| 802.11 information element definition
#define | MAC_HT_CAPA_EXTENDED_CAPA_OFT 21
| 802.11 information element definition
#define | MAC_HT_CAPA_TX_BEAM_FORMING_CAPA_OFT 23
| 802.11 information element definition
#define | MAC_HT_CAPA_ASEL_CAPA_OFT 27
| 802.11 information element definition
#define | MAC_HT_CAPA_ELMT_LEN 26
| 802.11 information element definition
#define | MAC_HT_CAPA_ELMT_LEN_WD (CO_ALIGN4_HI(MAC_HT_CAPA_ELMT_LEN) / 4)
| 802.11 information element definition
#define | MAC_HT_CAPA_LEN 28
| 802.11 information element definition
#define | MAC_HT_OPER_ID_OFT 0
| 802.11 information element definition
#define | MAC_HT_OPER_LEN_OFT 1
| 802.11 information element definition
#define | MAC_HT_OPER_PRIM_CH_OFT 2
| 802.11 information element definition
#define | MAC_HT_OPER_INFO_OFT 3
| 802.11 information element definition
#define | MAC_HT_OPER_INFO_SUBSET2_OFT 4
| 802.11 information element definition
#define | MAC_HT_OPER_OP_MODE_MASK 0x0003
| 802.11 information element definition
#define | MAC_HT_OPER_NONGF_MASK 0x0004
| 802.11 information element definition
#define | MAC_HT_OPER_OBSS_MASK 0x0010
| 802.11 information element definition
#define | MAC_HT_OPER_INFO_SUBSET3_OFT 6
| 802.11 information element definition
#define | MAC_HT_OPER_BASIC_MSC_SET_OFT 8
| 802.11 information element definition
#define | MAC_HT_OPER_ELMT_LEN 22
| 802.11 information element definition
#define | MAC_HT_OPER_LEN 24
| 802.11 information element definition
#define | MAC_VHT_CAPA_ELMT_LEN 12
| 802.11 information element definition
#define | MAC_VHT_CAPA_ELMT_LEN_WD (CO_ALIGN4_HI(MAC_VHT_CAPA_ELMT_LEN) / 4)
| 802.11 information element definition
#define | MAC_VHT_CAPA_LEN 14
| 802.11 information element definition
#define | MAC_VHT_CAPA_ID_OFT 0
| 802.11 information element definition
#define | MAC_VHT_CAPA_LEN_OFT 1
| 802.11 information element definition
#define | MAC_VHT_CAPA_INFO_OFT 2
| 802.11 information element definition
#define | MAC_VHT_RX_MCS_MAP_OFT 6
| 802.11 information element definition
#define | MAC_VHT_RX_HIGHEST_RATE_OFT 8
| 802.11 information element definition
#define | MAC_VHT_TX_MCS_MAP_OFT 10
| 802.11 information element definition
#define | MAC_VHT_TX_HIGHEST_RATE_OFT 12
| 802.11 information element definition
#define | MAC_VHT_OPER_ELMT_LEN 5
| 802.11 information element definition
#define | MAC_VHT_OPER_LEN 7
| 802.11 information element definition
#define | MAC_VHT_OPER_ID_OFT 0
| 802.11 information element definition
#define | MAC_VHT_OPER_LEN_OFT 1
| 802.11 information element definition
#define | MAC_VHT_CHAN_WIDTH_OFT 2
| 802.11 information element definition
#define | MAC_VHT_CENTER_FREQ0_OFT 3
| 802.11 information element definition
#define | MAC_VHT_CENTER_FREQ1_OFT 4
| 802.11 information element definition
#define | MAC_VHT_BASIC_MCS_OFT 5
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_ID_OFT 0
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_LEN_OFT 1
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_INFO_OFT 2
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_ELMT_LEN 1
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_LEN 3
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_INFO_REQ_MASK 0x01
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_40_INTOLERANT_MASK 0x02
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_20_BSS_WIDTH_REQ_MASK 0x04
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_OBSS_SCAN_REQ_MASK 0x08
| 802.11 information element definition
#define | MAC_20_40_COEXISTENCE_OBSS_SCAN_GRANT_MASK 0x10
| 802.11 information element definition
#define | MAC_MGMT_MIC_ID_OFT 0
| 802.11 information element definition
#define | MAC_MGMT_MIC_LEN_OFT 1
| 802.11 information element definition
#define | MAC_MGMT_MIC_KEYID_OFT 2
| 802.11 information element definition
#define | MAC_MGMT_MIC_IPN_OFT 4
| 802.11 information element definition
#define | MAC_MGMT_MIC_IPN_LEN 6
| 802.11 information element definition
#define | MAC_MGMT_MIC_MIC_OFT 10
| 802.11 information element definition
#define | MAC_MGMT_MIC_MIC_LEN 8
| 802.11 information element definition
#define | MAC_MGMT_MIC_LEN 18
| 802.11 information element definition
#define | MAC_WMM_PARAM_ELMT_LEN 24
| 802.11 information element definition
#define | MAC_WMM_PARAM_LEN 26
| 802.11 information element definition
#define | MAC_WMM_PARAM_QOS_INFO_OFT 8
| 802.11 information element definition
#define | MAC_WMM_PARAM_SET_CNT_MSK 0x0F
| 802.11 information element definition
#define | MAC_WMM_PARAM_RESERVED_OFT 9
| 802.11 information element definition
#define | MAC_WMM_PARAM_BK_PARAM_OFT 14
| 802.11 information element definition
#define | MAC_WMM_PARAM_BE_PARAM_OFT 10
| 802.11 information element definition
#define | MAC_WMM_PARAM_VI_PARAM_OFT 18
| 802.11 information element definition
#define | MAC_WMM_PARAM_VO_PARAM_OFT 22
| 802.11 information element definition
#define | MAC_QINFO_OFT 6
| 802.11 information element definition
#define | MAC_QINFO_SET_COUNT_OFT 8
| 802.11 information element definition
#define | MAC_QINFO_SET_UAPSD_OFT 8
| 802.11 information element definition
#define | MAC_QINFO_SET_COUNT 0x07
| 802.11 information element definition
#define | MAC_QINFO_SET_UAPSD 0x80
| 802.11 information element definition
#define | SUP_MCS_RX_HIGHEST_RATE_OFT 10
| 802.11 information element definition
#define | SUP_MCS_RX_HIGHEST_RATE_SIZE 10
| 802.11 information element definition
#define | SUP_TX_MCS_SET_OFT 12
| 802.11 information element definition
#define | MAC_HE_CAPA_ID_OFT 0
| 802.11 information element definition
#define | MAC_HE_CAPA_LEN_OFT 1
| 802.11 information element definition
#define | MAC_HE_CAPA_EXT_ID_OFT 2
| 802.11 information element definition
#define | MAC_HE_CAPA_IE_MAC_CAPA_LEN MAC_HE_MAC_CAPA_LEN
| 802.11 information element definition
#define | MAC_HE_CAPA_IE_PHY_CAPA_LEN MAC_HE_PHY_CAPA_LEN
| 802.11 information element definition
#define | MAC_HE_MAC_CAPA_INFO_OFT 3
| 802.11 information element definition
#define | MAC_HE_PHY_CAPA_INFO_OFT (MAC_HE_MAC_CAPA_INFO_OFT + MAC_HE_CAPA_IE_MAC_CAPA_LEN)
| 802.11 information element definition
#define | MAC_HE_MCS_INFO_OFT (MAC_HE_PHY_CAPA_INFO_OFT + MAC_HE_CAPA_IE_PHY_CAPA_LEN)
| 802.11 information element definition
#define | MAC_HE_MCS_INFO_PER_BW_LEN 4
| 802.11 information element definition
#define | MAC_HE_CAPA_MIN_LEN (MAC_HE_MCS_INFO_OFT + MAC_HE_MCS_INFO_PER_BW_LEN)
| 802.11 information element definition
#define | MAC_HE_CAPA_MAX_LEN
| 802.11 information element definition
#define | MAC_HE_OPER_ID_OFT 0
| 802.11 information element definition
#define | MAC_HE_OPER_LEN_OFT 1
| 802.11 information element definition
#define | MAC_HE_OPER_EXT_ID_OFT 2
| 802.11 information element definition
#define | MAC_HE_OPER_PARAM_OFT 3
| 802.11 information element definition
#define | MAC_HE_OPER_PARAM_LEN 4
| 802.11 information element definition
#define | MAC_HE_OPER_BSS_COLOR_OFT 24
| 802.11 information element definition
#define | MAC_HE_OPER_BSS_COLOR_PARTIAL_BIT CO_BIT(30)
| 802.11 information element definition
#define | MAC_HE_OPER_BSS_COLOR_DISABLED_BIT CO_BIT(31)
| 802.11 information element definition
#define | MAC_HE_OPER_BSS_COLOR_MASK (0x3F << MAC_HE_OPER_BSS_COLOR_OFT)
| 802.11 information element definition
#define | MAC_HE_OPER_TXOP_DUR_RTS_THRES_OFT 4
| 802.11 information element definition
#define | MAC_HE_OPER_TXOP_DUR_RTS_THRES_MSK (0x3FF << MAC_HE_OPER_TXOP_DUR_RTS_THRES_OFT)
| 802.11 information element definition
#define | MAC_HE_OPER_TXOP_DUR_RTS_THRES_DISABLED 1023
| 802.11 information element definition
#define | MAC_HE_OPER_BASIC_MCS_OFT 7
| 802.11 information element definition
#define | MAC_HE_OPER_MIN_LEN 9
| 802.11 information element definition
#define | MAC_HE_OPER_MAX_LEN 13
| 802.11 information element definition
#define | MAC_UORA_ELMT_LEN 1
| 802.11 information element definition
#define | MAC_UORA_LEN 4
| 802.11 information element definition
#define | MAC_UORA_ID_OFT 0
| 802.11 information element definition
#define | MAC_UORA_LEN_OFT 1
| 802.11 information element definition
#define | MAC_UORA_EXT_ID_OFT 2
| 802.11 information element definition
#define | MAC_UORA_OCW_RANGE 3
| 802.11 information element definition
#define | MAC_UORA_EOCW_MIN_OFT 0
| 802.11 information element definition
#define | MAC_UORA_EOCW_MIN_MASK (0x7 << MAC_UORA_EOCW_MIN_OFT)
| 802.11 information element definition
#define | MAC_UORA_EOCW_MAX_OFT 3
| 802.11 information element definition
#define | MAC_UORA_EOCW_MAX_MASK (0x7 << MAC_UORA_EOCW_MAX_OFT)
| 802.11 information element definition
#define | MAC_UORA_EOCW_DEFAULT_MIN 3
| 802.11 information element definition
#define | MAC_UORA_EOCW_DEFAULT_MAX 5
| 802.11 information element definition
#define | MAC_MU_EDCA_ELMT_LEN 13
| 802.11 information element definition
#define | MAC_MU_EDCA_LEN 16
| 802.11 information element definition
#define | MAC_MU_EDCA_ID_OFT 0
| 802.11 information element definition
#define | MAC_MU_EDCA_LEN_OFT 1
| 802.11 information element definition
#define | MAC_MU_EDCA_EXT_ID_OFT 2
| 802.11 information element definition
#define | MAC_MU_EDCA_QOS_INFO_OFT 3
| 802.11 information element definition
#define | MAC_MU_EDCA_PARAM_SET_CNT_MSK 0x0F
| 802.11 information element definition
#define | MAC_MU_EDCA_AC_BE_OFT 4
| 802.11 information element definition
#define | MAC_MU_EDCA_AC_BK_OFT 7
| 802.11 information element definition
#define | MAC_MU_EDCA_AC_VI_OFT 10
| 802.11 information element definition
#define | MAC_MU_EDCA_AC_VO_OFT 13
| 802.11 information element definition
#define | MAC_MESHID_ELMT_MAX_LEN 32
| 802.11 information element definition
#define | MAC_MESHID_MAX_LEN 34
| 802.11 information element definition
#define | MAC_MPM_INFO_MIN_LEN 4
| 802.11 information element definition
#define | MAC_MPM_PEERING_PROT_OFT (MAC_INFOELT_INFO_OFT + 0)
| 802.11 information element definition
#define | MAC_MPM_LOCAL_LINK_ID_OFT (MAC_INFOELT_INFO_OFT + 2)
| 802.11 information element definition
#define | MAC_MPM_OPT_FIELD_OFT (MAC_INFOELT_INFO_OFT + MAC_MPM_INFO_MIN_LEN)
| 802.11 information element definition
#define | MAC_MPM_MIN_LEN 6
| 802.11 information element definition
#define | MAC_MPM_MAX_LEN 26
| 802.11 information element definition
#define | MAC_MAW_AWAKE_WIND_OFT MAC_INFOELT_INFO_OFT
| 802.11 information element definition
#define | MAC_MAW_LEN 4
| 802.11 information element definition
#define | MAC_MCFG_ELMT_LEN 7
| 802.11 information element definition
#define | MAC_MCFG_PATH_SEL_PROT_OFT (MAC_INFOELT_INFO_OFT + 0)
| 802.11 information element definition
#define | MAC_MCFG_PATH_METRIC_PROT_OFT (MAC_INFOELT_INFO_OFT + 1)
| 802.11 information element definition
#define | MAC_MCFG_CONG_CTRL_MODE_OFT (MAC_INFOELT_INFO_OFT + 2)
| 802.11 information element definition
#define | MAC_MCFG_SYNC_METHOD_OFT (MAC_INFOELT_INFO_OFT + 3)
| 802.11 information element definition
#define | MAC_MCFG_AUTH_PROT_OFT (MAC_INFOELT_INFO_OFT + 4)
| 802.11 information element definition
#define | MAC_MCFG_MESH_FORM_INFO_OFT (MAC_INFOELT_INFO_OFT + 5)
| 802.11 information element definition
#define | MAC_MCFG_MESH_CAP_OFT (MAC_INFOELT_INFO_OFT + 6)
| 802.11 information element definition
#define | MAC_MCFG_LEN 9
| 802.11 information element definition
## Spectrum and Power Management Frame definitions
enum | { REMOTE_MEAS_REQ_LATE = 1, REMOTE_MEAS_REQ_INCAPABLE, REMOTE_MEAS_REQ_REFUSED }
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_FRAME_INFO_OFT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_CH_SWITCH_FRAME_INFO_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_FRAME_PRE_INFO_LEN 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_POWER_CONSTRAINT_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_POWER_CONSTRAINT_ELT_LEN 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MIN_TX_POWER_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MAX_TX_POWER_OFT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_POWER_CAPABILITY_ELT_LEN 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_POWER_CAPABILITY_ELT_LEN_FIELD 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_TX_POWER_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_LINK_MARGIN_OFT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_TPC_REQUEST_ELT_LEN 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_TPC_REPORT_ELT_LEN 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_LEN_VAL_TPC_REQ 0
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_LEN_VAL_TPC_REP 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_FRAME_TPC_REQ_LEN 5
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_FRAME_TPC_REP_LEN 7
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_FIRST_CHANNEL_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_NUMBER_CHANNEL_OFT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SWITCH_MODE_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SWITCH_NEW_CHAN_OFT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SWITCH_COUNT_OFT 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_CHANNEL_SWITCH_INFO_LEN 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_CHANNEL_SWITCH_ELT_LEN 5
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_EXT_SWITCH_MODE_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_EXT_SWITCH_NEW_CLASS 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_EXT_SWITCH_NEW_CHAN_OFT 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_EXT_SWITCH_COUNT_OFT 5
| 802.11 Spectrum and Power Management frame definition
#define | MAC_EXT_CHANNEL_SWITCH_INFO_LEN 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_EXT_CHANNEL_SWITCH_ELT_LEN 6
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SEC_CH_OFFSET_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SEC_CH_OFFSET_INFO_LEN 1
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SEC_CH_OFFSET_ELT_LEN 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SEC_CH_OFFSET_SEC_CH_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SEC_CH_OFFSET_NO_SEC_CH 0
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SEC_CH_OFFSET_SEC_ABOVE 1
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_SEC_CH_OFFSET_SEC_BELOW 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_WIDE_BW_CHAN_SWITCH_NEW_CW_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_WIDE_BW_CHAN_SWITCH_NEW_CENTER1_OFT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_WIDE_BW_CHAN_SWITCH_NEW_CENTER2_OFT 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_WIDE_BW_CHAN_SWITCH_INFO_LEN 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_WIDE_BW_CHAN_SWITCH_ELT_LEN 5
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MEASURE_TOKEN_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MEASURE_MODE_OFT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MEASURE_TYPE_OFT 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MEASURE_CH_NBR_OFT 5
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MEASURE_START_TIME_OFT 6
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MEASURE_DURATION_OFT 14
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MEASURE_INFO_OFT 16
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REQ_CNF_ELT_LEN 5
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REQ_ELT_LEN 16
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REQ_FRAME_LEN 19
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REP_BASIC_ELT_LEN 17
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REP_BASIC_FRAME_LEN 20
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REP_CCA_ELT_LEN 17
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REP_CCA_FRAME_LEN 20
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REP_RPI_ELT_LEN 24
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REP_RPI_FRAME_LEN 27
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REP_ERR_ELT_LEN 5
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEAS_REP_ERR_FRAME_LEN 8
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MDE_ID_OFT 0
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MDE_LEN_OFT 1
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MDE_MDID_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MDE_FT_CAPA_POL_OFT 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MDE_MDID_LEN 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MDE_FT_CAPA_POL_LEN 1
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MDE_ELMT_LEN 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_MDE_LEN 5
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_LINK_ID_LEN 18
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_LINK_ID_BSSID_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_LINK_ID_INIT_STA_OFT 8
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_LINK_ID_RESP_STA_OFT 14
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_CH_SWITCH_TIMING_LEN 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_CH_SWITCH_TIMING_SWTIME_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_CH_SWITCH_TIMING_SWTOUT_OFT 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_PTI_CONTROL_LEN 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_PTI_CONTROL_TID_OFT 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_PTI_CONTROL_SEQ_CTRL_OFT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_TPU_BUF_STATUS_LEN 1
| 802.11 Spectrum and Power Management frame definition
#define | MAC_INFOELT_TPU_BUF_STATUS_AC_STATUS 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_MEASURE_REQUEST 0
| 802.11 Spectrum management frame definition
#define | MAC_ACTION_MEASURE_REPORT 1
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_TPC_REQUEST 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_TPC_REPORT 3
| 802.11 Spectrum and Power Management frame definition
#define | MAC_ACTION_CHANNEL_SWITCH 4
| 802.11 Spectrum and Power Management frame definition
#define | MAC_SWITCH_MODE_TX_TRAFFIC_CONT 0
| 802.11 Spectrum and Power Management frame definition
#define | MAC_SWITCH_MODE_TX_TRAFFIC_STOP 1
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MODE_ENABLE CO_BIT(1)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MODE_REQUEST CO_BIT(2)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MODE_REPORT CO_BIT(3)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MODE_LATE CO_BIT(0)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MODE_INCAPABLE CO_BIT(1)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MODE_REFUSED CO_BIT(2)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_TYPE_BASIC 0
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_TYPE_CCA 1
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_TYPE_RPI 2
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MAP_FREE 0x00
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MAP_BSS CO_BIT(0)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MAP_OFDM CO_BIT(1)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MAP_UNIDENTIFIED CO_BIT(2)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MAP_RADAR CO_BIT(3)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MAP_UNMEASURED CO_BIT(4)
| 802.11 Spectrum and Power Management frame definition
#define | MAC_MEASURE_MAP_MASK 0x1F
| 802.11 Spectrum and Power Management frame definition
#define | MAC_DEFAULT_SWITCH_COUNT 0
| 802.11 Spectrum and Power Management frame definition
#define | MAC_DEFAULT_RADAR_CHECK_TIME 60
| 802.11 Spectrum and Power Management frame definition
## Various Field Length definitions
#define | MIC_HDR_LEN (16)
| MIC Header Length -> DA (6 bytes) + SA (6 bytes) + Priority (4 bytes).
#define | IV_LEN (4)
| IV Length.
#define | EIV_LEN (4)
| EIV Length.
#define | MIC_LEN (8)
| MIC Length.
#define | ICV_LEN (4)
| ICV Length.
#define | WPI_IV_LEN (18)
| MIC Header Length -> DA (6 bytes) + SA (6 bytes) + Priority (4 bytes).
#define | WPI_MIC_LEN (16)
| MIC Header Length -> DA (6 bytes) + SA (6 bytes) + Priority (4 bytes).
#define | MAC_FCS_LEN 4
| Length of the FCS field.
## MAC Header Length definitions
#define | MAC_LONG_QOS_HTC_MAC_HDR_LEN 36
| Long MAC Header length (with QoS control field and HT control field).
#define | MAC_LONG_QOS_MAC_HDR_LEN 32
| Long MAC Header length (with QoS control field).
#define | MAC_LONG_MAC_HDR_LEN 30
| Long MAC Header length (without QoS control field).
#define | MAC_SHORT_QOS_HTC_MAC_HDR_LEN 30
| Short MAC Header length (with QoS control field and HT control field).
#define | MAC_SHORT_QOS_MAC_HDR_LEN 26
| Short MAC Header length (with QoS control field).
#define | MAC_SHORT_MAC_HDR_LEN 24
| Short MAC Header length (without QoS control field).
#define | MAC_HDR_QOS_CTRL_LEN 2
| QoS Control Field Length.
#define | MAC_HDR_LEN_MAX MAC_LONG_QOS_HTC_MAC_HDR_LEN
| Longest possible MAC Header.
#define | MAC_LONG_CTRLFRAME_LEN 16
| Long control frame header length.
#define | MAC_SHORT_CTRLFRAME_LEN 10
| Short control frame header length (ACK/CTS).
## MAC Header offset definitions
#define | MAC_HEAD_FCTRL_OFT 0
| 802.11 MAC header definition
#define | MAC_HEAD_DURATION_OFT 2
| 802.11 MAC header definition
#define | MAC_HEAD_DURATION_CFP 0x8000
| 802.11 MAC header definition
#define | MAC_HEAD_ADDR1_OFT 4
| 802.11 MAC header definition
#define | MAC_HEAD_ADDR2_OFT 10
| 802.11 MAC header definition
#define | MAC_HEAD_ADDR3_OFT 16
| 802.11 MAC header definition
#define | MAC_HEAD_CTRL_OFT 22
| 802.11 MAC header definition
#define | MAC_HEAD_ADDR4_OFT 24
| 802.11 MAC header definition
#define | MAC_HEAD_SHORT_QOS_OFT 24
| 802.11 MAC header definition
#define | MAC_HEAD_LONG_QOS_OFT 30
| 802.11 MAC header definition
#define | MAC_ORIGINAL_ETHTYPE_OFT 36
| 802.11 MAC header definition
## Frame Control bit field definitions
#define | MAC_FCTRL_LEN 2
| 802.11 frame control definition
#define | MAC_FCTRL_PROTOCOLVERSION_MASK 0x0003
| 802.11 frame control definition
#define | MAC_FCTRL_TYPE_MASK 0x000C
| 802.11 frame control definition
#define | MAC_FCTRL_SUBT_MASK 0x00F0
| 802.11 frame control definition
#define | MAC_FCTRL_TODS 0x0100
| 802.11 frame control definition
#define | MAC_FCTRL_FROMDS 0x0200
| 802.11 frame control definition
#define | MAC_FCTRL_MOREFRAG 0x0400
| 802.11 frame control definition
#define | MAC_FCTRL_RETRY 0x0800
| 802.11 frame control definition
#define | MAC_FCTRL_PWRMGT 0x1000
| 802.11 frame control definition
#define | MAC_FCTRL_MOREDATA 0x2000
| 802.11 frame control definition
#define | MAC_FCTRL_PROTECTEDFRAME 0x4000
| 802.11 frame control definition
#define | MAC_FCTRL_ORDER 0x8000
| 802.11 frame control definition
#define | MAC_FCTRL_TODS_FROMDS (MAC_FCTRL_TODS | MAC_FCTRL_FROMDS)
| 802.11 frame control definition
## Frame Control Type definitions
#define | MAC_FCTRL_MGT_T 0x0000
| 802.11 type definition
#define | MAC_FCTRL_CTRL_T 0x0004
| 802.11 type definition
#define | MAC_FCTRL_DATA_T 0x0008
| 802.11 type definition
## Frame Control Subtype definitions
#define | MAC_FCTRL_ASSOCREQ_ST 0x0000
| 802.11 subtype definition
#define | MAC_FCTRL_ASSOCRSP_ST 0x0010
| 802.11 subtype definition
#define | MAC_FCTRL_REASSOCREQ_ST 0x0020
| 802.11 subtype definition
#define | MAC_FCTRL_REASSOCRSP_ST 0x0030
| 802.11 subtype definition
#define | MAC_FCTRL_PROBEREQ_ST 0x0040
| 802.11 subtype definition
#define | MAC_FCTRL_PROBERSP_ST 0x0050
| 802.11 subtype definition
#define | MAC_FCTRL_BEACON_ST 0x0080
| 802.11 subtype definition
#define | MAC_FCTRL_ATIM_ST 0x0090
| 802.11 subtype definition
#define | MAC_FCTRL_DISASSOC_ST 0x00A0
| 802.11 subtype definition
#define | MAC_FCTRL_AUTHENT_ST 0x00B0
| 802.11 subtype definition
#define | MAC_FCTRL_DEAUTHENT_ST 0x00C0
| 802.11 subtype definition
#define | MAC_FCTRL_ACTION_ST 0x00D0
| 802.11 subtype definition
#define | MAC_FCTRL_ACTION_NO_ACK_ST 0x00E0
| 802.11 subtype definition
#define | MAC_FCTRL_HE_TRIGGER_ST 0x0020
| 802.11 subtype definition
#define | MAC_FCTRL_BFM_REPORT_POLL_ST 0x0040
| 802.11 subtype definition
#define | MAC_FCTRL_VHT_NDPA_ST 0x0050
| 802.11 subtype definition
#define | MAC_FCTRL_CTRL_WRAPPER_ST 0x0070
| 802.11 subtype definition
#define | MAC_FCTRL_BAR_ST 0x0080
| 802.11 subtype definition
#define | MAC_FCTRL_BA_ST 0x0090
| 802.11 subtype definition
#define | MAC_FCTRL_PSPOLL_ST 0x00A0
| 802.11 subtype definition
#define | MAC_FCTRL_RTS_ST 0x00B0
| 802.11 subtype definition
#define | MAC_FCTRL_CTS_ST 0x00C0
| 802.11 subtype definition
#define | MAC_FCTRL_ACK_ST 0x00D0
| 802.11 subtype definition
#define | MAC_FCTRL_CFEND_ST 0x00E0
| 802.11 subtype definition
#define | MAC_FCTRL_CFEND_CFACK_ST 0x00F0
| 802.11 subtype definition
#define | MAC_CFACK_ST_BIT CO_BIT(4)
| 802.11 subtype definition
#define | MAC_CFPOLL_ST_BIT CO_BIT(5)
| 802.11 subtype definition
#define | MAC_NODATA_ST_BIT CO_BIT(6)
| 802.11 subtype definition
#define | MAC_QOS_ST_BIT CO_BIT(7)
| 802.11 subtype definition
#define | MAC_FCTRL_DATACFACKPOLL_ST (MAC_CFACK_ST_BIT | MAC_CFPOLL_ST_BIT)
| 802.11 subtype definition
## Frame Control various frame type/subtype definitions
#define | MAC_FCTRL_TYPESUBTYPE_MASK (MAC_FCTRL_TYPE_MASK | MAC_FCTRL_SUBT_MASK)
| 802.11 type/subtype definition
#define | MAC_FCTRL_ASSOCREQ (MAC_FCTRL_MGT_T | MAC_FCTRL_ASSOCREQ_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_ASSOCRSP (MAC_FCTRL_MGT_T | MAC_FCTRL_ASSOCRSP_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_REASSOCREQ (MAC_FCTRL_MGT_T | MAC_FCTRL_REASSOCREQ_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_REASSOCRSP (MAC_FCTRL_MGT_T | MAC_FCTRL_REASSOCRSP_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_PROBEREQ (MAC_FCTRL_MGT_T | MAC_FCTRL_PROBEREQ_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_PROBERSP (MAC_FCTRL_MGT_T | MAC_FCTRL_PROBERSP_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_BEACON (MAC_FCTRL_MGT_T | MAC_FCTRL_BEACON_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_ATIM (MAC_FCTRL_MGT_T | MAC_FCTRL_ATIM_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_DISASSOC (MAC_FCTRL_MGT_T | MAC_FCTRL_DISASSOC_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_AUTHENT (MAC_FCTRL_MGT_T | MAC_FCTRL_AUTHENT_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_DEAUTHENT (MAC_FCTRL_MGT_T | MAC_FCTRL_DEAUTHENT_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_ACTION (MAC_FCTRL_MGT_T | MAC_FCTRL_ACTION_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_ACTION_NO_ACK (MAC_FCTRL_MGT_T | MAC_FCTRL_ACTION_NO_ACK_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_BFM_REPORT_POLL (MAC_FCTRL_CTRL_T | MAC_FCTRL_BFM_REPORT_POLL_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_HE_TRIGGER (MAC_FCTRL_CTRL_T | MAC_FCTRL_HE_TRIGGER_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_VHT_NDPA (MAC_FCTRL_CTRL_T | MAC_FCTRL_VHT_NDPA_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_BA (MAC_FCTRL_CTRL_T | MAC_FCTRL_BA_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_BAR (MAC_FCTRL_CTRL_T | MAC_FCTRL_BAR_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_PSPOLL (MAC_FCTRL_CTRL_T | MAC_FCTRL_PSPOLL_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_RTS (MAC_FCTRL_CTRL_T | MAC_FCTRL_RTS_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_CTS (MAC_FCTRL_CTRL_T | MAC_FCTRL_CTS_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_ACK (MAC_FCTRL_CTRL_T | MAC_FCTRL_ACK_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_CFEND (MAC_FCTRL_CTRL_T | MAC_FCTRL_CFEND_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_CFEND_CFACK (MAC_FCTRL_CFEND | MAC_CFACK_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_DATA_CFACK (MAC_FCTRL_DATA_T | MAC_CFACK_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_DATA_CFPOLL (MAC_FCTRL_DATA_T | MAC_CFPOLL_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_DATA_CFACKPOLL (MAC_FCTRL_DATA_T | MAC_FCTRL_DATACFACKPOLL_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_NULL_FUNCTION (MAC_FCTRL_DATA_T | MAC_NODATA_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_NULL_CFACK (MAC_FCTRL_NULL_FUNCTION | MAC_CFACK_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_NULL_CFPOLL (MAC_FCTRL_NULL_FUNCTION | MAC_CFPOLL_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_NULL_CFACKPOLL (MAC_FCTRL_NULL_FUNCTION | MAC_FCTRL_DATACFACKPOLL_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_QOS_DATA (MAC_FCTRL_DATA_T | MAC_QOS_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_QOS_DATA_CFACK (MAC_FCTRL_QOS_DATA | MAC_CFACK_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_QOS_DATA_CFPOLL (MAC_FCTRL_QOS_DATA | MAC_CFPOLL_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_QOS_DATA_CFACKPOLL (MAC_FCTRL_QOS_DATA | MAC_FCTRL_DATACFACKPOLL_ST)
| 802.11 type/subtype definition
#define | MAC_FCTRL_QOS_NULL (MAC_FCTRL_QOS_DATA | MAC_NODATA_ST_BIT)
| 802.11 type/subtype definition
#define | MAC_FCTRL_QOS_NULL_CFACK (MAC_FCTRL_QOS_DATA | MAC_FCTRL_NULL_CFACK)
| 802.11 type/subtype definition
#define | MAC_FCTRL_QOS_NULL_CFPOLL (MAC_FCTRL_QOS_DATA | MAC_FCTRL_NULL_CFPOLL)
| 802.11 type/subtype definition
#define | MAC_FCTRL_QOS_NULL_CFACKPOLL (MAC_FCTRL_QOS_DATA | MAC_FCTRL_NULL_CFACKPOLL)
| 802.11 type/subtype definition
#define | MAC_FCTRL_IS(fc, type) (((fc) & MAC_FCTRL_TYPESUBTYPE_MASK) == MAC_FCTRL_##type)
| 802.11 type/subtype definition
#define | MAC_FCTRL_SUBTYPE(fc) (((fc) & MAC_FCTRL_SUBT_MASK) >> 4)
| 802.11 type/subtype definition
## Duration/AID field definitions
#define | MAC_DURATION_LEN 2
| DURATION FIELD Length.
#define | MAC_AID_MSK 0x3FFF
| ASSOCIATION ID Field Mask.
## Sequence Control definitions
#define | MAC_SEQCTRL_LEN 2
| 802.11 Sequence Control definition
#define | MAC_SEQCTRL_NUM_OFT 4
| 802.11 Sequence Control definition
#define | MAC_SEQCTRL_NUM_MSK 0xFFF0
| 802.11 Sequence Control definition
#define | MAC_SEQCTRL_NUM_MAX (MAC_SEQCTRL_NUM_MSK >> MAC_SEQCTRL_NUM_OFT)
| 802.11 Sequence Control definition
#define | MAC_SEQCTRL_FRAG_OFT 0
| 802.11 Sequence Control definition
#define | MAC_SEQCTRL_FRAG_MSK 0x000F
| 802.11 Sequence Control definition
## Security header definitions
#define | MAC_HDR_TSC_LEN 6
| 802.11 Security header definition
#define | MAC_TKIP_TSC1_OFT 0
| 802.11 Security header definition
#define | MAC_TKIP_TSC0_OFT 2
| 802.11 Security header definition
#define | MAC_TKIP_KEYID_OFT 3
| 802.11 Security header definition
#define | MAC_CCMP_PN0_OFT 0
| 802.11 Security header definition
#define | MAC_CCMP_PN1_OFT 1
| 802.11 Security header definition
#define | MAC_CCMP_RSV_OFT 2
| 802.11 Security header definition
#define | MAC_CCMP_PN2BIT_OFT 8
| 802.11 Security header definition
#define | MAC_IV_EXTIV 0x20000000
| 802.11 Security header definition
## QoS Control definitions
#define | MAC_QOSCTRL_LEN 2
| 802.11 QoS control definition
#define | MAC_QOSCTRL_UP_OFT 0
| 802.11 QoS control definition
#define | MAC_QOSCTRL_UP_MSK 0x0007
| 802.11 QoS control definition
#define | MAC_QOSCTRL_EOSP_OFT 4
| 802.11 QoS control definition
#define | MAC_QOSCTRL_EOSP 0x10
| 802.11 QoS control definition
#define | MAC_QOSCTRL_QUEUE_SIZE_PRESENT 0x10
| 802.11 QoS control definition
#define | MAC_QOSCTRL_QUEUE_SIZE_OFT 8
| 802.11 QoS control definition
#define | MAC_QOSCTRL_QUEUE_SIZE_UNKNOWN (0xFF << MAC_QOSCTRL_QUEUE_SIZE_OFT)
| 802.11 QoS control definition
#define | MAC_QOSCTRL_HE_QUEUE_SIZE
| 802.11 QoS control definition
#define | MAC_QOSCTRL_ACK_OFT 5
| 802.11 QoS control definition
#define | MAC_QOSCTRL_ACK_NORMAL 0x0000
| 802.11 QoS control definition
#define | MAC_QOSCTRL_ACK_NOACK 0x0020
| 802.11 QoS control definition
#define | MAC_QOSCTRL_ACK_NOEXPL 0x0040
| 802.11 QoS control definition
#define | MAC_QOSCTRL_ACK_BLOCK 0x0060
| 802.11 QoS control definition
#define | MAC_QOSCTRL_AMSDU_OFT 7
| 802.11 QoS control definition
#define | MAC_QOSCTRL_AMSDU_PRESENT CO_BIT(7)
| 802.11 QoS control definition
#define | MAC_QOSCTRL_MESH_CTRL_PRESENT CO_BIT(8)
| 802.11 QoS control definition
#define | MAC_QOSCTRL_MESH_POWER_SAVE_LVL CO_BIT(9)
| 802.11 QoS control definition
#define | MAC_QOSCTRL_MESH_RSPI CO_BIT(10)
| 802.11 QoS control definition
## HT Control definitions
#define | MAC_HTC_LEN 4
| HT CONTROL FIELD.
#define | MAC_HTC_TYPE_OFT 0
| HT CONTROL FIELD.
#define | MAC_HTC_TYPE_HT_MSK (0x01 << MAC_HTC_TYPE_OFT)
| HT CONTROL FIELD.
#define | MAC_HTC_TYPE_HT (0x00 << MAC_HTC_TYPE_OFT)
| HT CONTROL FIELD.
#define | MAC_HTC_TYPE_VHT_HE_MSK (0x03 << MAC_HTC_TYPE_OFT)
| HT CONTROL FIELD.
#define | MAC_HTC_TYPE_VHT (0x01 << MAC_HTC_TYPE_OFT)
| HT CONTROL FIELD.
#define | MAC_HTC_TYPE_HE (0x03 << MAC_HTC_TYPE_OFT)
| HT CONTROL FIELD.
#define | MAC_HTC_HE_A_CONTROL_OFT 2
| HT CONTROL FIELD.
#define | MAC_HTC_HE_A_CONTROL_MSK (0x3FFFFFFF << MAC_HTC_HE_A_CONTROL_OFT)
| HT CONTROL FIELD.
## +HTC HE Variant definitions
#define | MAC_HTC_HE_CTRL_ID_OFT 0
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_MSK (0x0F << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_TRS (0x00 << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_OM (0x01 << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_HLA (0x02 << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_BSR (0x03 << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_UPH (0x04 << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_BQR (0x05 << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_CAS (0x06 << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_ID_ONES (0x0F << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_INFO_OFT 4
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_CTRL_INFO_MSK (0x0F << MAC_HTC_HE_CTRL_ID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_ACI_BMP_OFT MAC_HTC_HE_CTRL_INFO_OFT
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_ACI_BMP_MSK (0x0F << MAC_HTC_HE_BSR_ACI_BMP_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_DELTA_TID_OFT (MAC_HTC_HE_CTRL_INFO_OFT + 4)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_DELTA_TID_MSK (0x03 << MAC_HTC_HE_BSR_DELTA_TID_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_ACI_HIGH_OFT (MAC_HTC_HE_CTRL_INFO_OFT + 6)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_ACI_HIGH_MSK (0x03 << MAC_HTC_HE_BSR_ACI_HIGH_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_SCALING_FAC_OFT (MAC_HTC_HE_CTRL_INFO_OFT + 8)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_SCALING_FAC_MSK (0x03 << MAC_HTC_HE_BSR_SCALING_FAC_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_QSIZE_HIGH_OFT (MAC_HTC_HE_CTRL_INFO_OFT + 10)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_QSIZE_HIGH_MSK (0xFF << MAC_HTC_HE_BSR_QSIZE_HIGH_OFT)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_QSIZE_ALL_OFT (MAC_HTC_HE_CTRL_INFO_OFT + 18)
| +HTC HE VARIANT FIELD
#define | MAC_HTC_HE_BSR_QSIZE_ALL_MSK (0xFF << MAC_HTC_HE_BSR_QSIZE_ALL_OFT)
| +HTC HE VARIANT FIELD
## +HTC HE Variant building macros
#define | MAC_HTC_HE_CTRL(id, info) (MAC_HTC_HE_CTRL_ID_##id | ((info) << MAC_HTC_HE_CTRL_INFO_OFT))
| Format a control subfield for a +HTC HE.
#define | MAC_HTC_HE(a_control) (MAC_HTC_TYPE_HE | ((a_control) << MAC_HTC_HE_A_CONTROL_OFT))
| Format a +HTC HE Variant field.
## Capability Information definitions
See IEEE 802.1H for LLC/SNAP encapsulation/decapsulation Ethernet-II snap header (RFC1042 for most EtherTypes)
#define | MAC_CAPA_ESS CO_BIT(0)
| 802.11 Capability definition
#define | MAC_CAPA_IBSS CO_BIT(1)
| 802.11 Capability definition
#define | MAC_CAPA_CFPOLL CO_BIT(2)
| 802.11 Capability definition
#define | MAC_CAPA_CFREQ CO_BIT(3)
| 802.11 Capability definition
#define | MAC_CAPA_PRIVA CO_BIT(4)
| 802.11 Capability definition
#define | MAC_CAPA_SHORT_PREAMBLE CO_BIT(5)
| 802.11 Capability definition
#define | MAC_CAPA_PBCB CO_BIT(6)
| 802.11 Capability definition
#define | MAC_CAPA_AGILITY CO_BIT(7)
| 802.11 Capability definition
#define | MAC_CAPA_SPECTRUM CO_BIT(8)
| 802.11 Capability definition
#define | MAC_CAPA_QOS CO_BIT(9)
| 802.11 Capability definition
#define | MAC_CAPA_SHORT_SLOT CO_BIT(10)
| 802.11 Capability definition
#define | MAC_CAPA_APSD CO_BIT(11)
| 802.11 Capability definition
#define | MAC_CAPA_DSSS_OFDM CO_BIT(13)
| 802.11 Capability definition
#define | MAC_CAPA_DELAYED_BA CO_BIT(14)
| 802.11 Capability definition
#define | MAC_CAPA_IMMEDIATE_BA CO_BIT(15)
| 802.11 Capability definition
#define | MAC_CAPA_BA_POLICY (MAC_CAPA_DELAYED_BA | MAC_CAPA_IMMEDIATE_BA)
| 802.11 Capability definition
#define | FRAME_BODY_LLC_H 0x0003AAAA
| LLC definition.
#define | FRAME_BODY_LLC_L 0x0D890000
| 802.11 Capability definition
#define | PAYLOAD_TYPE_TDLS 0x02
| 802.11 Capability definition
#define | MAC_ENCAPSULATED_LLC_H_OFT 0
| 802.11 Capability definition
#define | MAC_ENCAPSULATED_LLC_L_OFT 4
| 802.11 Capability definition
#define | MAC_ENCAPSULATED_PAYLOAD_TYPE_OFT 8
| 802.11 Capability definition
#define | MAC_ENCAPSULATED_PAYLOAD_OFT 9
| 802.11 Capability definition
## HT Capability Information Element definitions
#define | MAC_HTCAPA_LDPC CO_BIT(0)
| 802.11 HT capability definition
#define | MAC_HTCAPA_40_MHZ CO_BIT(1)
| 802.11 HT capability definition
#define | MAC_HTCAPA_SMPS_OFT 2
| 802.11 HT capability definition
#define | MAC_HTCAPA_SMPS_MSK (0x03 << MAC_HTCAPA_SMPS_OFT)
| 802.11 HT capability definition
#define | MAC_HTCAPA_SMPS_STATIC (0x00 << MAC_HTCAPA_SMPS_OFT)
| 802.11 HT capability definition
#define | MAC_HTCAPA_SMPS_DYNAMIC (0x01 << MAC_HTCAPA_SMPS_OFT)
| 802.11 HT capability definition
#define | MAC_HTCAPA_SMPS_DISABLE (0x03 << MAC_HTCAPA_SMPS_OFT)
| 802.11 HT capability definition
#define | MAC_HTCAPA_GREEN_FIELD CO_BIT(4)
| 802.11 HT capability definition
#define | MAC_HTCAPA_SHORTGI_20 CO_BIT(5)
| 802.11 HT capability definition
#define | MAC_HTCAPA_SHORTGI_40 CO_BIT(6)
| 802.11 HT capability definition
#define | MAC_HTCAPA_TX_STBC CO_BIT(7)
| 802.11 HT capability definition
#define | MAC_HTCAPA_RX_STBC_OFT 8
| 802.11 HT capability definition
#define | MAC_HTCAPA_RX_STBC_MSK (0x03 << MAC_HTCAPA_RX_STBC_OFT)
| 802.11 HT capability definition
#define | MAC_HTCAPA_AMSDU CO_BIT(11)
| 802.11 HT capability definition
#define | MAC_HTCAPA_DSSS_CCK_40 CO_BIT(12)
| 802.11 HT capability definition
#define | MAC_HTCAPA_40_INTOLERANT CO_BIT(14)
| 802.11 HT capability definition
#define | MAC_HTCAPA_LSIG CO_BIT(15)
| 802.11 HT capability definition
#define | MAC_AMPDU_LEN_EXP_OFT 0
| 802.11 HT capability definition
#define | MAC_AMPDU_LEN_EXP_MSK (0x03 << MAC_AMPDU_LEN_EXP_OFT)
| 802.11 HT capability definition
#define | MAC_AMPDU_MIN_SPACING_OFT 2
| 802.11 HT capability definition
#define | MAC_AMPDU_MIN_SPACING_MSK (0x07 << MAC_AMPDU_MIN_SPACING_OFT)
| 802.11 HT capability definition
#define | MAC_HT_MAX_AMPDU_FACTOR 13
| 802.11 HT capability definition
#define | MAC_HTXCAPA_MFB_UNSOLICIT CO_BIT(9)
| 802.11 HT capability definition
## VHT Capability Information Element definitions
#define | MAC_VHTCAPA_MAX_MPDU_LENGTH_OFT 0
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_MAX_MPDU_LENGTH_MSK (0x03 << MAC_VHTCAPA_MAX_MPDU_LENGTH_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_MAX_MPDU_LENGTH_3895 (0x00 << MAC_VHTCAPA_MAX_MPDU_LENGTH_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_MAX_MPDU_LENGTH_7991 (0x01 << MAC_VHTCAPA_MAX_MPDU_LENGTH_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_MAX_MPDU_LENGTH_11454 (0x02 << MAC_VHTCAPA_MAX_MPDU_LENGTH_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SUPP_CHAN_WIDTH_OFT 2
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SUPP_CHAN_WIDTH_MSK (0x03 << MAC_VHTCAPA_SUPP_CHAN_WIDTH_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SUPP_CHAN_WIDTH_80 (0x00 << MAC_VHTCAPA_SUPP_CHAN_WIDTH_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SUPP_CHAN_WIDTH_160 (0x01 << MAC_VHTCAPA_SUPP_CHAN_WIDTH_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SUPP_CHAN_WIDTH_160_80P80 (0x02 << MAC_VHTCAPA_SUPP_CHAN_WIDTH_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_RXLDPC CO_BIT(4)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SHORT_GI_80 CO_BIT(5)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SHORT_GI_160 CO_BIT(6)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_TXSTBC CO_BIT(7)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_RXSTBC_OFT 8
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_RXSTBC_MSK (0x07 << MAC_VHTCAPA_RXSTBC_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_RXSTBC_1 (0x01 << MAC_VHTCAPA_RXSTBC_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_RXSTBC_2 (0x02 << MAC_VHTCAPA_RXSTBC_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_RXSTBC_3 (0x03 << MAC_VHTCAPA_RXSTBC_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_RXSTBC_4 (0x04 << MAC_VHTCAPA_RXSTBC_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SU_BEAMFORMER_CAPABLE CO_BIT(11)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SU_BEAMFORMEE_CAPABLE CO_BIT(12)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_BEAMFORMEE_STS_OFT 13
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_BEAMFORMEE_STS_MSK (0x07 << MAC_VHTCAPA_BEAMFORMEE_STS_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SOUNDING_DIMENSIONS_OFT 16
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_SOUNDING_DIMENSIONS_MSK (0x07 << MAC_VHTCAPA_SOUNDING_DIMENSIONS_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_MU_BEAMFORMER_CAPABLE CO_BIT(19)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_MU_BEAMFORMEE_CAPABLE CO_BIT(20)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_VHT_TXOP_PS CO_BIT(21)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_HTC_VHT CO_BIT(22)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_MAX_A_MPDU_LENGTH_EXP_OFT 23
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_MAX_A_MPDU_LENGTH_EXP_MSK (0x07 << MAC_VHTCAPA_MAX_A_MPDU_LENGTH_EXP_OFT)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_VHT_LA_VHT_UNSOL_MFB 0x08000000
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_VHT_LA_VHT_MRQ_MFB 0x0c000000
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_RX_ANTENNA_PATTERN CO_BIT(28)
| 802.11 VHT capability definition
#define | MAC_VHTCAPA_TX_ANTENNA_PATTERN CO_BIT(29)
| 802.11 VHT capability definition
#define | MAC_VHT_MCS_MAP_MSK 0x03
| 802.11 VHT capability definition
#define | MAC_VHT_MCS_MAP_0_7 0x00
| 802.11 VHT capability definition
#define | MAC_VHT_MCS_MAP_0_8 0x01
| 802.11 VHT capability definition
#define | MAC_VHT_MCS_MAP_0_9 0x02
| 802.11 VHT capability definition
#define | MAC_VHT_MCS_MAP_NONE 0x03
| 802.11 VHT capability definition
## HE MAC Capability Information Element definitions
#define | HE_MAC_CAPA_HTC_HE_POS 0
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_TWT_REQ_POS 1
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_TWT_RES_POS 2
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_DYNAMIC_FRAG_OFT 3
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_DYNAMIC_FRAG_WIDTH 2
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_DYNAMIC_FRAG_NOT_SUPP 0x00
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_DYNAMIC_FRAG_LEVEL_1 0x01
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_DYNAMIC_FRAG_LEVEL_2 0x02
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_DYNAMIC_FRAG_LEVEL_3 0x03
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_OFT 5
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_WIDTH 3
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_1 0x00
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_2 0x01
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_4 0x02
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_8 0x03
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_16 0x04
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_32 0x05
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_64 0x06
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_NUM_FRAG_MSDU_UNLIMITED 0x07
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MIN_FRAG_SIZE_OFT 8
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MIN_FRAG_SIZE_WIDTH 2
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MIN_FRAG_SIZE_UNLIMITED 0x00
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MIN_FRAG_SIZE_128 0x01
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MIN_FRAG_SIZE_256 0x02
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MIN_FRAG_SIZE_512 0x03
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_TF_MAC_PAD_DUR_OFT 10
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_TF_MAC_PAD_DUR_WIDTH 2
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_TF_MAC_PAD_DUR_0US 0x00
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_TF_MAC_PAD_DUR_8US 0x01
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_TF_MAC_PAD_DUR_16US 0x02
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_OFT 12
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_WIDTH 3
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_1 0x00
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_2 0x01
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_3 0x02
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_4 0x03
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_5 0x04
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_6 0x05
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_7 0x06
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_RX_8 0x07
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_LINK_ADAPTATION_OFT 15
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_LINK_ADAPTATION_WIDTH 2
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_LINK_ADAPTATION_NONE 0x00
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_LINK_ADAPTATION_RSVD 0x01
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_LINK_ADAPTATION_UNSOL 0x02
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_LINK_ADAPTATION_BOTH 0x03
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_ALL_ACK_POS 17
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_TSR_POS 18
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_BSR_POS 19
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_BCAST_TWT_POS 20
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_32BIT_BA_BITMAP_POS 21
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MU_CASCADING_POS 22
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_ACK_EN_POS 23
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_OM_CONTROL_POS 25
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_OFDMA_RA_POS 26
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_A_AMPDU_LEN_EXP_OFT 27
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_A_AMPDU_LEN_EXP_WIDTH 2
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_A_AMPDU_LEN_EXP_USE_VHT 0x00
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_A_AMPDU_LEN_EXP_VHT_1 0x01
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_A_AMPDU_LEN_EXP_VHT_2 0x02
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MAX_A_AMPDU_LEN_EXP_RSVD 0x03
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_A_AMSDU_FRAG_POS 29
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_FLEX_TWT_SCHED_POS 30
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_RX_CTRL_FRAME_TO_MULTIBSS_POS 31
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_BSRP_BQRP_A_MPDU_AGG_POS 32
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_QTP_POS 33
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_BQR_POS 34
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_SRP_RESP_POS 35
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_NDP_FB_REP_POS 36
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_OPS_POS 37
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_AMDSU_IN_AMPDU_POS 38
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_OFT 39
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_WIDTH 3
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_1 0x00
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_2 0x01
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_3 0x02
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_4 0x03
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_5 0x04
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_6 0x05
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_7 0x06
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_MULTI_TID_AGG_TX_8 0x07
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_SUB_CHNL_SEL_TX_POS 42
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_UL_2_996_TONE_RU_POS 43
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_OM_CONTROL_UL_MU_DIS_RX_POS 44
| 802.11 HE MAC capability definition
#define | HE_MAC_CAPA_DYN_SMPS_POS 45
| 802.11 HE MAC capability definition
## HE PHY Capability Information Element definitions
#define | HE_PHY_CAPA_CHAN_WIDTH_SET_OFT 1
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CHAN_WIDTH_SET_WIDTH 7
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CHAN_WIDTH_SET_40MHZ_IN_2G 0x01
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CHAN_WIDTH_SET_40MHZ_80MHZ_IN_5G 0x02
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CHAN_WIDTH_SET_160MHZ_IN_5G 0x04
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CHAN_WIDTH_SET_80PLUS80_MHZ_IN_5G 0x08
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CHAN_WIDTH_SET_RU_MAPPING_IN_2G 0x10
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CHAN_WIDTH_SET_RU_MAPPING_IN_5G 0x20
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PREAMBLE_PUNC_RX_OFT 8
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PREAMBLE_PUNC_RX_WIDTH 4
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PREAMBLE_PUNC_RX_80M_ONLY_SCND_20M 0x01
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PREAMBLE_PUNC_RX_80M_ONLY_SCND_40M 0x02
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PREAMBLE_PUNC_RX_160M_ONLY_SCND_20M 0x04
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PREAMBLE_PUNC_RX_160M_ONLY_SCND_40M 0x08
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DEVICE_CLASS_A_POS 12
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_LDPC_CODING_IN_PAYLOAD_POS 13
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_HE_SU_PPDU_1x_LTF_AND_GI_0_8US_POS 14
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MIDAMBLE_RX_MAX_NSTS_OFT 15
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MIDAMBLE_RX_MAX_NSTS_WIDTH 2
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_NDP_4x_LTF_AND_3_2US_POS 17
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_STBC_TX_UNDER_80MHZ_POS 18
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_STBC_RX_UNDER_80MHZ_POS 19
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DOPPLER_TX_POS 20
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DOPPLER_RX_POS 21
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_FULL_BW_UL_MU_MIMO_POS 22
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PARTIAL_BW_UL_MU_MIMO_POS 23
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_TX_OFT 24
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_TX_WIDTH 2
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_TX_NO_DCM 0x00
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_TX_BPSK 0x01
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_TX_QPSK 0x02
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_TX_16_QAM 0x03
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_NSS_TX_POS 26
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_RX_OFT 27
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_RX_WIDTH 2
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_RX_NO_DCM 0x00
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_RX_BPSK 0x01
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_RX_QPSK 0x02
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_CONST_RX_16_QAM 0x03
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_NSS_RX_POS 29
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_RX_HE_MU_PPDU_FRM_NON_AP_POS 30
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_SU_BEAMFORMER_POS 31
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_SU_BEAMFORMEE_POS 32
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MU_BEAMFORMER_POS 33
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_UNDER_80MHZ_OFT 34
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_UNDER_80MHZ_WIDTH 3
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_UNDER_80MHZ_4 0x03
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_UNDER_80MHZ_5 0x04
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_UNDER_80MHZ_6 0x05
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_UNDER_80MHZ_7 0x06
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_UNDER_80MHZ_8 0x07
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_ABOVE_80MHZ_OFT 37
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_ABOVE_80MHZ_WIDTH 3
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_ABOVE_80MHZ_4 0x03
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_ABOVE_80MHZ_5 0x04
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_ABOVE_80MHZ_6 0x05
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_ABOVE_80MHZ_7 0x06
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_MAX_STS_ABOVE_80MHZ_8 0x07
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_OFT 40
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_WIDTH 3
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_1 0x00
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_2 0x01
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_3 0x02
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_4 0x03
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_5 0x04
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_6 0x05
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_7 0x06
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_UNDER_80MHZ_8 0x07
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_OFT 43
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_WIDTH 3
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_1 0x00
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_2 0x01
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_3 0x02
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_4 0x03
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_5 0x04
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_6 0x05
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_7 0x06
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_BFMEE_NUM_SND_DIM_ABOVE_80MHZ_8 0x07
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_NG16_SU_FEEDBACK_POS 46
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_NG16_MU_FEEDBACK_POS 47
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CODEBOOK_SIZE_42_SU_POS 48
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_CODEBOOK_SIZE_75_MU_POS 49
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_TRIG_SU_BEAMFORMER_FB_POS 50
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_TRIG_MU_BEAMFORMER_FB_POS 51
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_TRIG_CQI_FB_POS 52
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PARTIAL_BW_EXT_RANGE_POS 53
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PARTIAL_BW_DL_MUMIMO_POS 54
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_PPE_THRESHOLD_PRESENT_POS 55
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_SRP_BASED_SR_POS 56
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_POWER_BOOST_FACTOR_AR_POS 57
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_HE_SU_MU_PPDU_4x_LTF_AND_08_US_GI_POS 58
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_OFT 59
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_WIDTH 3
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_1 0x01
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_2 0x02
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_3 0x03
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_4 0x04
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_5 0x05
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_6 0x06
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MAX_NC_7 0x07
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_STBC_TX_ABOVE_80MHZ_POS 62
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_STBC_RX_ABOVE_80MHZ_POS 63
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_HE_ER_SU_PPDU_4x_LTF_AND_08_US_GI_POS 64
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_20MHZ_IN_40MHZ_HE_PPDU_IN_2G_POS 65
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_20MHZ_IN_160MHZ_HE_PPDU_POS 66
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_80MHZ_IN_160MHZ_HE_PPDU_POS 67
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_HE_ER_SU_1x_LTF_AND_08_US_GI_POS 68
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_MIDAMBLE_RX_2x_AND_1x_LTF_POS 69
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_BW_OFT 70
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_BW_WIDTH 3
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_BW_20MHZ 0x00
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_BW_40MHZ 0x01
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_BW_80MHZ 0x02
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_DCM_MAX_BW_160MHZ_80P80MHZ 0x03
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_16PLUS_HE_SIGB_OFDM_SYM_POS 72
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_NON_TRIG_CQI_FEEDBACK_POS 73
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_TX_1024QAM_LESS_242_RU_POS 74
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_RX_1024QAM_LESS_242_RU_POS 75
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_RX_FULL_BW_SU_COMP_SIGB_POS 76
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_RX_FULL_BW_SU_NON_COMP_SIGB_POS 77
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_NOMINAL_PACKET_PADDING_OFT 78
| 802.11 HE PHY capability definition
#define | HE_PHY_CAPA_NOMINAL_PACKET_PADDING_WIDTH 2
| 802.11 HE PHY capability definition
## HE MCS MAP definitions
#define | MAC_HE_MCS_MAP_MSK 0x03
| 802.11 HE MCS map definition
#define | MAC_HE_MCS_MAP_0_7 0x00
| 802.11 HE MCS map definition
#define | MAC_HE_MCS_MAP_0_9 0x01
| 802.11 HE MCS map definition
#define | MAC_HE_MCS_MAP_0_11 0x02
| 802.11 HE MCS map definition
#define | MAC_HE_MCS_MAP_NONE 0x03
| 802.11 HE MCS map definition
## Multiple BSSID Subelement offsets, lengths and other definitions
#define | MAC_MBSSID_NON_TXED_PROF_ID_OFT 0
#define | MAC_MBSSID_NON_TXED_PROF_LEN_OFT 1
#define | MAC_MBSSID_NON_TXED_PROF_INFO_OFT 2
#define | MAC_MBSSID_NON_TXED_PROF_ELMT_MIN_LEN 4
#define | MAC_MBSSID_NON_TXED_PROF_MIN_LEN 6
## Management Frame Element definitions and offsets
#define | MAC_BEACON_MAX_LEN 333
| 802.11 Management frame element and offset definition
#define | MAC_BEACONINFO_SIZE 78
| 802.11 Management frame element and offset definition
#define | MAC_TIM_SIZE 251
| 802.11 Management frame element and offset definition
#define | MAC_BEACON_HDR_LEN 36
| 802.11 Management frame element and offset definition
#define | MAC_BEACON_TIMESTAMP_OFT MAC_SHORT_MAC_HDR_LEN
| 802.11 Management frame element and offset definition
#define | MAC_BEACON_INTERVAL_OFT (MAC_SHORT_MAC_HDR_LEN + 8)
| 802.11 Management frame element and offset definition
#define | MAC_BEACON_CAPA_OFT (MAC_SHORT_MAC_HDR_LEN + 10)
| 802.11 Management frame element and offset definition
#define | MAC_BEACON_VARIABLE_PART_OFT (MAC_SHORT_MAC_HDR_LEN + 12)
| 802.11 Management frame element and offset definition
#define | MAC_PROBEREQ_SSID_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_PROBE_TIMESTAMP_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_PROBE_INTERVAL_OFT 8
| 802.11 Management frame element and offset definition
#define | MAC_PROBE_CAPA_OFT 10
| 802.11 Management frame element and offset definition
#define | MAC_PROBE_SSID_OFT 12
| 802.11 Management frame element and offset definition
#define | MAC_AUTH_ALGONBR_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_AUTH_SEQNBR_OFT 2
| 802.11 Management frame element and offset definition
#define | MAC_AUTH_STATUS_OFT 4
| 802.11 Management frame element and offset definition
#define | MAC_AUTH_CHALLENGE_OFT 6
| 802.11 Management frame element and offset definition
#define | MAC_AUTH_CHALLENGE_LEN 128
| 802.11 Management frame element and offset definition
#define | CHALLENGE_TEXT_SIZE 130
| 802.11 Management frame element and offset definition
#define | MAC_ASSO_REQ_CAPA_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_ASSO_REQ_LISTEN_OFT 2
| 802.11 Management frame element and offset definition
#define | MAC_ASSO_REQ_SSID_OFT 4
| 802.11 Management frame element and offset definition
#define | MAC_ASSO_RSP_CAPA_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_ASSO_RSP_STATUS_OFT 2
| 802.11 Management frame element and offset definition
#define | MAC_ASSO_RSP_AID_OFT 4
| 802.11 Management frame element and offset definition
#define | MAC_ASSO_RSP_RATES_OFT 6
| 802.11 Management frame element and offset definition
#define | MAC_REASSO_REQ_CAPA_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_REASSO_REQ_LISTEN_OFT 2
| 802.11 Management frame element and offset definition
#define | MAC_REASSO_REQ_AP_ADDR_OFT 4
| 802.11 Management frame element and offset definition
#define | MAC_REASSO_REQ_SSID_OFT 10
| 802.11 Management frame element and offset definition
#define | MAC_DEAUTH_REASON_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_DISASSOC_REASON_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_DISASSOC_REASON_LEN 2
| 802.11 Management frame element and offset definition
#define | MAC_ACTION_CATEGORY_OFT 0
| 802.11 Management frame element and offset definition
#define | MAC_ACTION_ACTION_OFT 1
| 802.11 Management frame element and offset definition
#define | MAC_ACTION_TOKEN_OFT 2
| 802.11 Management frame element and offset definition
#define | MAC_ACTION_P2P_ACTION_OFT 5
| 802.11 Management frame element and offset definition
#define | MAC_ACTION_P2P_TAGGED_OFT 7
| 802.11 Management frame element and offset definition
## Action Frames categories and other definitions
#define | MAC_SPECTRUM_ACTION_CATEGORY 0
| 802.11 Action frame category
#define | MAC_WMMAC_QOS_ACTION_CATEGORY 1
| 802.11 Action frame category
#define | MAC_DLS_ACTION_CATEGORY 2
| 802.11 Action frame category
#define | MAC_BA_ACTION_CATEGORY 3
| 802.11 Action frame category
#define | MAC_PUBLIC_ACTION_CATEGORY 4
| 802.11 Action frame category
#define | MAC_RADIO_MEASURE_ACTION_CATEGORY 5
| 802.11 Action frame category
#define | MAC_FAST_BSS_ACTION_CATEGORY 6
| 802.11 Action frame category
#define | MAC_HT_ACTION_CATEGORY 7
| 802.11 Action frame category
#define | MAC_SA_QUERY_ACTION_CATEGORY 8
| 802.11 Action frame category
#define | MAC_PROT_PUBLIC_ACTION_CATEGORY 9
| 802.11 Action frame category
#define | MAC_WNM_ACTION_CATEGORY 10
| 802.11 Action frame category
#define | MAC_UNPROT_WNM_ACTION_CATEGORY 11
| 802.11 Action frame category
#define | MAC_TDLS_ACTION_CATEGORY 12
| 802.11 Action frame category
#define | MAC_MESH_ACTION_CATEGORY 13
| 802.11 Action frame category
#define | MAC_MULTIHOP_ACTION_CATEGORY 14
| 802.11 Action frame category
#define | MAC_SELF_PROT_ACTION_CATEGORY 15
| 802.11 Action frame category
#define | MAC_VHT_ACTION_CATEGORY 21
| 802.11 Action frame category
#define | MAC_VENDOR_PROT_ACTION_CATEGORY 126
| 802.11 Action frame category
#define | MAC_VENDOR_ACTION_CATEGORY 127
| 802.11 Action frame category
#define | MAC_ACTION_CATEGORY_ERROR 128
| 802.11 Action frame category
#define | MAC_P2P_ACTION_NOA_SUBTYPE 0
| 802.11 Action frame category
#define | MAC_SELF_PROT_ACTION_CAPA_OFT 2
| 802.11 Action frame category
#define | MAC_SELF_PROT_ACTION_CAPA_LEN 2
| 802.11 Action frame category
#define | MAC_SELF_PROT_ACTION_AID_OFT 4
| 802.11 Action frame category
#define | MAC_SELF_PROT_ACTION_AID_LEN 2
| 802.11 Action frame category
## WMM-AC Frames and Values definitions
#define | MAC_WMMAC_OUI_BYTE 0x00
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_OUI_TYPE_BYTE 0x50
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_OUI_SUBTYPE_BYTE 0xF2
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_HDR_OFT 0
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_TSINFO_OFT 8
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_NOM_MSDU_SIZE_OFT 11
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_MAX_MSDU_SIZE_OFT 13
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_MINSI_OFT 15
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_MAXSI_OFT 19
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_INACTIVITY_INTERVAL_OFT 23
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_SUSPENSION_INTERVAL_OFT 27
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_SERVICE_START_TIME_OFT 31
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_MIN_DATA_RATE_OFT 35
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_MEAN_DATA_RATE_OFT 39
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_PEAK_DATA_RATE_OFT 43
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_BURST_SIZE_OFT 47
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_DELAY_BOUND_OFT 51
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_MIN_PHY_RATE_OFT 55
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_SURPLUS_BW_OFT 59
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSPEC_MEDUIM_TIME_OFT 61
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSINFO_HDR_OFT 0
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_TSINFO_BODY_OFT 8
| 802.11 WMM-AC frame definition
#define | MAC_WMMSA_TSDELAY_HDR_OFT 0
| 802.11 WMM-AC frame definition
#define | MAC_WMMSA_TSDELAY_BODY_OFT 8
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_OUI_SUBTYPE_TSPEC_LEN 61
| 802.11 WMM-AC frame definition
#define | MAC_OUI_SUBTYPE_WMMAC_TSINFO_LEN 9
| 802.11 WMM-AC frame definition
#define | MAC_OUI_SUBTYPE_WMMAC_TSDELAY_LEN 10
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_TRAFIC_TYPE_OFT 0
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_TRAFIC_TYPE_MASK (CO_BIT(0))
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_TSID_OFT 1
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_TSID_MASK (CO_BIT(1)|CO_BIT(2)|CO_BIT(3)|CO_BIT(4))
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_DIRECTION_OFT 5
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_DIRECTION_MASK (CO_BIT(5)|CO_BIT(6))
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_ACCESS_POLICY_OFT 7
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_ACCESS_POLICY_MASK (CO_BIT(7)|CO_BIT(8))
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_AGGREGATION_OFT 9
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_AGGREGATION_MASK (CO_BIT(9))
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_APSD_OFT 10
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_APSD_MASK (CO_BIT(10))
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_USER_PRIORITY_OFT 11
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_USER_PRIORITY_MASK (CO_BIT(11)|CO_BIT(12)|CO_BIT(13))
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_ACK_POLICY_OFT 14
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_ACK_POLICY_MASK (CO_BIT(14)|CO_BIT(15))
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_SCHEDULE_OFT 16
| 802.11 WMM-AC frame definition
#define | MAC_TSPEC_SCHEDULE_MASK (CO_BIT(16))
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ST_ADDTS_SUCESS 0
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ST_DELTS_POOR_CHANNEL_COND 34
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ST_ADDTS_REQUEST_DECLINED 37
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ST_ADDTS_INVALID_PARAMETERS 38
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ST_ADDTS_REJ_W_SUG_CHANGES 39
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ST_ADDTS_REJ_W_DELAY_PRD 47
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_RS_DELTS_QSTA_LEAVING 36
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_RS_DELTS_END_TS 37
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_RS_DELTS_UNKOWN_TS 38
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_RS_DELTS_TIMEOUT 39
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_RS_DELTS_UNSPECIFIED 32
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ACTION_ADDTS_REQ 0
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ACTION_ADDTS_RSP 1
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ACTION_DELTS 2
| 802.11 WMM-AC frame definition
#define | MAC_WMMAC_ACTION_SCHEDULE 3
| 802.11 WMM-AC frame definition
#define | MAC_ADDTS_REQ_TSPEC_OFT 3
| 802.11 WMM-AC frame definition
#define | MAC_ADDTS_REQ_TCLASS_OFT 66
| 802.11 WMM-AC frame definition
#define | MAC_ADDTS_RSP_STATUS_OFT 3
| 802.11 WMM-AC frame definition
#define | MAC_ADDTS_RSP_TSDELAY_OFT 5
| 802.11 WMM-AC frame definition
#define | MAC_ADDTS_RSP_TSPEC_OFT 17
| 802.11 WMM-AC frame definition
#define | MAC_ADDTS_RSP_TCLASS_OFT 80
| 802.11 WMM-AC frame definition
#define | MAC_DELTS_TSINFO_OFT 2
| 802.11 WMM-AC frame definition
#define | MAC_DELTS_REASON_OFT 13
| 802.11 WMM-AC frame definition
## Block-Ack Frames and Values definitions
#define | MAC_BARINFO_PERTIDINFO_OFT 0
| 802.11 BlockAck action frame definition
#define | MAC_BARINFO_PERTIDINFO_STEP 1
| 802.11 BlockAck action frame definition
#define | MAC_BARINFO_SEQ_OFT 2
| 802.11 BlockAck action frame definition
#define | MAC_BARINFO_PERTIDINFO_TID_STEP 4
| 802.11 BlockAck action frame definition
#define | MAC_CAPA_BA_OFT 14
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_LEN 2
| 802.11 BlockAck action frame definition
#define | MAC_BA_TIMEOUT_LEN 2
| 802.11 BlockAck action frame definition
#define | MAC_BA_BARINFO_LEN 4
| 802.11 BlockAck action frame definition
#define | MAC_BA_DELBA_REASON_LEN 2
| 802.11 BlockAck action frame definition
#define | MAC_BARINFO_SEQ_FRAG 0
| 802.11 BlockAck action frame definition
#define | MAC_DELPARAMSET_START_OFT 0
| 802.11 BlockAck action frame definition
#define | MAC_DELPARAMSET_STEP_OFT 1
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_AMSDU_OFT 0
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_AMSDU_MASK CO_BIT(0)
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_POLICY_OFT 1
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_POLICY_MASK CO_BIT(1)
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_TID_OFT 2
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_TID_MASK (CO_BIT(2)|CO_BIT(3)|CO_BIT(4)|CO_BIT(5))
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_BUFFER_OFT 6
| 802.11 BlockAck action frame definition
#define | MAC_BA_PARAMSET_BUFFER_MASK 0xFFC0
| 802.11 BlockAck action frame definition
#define | MAC_BA_BARINFO_PERTIDINFO_TID_OFT 12
| 802.11 BlockAck action frame definition
#define | MAC_BA_BARINFO_PERTIDINFO_TID_MASK (CO_BIT(12)|CO_BIT(13))|(CO_BIT(14)|CO_BIT(15))
| 802.11 BlockAck action frame definition
#define | MAC_BA_BARINFO_SEQ_FRAG_OFT 0
| 802.11 BlockAck action frame definition
#define | MAC_BA_BARINFO_SEQ_FRAG_MASK (CO_BIT(0)|CO_BIT(1))|(CO_BIT(2)|CO_BIT(3))
| 802.11 BlockAck action frame definition
#define | MAC_BA_BARINFO_SEQ_STARTSEQ_OFT 4
| 802.11 BlockAck action frame definition
#define | MAC_BA_BARINFO_SEQ_STARTSEQ_MASK 0x7FF0
| 802.11 BlockAck action frame definition
#define | MAC_BA_DELPARAMSET_INIT_OFT 3
| 802.11 BlockAck action frame definition
#define | MAC_BA_DELBARINFO_INIT_MASK CO_BIT(3)
| 802.11 BlockAck action frame definition
#define | MAC_BA_DELPARAMSET_TID_OFT 4
| 802.11 BlockAck action frame definition
#define | MAC_BA_DELPARAMSET_TID_MASK (CO_BIT(4)|CO_BIT(5)|CO_BIT(6)|CO_BIT(7))
| 802.11 BlockAck action frame definition
#define | MAC_BA_ST_SUCCESS 0
| 802.11 BlockAck action frame definition
#define | MAC_BA_ST_REQUEST_REFUSED 37
| 802.11 BlockAck action frame definition
#define | MAC_BA_ST_INVALID_PARAMETERS 38
| 802.11 BlockAck action frame definition
#define | MAC_BA_RS_STA_LEAVING 36
| 802.11 BlockAck action frame definition
#define | MAC_BA_RS_END_BA 37
| 802.11 BlockAck action frame definition
#define | MAC_BA_RS_UNKNOWN_BA 38
| 802.11 BlockAck action frame definition
#define | MAC_BA_RS_TIMEOUT 39
| 802.11 BlockAck action frame definition
#define | MAC_BA_ACTION_ADDBA_REQ 0
| 802.11 BlockAck action frame definition
#define | MAC_BA_ACTION_ADDBA_RSP 1
| 802.11 BlockAck action frame definition
#define | MAC_BA_ACTION_DELBA 2
| 802.11 BlockAck action frame definition
#define | MAC_ADDBA_REQ_PARAMSET_OFT 3
| 802.11 BlockAck action frame definition
#define | MAC_ADDBA_REQ_TIMEOUT_OFT 5
| 802.11 BlockAck action frame definition
#define | MAC_ADDBA_REQ_BARINFO_OFT 7
| 802.11 BlockAck action frame definition
#define | MAC_ADDBA_RSP_STATUS_OFT 3
| 802.11 BlockAck action frame definition
#define | MAC_ADDBA_RSP_PARAMSET_OFT 5
| 802.11 BlockAck action frame definition
#define | MAC_ADDBA_RSP_TIMEOUT_OFT 7
| 802.11 BlockAck action frame definition
#define | MAC_DELBA_PARAMSET_OFT 2
| 802.11 BlockAck action frame definition
#define | MAC_DELBA_REASON_OFT 4
| 802.11 BlockAck action frame definition
## TDLS Action Frames definitions
#define | MAC_TDLS_ACTION_SETUP_REQ 0
| 802.11 TDLS action frame definition
#define | MAC_TDLS_ACTION_SETUP_RSP 1
| 802.11 TDLS action frame definition
#define | MAC_TDLS_ACTION_SETUP_CFM 2
| 802.11 TDLS action frame definition
#define | MAC_TDLS_ACTION_TEARDOWN 3
| 802.11 TDLS action frame definition
#define | MAC_TDLS_ACTION_PEER_TRAFFIC_IND 4
| 802.11 TDLS action frame definition
#define | MAC_TDLS_ACTION_CHANSW_REQ 5
| 802.11 TDLS action frame definition
#define | MAC_TDLS_ACTION_CHANSW_RSP 6
| 802.11 TDLS action frame definition
#define | MAC_TDLS_ACTION_PEER_TRAFFIC_RSP 9
| 802.11 TDLS action frame definition
#define | MAC_TDLS_ACTION_DISCOVERY_REQ 10
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQ_TARGET_CH_OFFSET 2
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQ_OP_CLASS 3
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQ_IES_OFFSET 4
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQ_IE_SEC_CH_OFT_LEN 3
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQ_IE_LINK_ID_LEN 20
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQ_IE_CH_SWITCH_TIMING_LEN 6
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQ_IE_WIDE_BW_CHAN_SWITCH_LEN 5
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_RSP_STATUS_OFFSET 2
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_RSP_IES_OFFSET 4
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQUEST_ACCEPTED 0
| 802.11 TDLS action frame definition
#define | TDLS_CHANSW_REQUEST_DECLINED 37
| 802.11 TDLS action frame definition
#define | TDLS_PEER_TRAFFIC_IND_IES_OFFSET 3
| 802.11 TDLS action frame definition
#define | TDLS_PEER_TRAFFIC_IND_IE_LINK_ID_LEN 20
| 802.11 TDLS action frame definition
#define | TDLS_PEER_TRAFFIC_IND_IE_PTI_CTRL_LEN 5
| 802.11 TDLS action frame definition
#define | TDLS_PEER_TRAFFIC_IND_IE_TPU_BUF_STATUS_LEN 3
| 802.11 TDLS action frame definition
#define | TDLS_PEER_TRAFFIC_RSP_IES_OFFSET 3
| 802.11 TDLS action frame definition
#define | TDLS_PEER_TRAFFIC_RSP_IE_LINK_ID_LEN 20
| 802.11 TDLS action frame definition
## Link Management definitions
#define | MAC_HEAD_HT_OFT 32
| 802.11 Link Management frame definition
#define | MAC_MAI_MASK 0x003C
| 802.11 Link Management frame definition
#define | MAC_MAI_OFT 2
| 802.11 Link Management frame definition
#define | MAC_MAI_IND_ASELI 14
| 802.11 Link Management frame definition
#define | MAC_MFB_MASK 0xFE00
| 802.11 Link Management frame definition
#define | MAC_MFB_OFT 9
| 802.11 Link Management frame definition
#define | NO_FEEDBACK 127
| 802.11 Link Management frame definition
#define | MAC_ADDR2_OFT 10
| 802.11 Link Management frame definition
#define | MCS_IDX3_MASK 0x0000FF
| 802.11 Link Management frame definition
#define | MCS_IDX2_MASK 0x00FF00
| 802.11 Link Management frame definition
#define | MCS_IDX1_MASK 0xFF0000
| 802.11 Link Management frame definition
#define | MCS_IDX2_OFT 8
| 802.11 Link Management frame definition
#define | MCS_IDX1_OFT 16
| 802.11 Link Management frame definition
## HT Action Frame definitions
#define | MAC_CHAN_WIDTH_HT_ACTION 0
| 802.11 HT action frame definition
#define | MAC_SMPS_HT_ACTION 1
| 802.11 HT action frame definition
#define | MAC_PSMP_HT_ACTION 2
| 802.11 HT action frame definition
#define | MAC_SET_PCO_PHASE_HT_ACTION 3
| 802.11 HT action frame definition
#define | MAC_CSI_HT_ACTION 4
| 802.11 HT action frame definition
#define | MAC_NON_COMP_BEAMFORMING_HT_ACTION 5
| 802.11 HT action frame definition
#define | MAC_COMP_BEAMFORMING_HT_ACTION 6
| 802.11 HT action frame definition
#define | MAC_ASEL_INDICES_FEEDBACK_HT_ACTION 7
| 802.11 HT action frame definition
#define | MAC_CHAN_WIDTH_WIDTH_OFT 2
| 802.11 HT action frame definition
#define | MAC_SM_PRW_CTRL_OFT 2
| 802.11 HT action frame definition
#define | MAC_SMPS_ENABLE_BIT CO_BIT(0)
| 802.11 HT action frame definition
#define | MAC_SMPS_DYNAMIC_BIT CO_BIT(1)
| 802.11 HT action frame definition
## VHT Action Frame definitions
#define | MAC_COMP_BEAMFORMING_VHT_ACTION 0
| 802.11 VHT action frame definition
#define | MAC_GROUP_ID_MGMT_VHT_ACTION 1
| 802.11 VHT action frame definition
#define | MAC_OP_MODE_NOTIF_VHT_ACTION 2
| 802.11 VHT action frame definition
#define | MAC_GROUP_ID_MGT_PAYL_LENGTH 26
| 802.11 VHT action frame definition
#define | MAC_GROUP_ID_MGT_MEMBERSHIP_OFT 2
| 802.11 VHT action frame definition
#define | MAC_GROUP_ID_MGT_USER_POS_OFT 10
| 802.11 VHT action frame definition
#define | MAC_OP_MODE_NOTIF_OPMODE_OFT 2
| 802.11 VHT action frame definition
#define | MAC_OP_MODE_NOTIF_LEN 3
| 802.11 VHT action frame definition
#define | MAC_OP_MODE_NOTIF_PARAM_LEN 1
| 802.11 VHT action frame definition
#define | MAC_OPMODE_BW_OFT 0
| 802.11 VHT action frame definition
#define | MAC_OPMODE_BW_MSK (0x3 << MAC_OPMODE_BW_OFT)
| 802.11 VHT action frame definition
#define | MAC_OPMODE_RXNSS_OFT 4
| 802.11 VHT action frame definition
#define | MAC_OPMODE_RXNSS_MSK (0x7 << MAC_OPMODE_RXNSS_OFT)
| 802.11 VHT action frame definition
#define | MAC_OPMODE_RXNSS_TYPE_BIT CO_BIT(7)
| 802.11 VHT action frame definition
## SA QUERY Action Frame definitions
#define | MAC_SA_QUERY_ACTION_OFT 1
#define | MAC_SA_QUERY_REQUEST 0
#define | MAC_SA_QUERY_RESPONSE 1
#define | MAC_SA_QUERY_TR_ID_OFT 2
#define | MAC_SA_QUERY_TR_ID_LEN 2
#define | MAC_SA_QUERY_MIN_LEN (MAC_SA_QUERY_TR_ID_OFT + MAC_SA_QUERY_TR_ID_LEN)
## Information Element Identifier definitions
#define | MAC_INFOELT_ID_OFT 0
| 802.11 IE identifier
#define | MAC_INFOELT_LEN_OFT 1
| 802.11 IE identifier
#define | MAC_INFOELT_EXT_ID_OFT 2
| 802.11 IE identifier
#define | MAC_INFOELT_INFO_OFT 2
| 802.11 IE identifier
#define | MAC_INFOELT_EXT_INFO_OFT 3
| 802.11 IE identifier
#define | MAC_ELTID_SSID 0
| 802.11 IE identifier
#define | MAC_ELTID_RATES 1
| 802.11 IE identifier
#define | MAC_ELTID_FH 2
| 802.11 IE identifier
#define | MAC_ELTID_DS 3
| 802.11 IE identifier
#define | MAC_ELTID_CF 4
| 802.11 IE identifier
#define | MAC_ELTID_TIM 5
| 802.11 IE identifier
#define | MAC_ELTID_IBSS 6
| 802.11 IE identifier
#define | MAC_ELTID_COUNTRY 7
| 802.11 IE identifier
#define | MAC_ELTID_HOP_PARAM 8
| 802.11 IE identifier
#define | MAC_ELTID_HOP_TABLE 9
| 802.11 IE identifier
#define | MAC_ELTID_REQUEST 10
| 802.11 IE identifier
#define | MAC_ELTID_BSS_LOAD 11
| 802.11 IE identifier
#define | MAC_ELTID_EDCA_PARAM 12
| 802.11 IE identifier
#define | MAC_ELTID_CHALLENGE 16
| 802.11 IE identifier
#define | MAC_ELTID_POWER_CONSTRAINT 32
| 802.11 IE identifier
#define | MAC_ELTID_POWER_CAPABILITY 33
| 802.11 IE identifier
#define | MAC_POWER_CAPABILITY_IE_LEN 2
| 802.11 IE identifier
#define | MAC_ELTID_TPC_REQUEST 34
| 802.11 IE identifier
#define | MAC_ELTID_TPC_REPORT 35
| 802.11 IE identifier
#define | MAC_ELTID_SUPPORTED_CHANNELS 36
| 802.11 IE identifier
#define | MAC_ELTID_CHANNEL_SWITCH 37
| 802.11 IE identifier
#define | MAC_ELTID_MEASUREMENT_REQUEST 38
| 802.11 IE identifier
#define | MAC_ELTID_MEASUREMENT_REPORT 39
| 802.11 IE identifier
#define | MAC_ELTID_QUIET 40
| 802.11 IE identifier
#define | MAC_ELTID_IBSS_DFS 41
| 802.11 IE identifier
#define | MAC_ELTID_ERP 42
| 802.11 IE identifier
#define | MAC_ELTID_HT_CAPA 45
| 802.11 IE identifier
#define | MAC_ELTID_QOS_CAPA 46
| 802.11 IE identifier
#define | MAC_ELTID_RSN_IEEE 48
| 802.11 IE identifier
#define | MAC_ELTID_EXT_RATES 50
| 802.11 IE identifier
#define | MAC_ELTID_MDE 54
| 802.11 IE identifier
#define | MAC_ELTID_FTE 55
| 802.11 IE identifier
#define | MAC_ELTID_SUPP_OPER_CLASS 59
| 802.11 IE identifier
#define | MAC_ELTID_EXT_CHANNEL_SWITCH 60
| 802.11 IE identifier
#define | MAC_ELTID_SEC_CH_OFFSET 62
| 802.11 IE identifier
#define | MAC_ELTID_WAPI 68
| 802.11 IE identifier
#define | MAC_ELTID_MULTIPLE_BSSID 71
| 802.11 IE identifier
#define | MAC_ELTID_20_40_COEXISTENCE 72
| 802.11 IE identifier
#define | MAC_ELTID_OBSS_SCAN_PARAM 74
| 802.11 IE identifier
#define | MAC_ELTID_MGMT_MIC 76
| 802.11 IE identifier
#define | MAC_ELTID_NON_TXED_BSSID_CAPA 83
| 802.11 IE identifier
#define | MAC_ELTID_MULTI_BSSID_INDEX 85
| 802.11 IE identifier
#define | MAC_ELTID_HT_OPERATION 61
| 802.11 IE identifier
#define | MAC_ELTID_LINK_IDENTIFIER 101
| 802.11 IE identifier
#define | MAC_ELTID_CHANNEL_SWITCH_TIMING 104
| 802.11 IE identifier
#define | MAC_ELTID_PTI_CONTROL 105
| 802.11 IE identifier
#define | MAC_ELTID_TPU_BUFFER_STATUS 106
| 802.11 IE identifier
#define | MAC_ELTID_MESH_CONF 113
| 802.11 IE identifier
#define | MAC_ELTID_MESH_ID 114
| 802.11 IE identifier
#define | MAC_ELTID_MESH_LINK_METRIC_REP 115
| 802.11 IE identifier
#define | MAC_ELTID_CONGESTION_NOTIF 116
| 802.11 IE identifier
#define | MAC_ELTID_MESH_PEER_MGMT 117
| 802.11 IE identifier
#define | MAC_ELTID_MESH_CHAN_SWITCH_PARAM 118
| 802.11 IE identifier
#define | MAC_ELTID_MESH_AWAKE_WINDOW 119
| 802.11 IE identifier
#define | MAC_ELTID_MESH_GANN 125
| 802.11 IE identifier
#define | MAC_ELTID_MESH_RANN 126
| 802.11 IE identifier
#define | MAC_ELTID_EXT_CAPA 127
| 802.11 IE identifier
#define | MAC_ELTID_MESH_PREQ 130
| 802.11 IE identifier
#define | MAC_ELTID_MESH_PREP 131
| 802.11 IE identifier
#define | MAC_ELTID_MESH_PERR 132
| 802.11 IE identifier
#define | MAC_ELTID_VHT_CAPA 191
| 802.11 IE identifier
#define | MAC_ELTID_VHT_OPERATION 192
| 802.11 IE identifier
#define | MAC_ELTID_WIDE_BANDWIDTH_CHAN_SWITCH 194
| 802.11 IE identifier
#define | MAC_ELTID_VHT_TRANSMIT_PWR_ENVELOP 195
| 802.11 IE identifier
#define | MAC_ELTID_CHAN_SWITCH_WRP 196
| 802.11 IE identifier
#define | MAC_ELTID_OP_MODE_NOTIF 199
| 802.11 IE identifier
#define | MAC_ELTID_OUI 221
| 802.11 IE identifier
#define | MAC_ELTID_EXT 255
| 802.11 IE identifier
#define | MAC_OUI_TYPE_WPA 1
| 802.11 IE identifier
#define | MAC_OUI_TYPE_WME 2
| 802.11 IE identifier
#define | MAC_OUI_SUBTYPE_WME_INFORMATION 0
| 802.11 IE identifier
#define | MAC_OUI_SUBTYPE_WME_PARAMETER 1
| 802.11 IE identifier
#define | MAC_OUI_TYPE_WMMAC 2
| 802.11 IE identifier
#define | MAC_OUI_SUBTYPE_WMMAC_TSPEC 2
| 802.11 IE identifier
#define | MAC_OUI_SUBTYPE_WMMAC_TSDELAY 8
| 802.11 IE identifier
#define | MAC_OUI_SUBTYPE_WMMAC_TSINFO 10
| 802.11 IE identifier
#define | MAC_ELTID_EXT_HE_CAPA 35
| 802.11 IE identifier
#define | MAC_ELTID_EXT_HE_OPERATION 36
| 802.11 IE identifier
#define | MAC_ELTID_EXT_UORA 37
| 802.11 IE identifier
#define | MAC_ELTID_EXT_MU_EDCA 38
| 802.11 IE identifier
## Information Subelement Identifier definitions for Multiple BSSID element
#define | MAC_SUBID_MBSSID_NON_TXED_PROF 0
| 802.11 Multiple BSSID subelement identifier
#define | MAC_SUBID_MBSSID_VENDOR_SPECIFIC 221
| 802.11 Multiple BSSID subelement identifier
## Standard Status Code definitions
#define | MAC_ST_SUCCESSFUL 0
| 802.11 Status Code
#define | MAC_ST_FAILURE 1
| 802.11 Status Code
#define | MAC_ST_RESERVED 2
| 802.11 Status Code
#define | MAC_ST_CAPA_NOT_SUPPORTED 10
| 802.11 Status Code
#define | MAC_ST_REASSOC_NOT_ASSOC 11
| 802.11 Status Code
#define | MAC_ST_ASSOC_DENIED 12
| 802.11 Status Code
#define | MAC_ST_AUTH_ALGO_NOT_SUPPORTED 13
| 802.11 Status Code
#define | MAC_ST_AUTH_FRAME_WRONG_SEQ 14
| 802.11 Status Code
#define | MAC_ST_AUTH_CHALLENGE_FAILED 15
| 802.11 Status Code
#define | MAC_ST_AUTH_TIMEOUT 16
| 802.11 Status Code
#define | MAC_ST_ASSOC_TOO_MANY_STA 17
| 802.11 Status Code
#define | MAC_ST_ASSOC_RATES_NOT_SUPPORTED 18
| 802.11 Status Code
#define | MAC_ST_ASSOC_PREAMBLE_NOT_SUPPORTED 19
| 802.11 Status Code
#define | MAC_ST_ASSOC_SPECTRUM_REQUIRED 22
| 802.11 Status Code
#define | MAC_ST_ASSOC_POWER_CAPA 23
| 802.11 Status Code
#define | MAC_ST_ASSOC_SUPPORTED_CHANNEL 24
| 802.11 Status Code
#define | MAC_ST_ASSOC_SLOT_NOT_SUPPORTED 25
| 802.11 Status Code
#define | MAC_ST_REFUSED_TEMPORARILY 30
| 802.11 Status Code
#define | MAC_ST_INVALID_MFP_POLICY 31
| 802.11 Status Code
#define | MAC_ST_INVALID_IE 40
| 802.11 Status Code
#define | MAC_ST_GROUP_CIPHER_INVALID 41
| 802.11 Status Code
#define | MAC_ST_PAIRWISE_CIPHER_INVALID 42
| 802.11 Status Code
#define | MAC_ST_AKMP_INVALID 43
| 802.11 Status Code
#define | MAC_ST_UNSUPPORTED_RSNE_VERSION 44
| 802.11 Status Code
#define | MAC_ST_INVALID_RSNE_CAPA 45
| 802.11 Status Code
#define | MAC_ST_CIPHER_SUITE_REJECTED 46
| 802.11 Status Code
## Standard Reason Code definitions
#define | MAC_RS_RESERVED 0
| 802.11 Reason Code
#define | MAC_RS_UNSPECIFIED 1
| 802.11 Reason Code
#define | MAC_RS_PREVIOUS_AUTH_NOT_VALID 2
| 802.11 Reason Code
#define | MAC_RS_DEAUTH_SENDER_LEFT_IBSS_ESS 3
| 802.11 Reason Code
#define | MAC_RS_DIASSOC_INACTIVITY 4
| 802.11 Reason Code
#define | MAC_RS_DIASSOC_TOO_MANY_STA 5
| 802.11 Reason Code
#define | MAC_RS_CLASS_2_FORBIDDEN 6
| 802.11 Reason Code
#define | MAC_RS_CLASS_3_FORBIDDEN 7
| 802.11 Reason Code
#define | MAC_RS_DEAUTH_SENDER_LEFT_BSS 8
| 802.11 Reason Code
#define | MAC_RS_STA_REQ_ASSOC_NOT_AUTH 9
| 802.11 Reason Code
#define | MAC_RS_DIASSOC_POWER_CAPA 10
| 802.11 Reason Code
#define | MAC_RS_DIASSOC_SUPPORTED_CHANNEL 11
| 802.11 Reason Code
#define | MAC_RS_RESERVED_12 12
| 802.11 Reason Code
#define | MAC_RS_INVALID_IE 13
| 802.11 Reason Code
#define | MAC_RS_MIC_FAILURE 14
| 802.11 Reason Code
#define | MAC_RS_4WAY_HANDSHAKE_TIMEOUT 15
| 802.11 Reason Code
#define | MAC_RS_GROUP_KEY_UPDATE_TIMEOUT 16
| 802.11 Reason Code
#define | MAC_RS_BAD_RSNIE 17
| 802.11 Reason Code
#define | MAC_RS_GROUP_CIPHER_INVALID 18
| 802.11 Reason Code
#define | MAC_RS_PAIRWISE_CIPHER_INVALID 19
| 802.11 Reason Code
#define | MAC_RS_AKMP_INVALID 20
| 802.11 Reason Code
#define | MAC_RS_UNSUPPORTED_RSNE_VERSION 21
| 802.11 Reason Code
#define | MAC_RS_INVALID_RSNE_CAPA 22
| 802.11 Reason Code
#define | MAC_RS_802_1X_AUTH_FAIL 23
| 802.11 Reason Code
#define | MAC_RS_CIPHER_SUITE_REJECTED 24
| 802.11 Reason Code
#define | MAC_RS_TIMEOUT 39
| 802.11 Reason Code
## WMMIE definitions
#define | MAC_WME_PARAM_LEN 16
| WMM IE definition.
#define | MAC_RAW_WME_INFO_ELMT_DEFAULT
| Default WME information element format.
#define | MAC_ACI_BE 0
| WMM IE definition.
#define | MAC_ACI_BK 1
| WMM IE definition.
#define | MAC_ACI_VI 2
| WMM IE definition.
#define | MAC_ACI_VO 3
| WMM IE definition.
#define | MAC_ACI_OFT 5
| WMM IE definition.
#define | MAC_ECWMIN 4
| WMM IE definition.
#define | MAC_ECWMAX 10
| WMM IE definition.
#define | MAC_ECW_BK_MIN MAC_ECWMIN
| WMM IE definition.
#define | MAC_ECW_BE_MIN MAC_ECWMIN
| WMM IE definition.
#define | MAC_ECW_VI_MIN ((MAC_ECWMIN) - 1)
| WMM IE definition.
#define | MAC_ECW_VO_MIN ((MAC_ECWMIN)/2)
| WMM IE definition.
#define | MAC_ECW_BK_MAX MAC_ECWMAX
| WMM IE definition.
#define | MAC_ECW_BE_MAX MAC_ECWMAX
| WMM IE definition.
#define | MAC_ECW_VI_MAX MAC_ECWMIN
| WMM IE definition.
#define | MAC_ECW_VO_MAX ((MAC_ECWMIN) - 1)
| WMM IE definition.
#define | MAC_AIFSN_BK 7
| WMM IE definition.
#define | MAC_AIFSN_BE 3
| WMM IE definition.
#define | MAC_AIFSN_VI 2
| WMM IE definition.
#define | MAC_AIFSN_VO 2
| WMM IE definition.
#define | MAC_AC_BE_TXOP 0
| WMM IE definition.
#define | MAC_AC_BK_TXOP 0
| WMM IE definition.
#define | MAC_AC_VI_TXOP_b 188
| WMM IE definition.
#define | MAC_AC_VI_TXOP_ag 94
| WMM IE definition.
#define | MAC_AC_VO_TXOP_b 102
| WMM IE definition.
#define | MAC_AC_VO_TXOP_ag 47
| WMM IE definition.
## RSNIE definitions
#define | MAC_RSNIE_CIPHER_USE_GROUP 0x000FAC00
#define | MAC_RSNIE_CIPHER_WEP_40 0x000FAC01
#define | MAC_RSNIE_CIPHER_TKIP 0x000FAC02
#define | MAC_RSNIE_CIPHER_RSVD 0x000FAC03
#define | MAC_RSNIE_CIPHER_CCMP_128 0x000FAC04
#define | MAC_RSNIE_CIPHER_WEP_104 0x000FAC05
#define | MAC_RSNIE_CIPHER_BIP_CMAC_128 0x000FAC06
#define | MAC_RSNIE_CIPHER_NO_GROUP 0x000FAC07
#define | MAC_RSNIE_CIPHER_GCMP_128 0x000FAC08
#define | MAC_RSNIE_CIPHER_GCMP_256 0x000FAC09
#define | MAC_RSNIE_CIPHER_CCMP_256 0x000FAC0A
#define | MAC_RSNIE_CIPHER_BIP_GMAC_128 0x000FAC0B
#define | MAC_RSNIE_CIPHER_BIP_GMAC_256 0x000FAC0C
#define | MAC_RSNIE_CIPHER_BIP_CMAC_256 0x000FAC0D
#define | MAC_RSNIE_AKM_8021X 0x000FAC01
#define | MAC_RSNIE_AKM_PSK 0x000FAC02
#define | MAC_RSNIE_AKM_FT_8021X 0x000FAC03
#define | MAC_RSNIE_AKM_FT_PSK 0x000FAC04
#define | MAC_RSNIE_AKM_8021X_SHA256 0x000FAC05
#define | MAC_RSNIE_AKM_PSK_SHA256 0x000FAC06
#define | MAC_RSNIE_AKM_TDLS 0x000FAC07
#define | MAC_RSNIE_AKM_SAE 0x000FAC08
#define | MAC_RSNIE_AKM_FT_OVER_SAE 0x000FAC09
#define | MAC_RSNIE_AKM_8021X_SUITE_B 0x000FAC0B
#define | MAC_RSNIE_AKM_8021X_SUITE_B_192 0x000FAC0C
#define | MAC_RSNIE_AKM_FILS_SHA256 0x000FAC0D
#define | MAC_RSNIE_AKM_FILS_SHA384 0x000FAC0F
#define | MAC_RSNIE_AKM_FT_FILS_SHA256 0x000FAC10
#define | MAC_RSNIE_AKM_FT_FILS_SHA384 0x000FAC11
#define | MAC_RSNIE_AKM_OWE 0x000FAC12
#define | MAC_RSNIE_CAPA_PREAUTH_BIT CO_BIT(0)
#define | MAC_RSNIE_CAPA_NO_PAIRWISE_BIT CO_BIT(1)
#define | MAC_RSNIE_CAPA_PTKSA_REPLAY_CNT_MSK 0x000C
#define | MAC_RSNIE_CAPA_GTKSA_REPLAY_CNT_MSK 0x0030
#define | MAC_RSNIE_CAPA_MFPR_BIT CO_BIT(6)
#define | MAC_RSNIE_CAPA_MFPC_BIT CO_BIT(7)
#define | MAC_RSNIE_CAPA_JOINT_MULIT_BAND_BIT CO_BIT(8)
#define | MAC_RSNIE_CAPA_PEERKEY_BIT CO_BIT(9)
#define | MAC_RSNIE_CAPA_SPP_AMSDU_CAP_BIT CO_BIT(10)
#define | MAC_RSNIE_CAPA_SPP_AMSDU_REQ_BIT CO_BIT(11)
#define | MAC_RSNIE_CAPA_PBAC_BIT CO_BIT(12)
#define | MAC_RSNIE_CAPA_EXT_KEY_ID_BIT CO_BIT(13)
## WPA (pre-RSN) definitions
#define | MAC_WPA_CIPHER_TKIP 0x0050F202
#define | MAC_WPA_CIPHER_CCMP 0x0050F204
#define | MAC_WPA_AKM_8021X 0x0050F201
#define | MAC_WPA_AKM_PSK 0x0050F202
## WAPI definitions
#define | MAC_WAPI_CIPHER_WPI_SMS4 0x00147201
#define | MAC_WAPI_AKM_CERT 0x00147201
#define | MAC_WAPI_AKM_PSK 0x00147202
## Country IE definitions
#define | MAC_COUNTRY_2G4_FULL { 3, {'x', 'x', ' '}, { 1, 14, 30}}
| Country IE definition.
#define | MAC_COUNTRY_2G4_USA { 6, {'U', 'S', ' '}, { 1, 11, 30}}
| Country IE definition.
#define | MAC_COUNTRY_2G4_CANADA { 6, {'C', 'A', ' '}, { 1, 11, 30}}
| Country IE definition.
#define | MAC_COUNTRY_2G4_EUROPE { 6, {'E', 'U', ' '}, { 1, 13, 30}}
| Country IE definition.
#define | MAC_COUNTRY_2G4_SPAIN { 6, {'S', 'P', ' '}, {10, 2, 30}}
| Country IE definition.
#define | MAC_COUNTRY_2G4_FRANCE { 6, {'F', 'R', ' '}, {10, 4, 20}}
| Country IE definition.
#define | MAC_COUNTRY_2G4_JAPAN { 6, {'J', 'P', ' '}, {14, 1, 30}}
| Country IE definition.
#define | MAC_COUNTRY_2G4_CHINA { 6, {'C', 'N', ' '}, { 1, 13, 30}}
| Country IE definition.
#define | MAC_COUNTRY_5G_FULL { 3, {'x', 'x', ' '}, {{ 36, 8, 23}}}
| Country IE definition.

## Detailed Description

Common MAC types, defines and utils functions.

This module contains various types and definitions related to 802.11 standard and used by all MACSW fimware modules.

- Types, definitions and functions that are only used internally

- Definitions for various fields found in 802.11 frames

- Information Elements (IE) parsing functions

- Types and definitions that are used by the MACSW firmware and integration layers

## Define Documentation

struct he_trigger_base __PACKED __attribute__ ((__packed__))

Pack a structure field.

Base structure of a HE Trigger frame.

Base part of the User Info field present in the HE trigger frames.

Structure of the User Info part of the HE Basic Trigger frame.

Structure of A-MSDU Header.

Structure of a Compressed Block Acknowledgment frame.

Multi-STA AID/TID info field.

Structure of BA SSC + 256-bit bitmap.

Structure of BA SSC + 128-bit bitmap.

Structure of BA SSC + 64-bit bitmap.

Structure of BA SSC + 32-bit bitmap.

Structure of generic BA SSC + bitmap.

Base structure of a Block Acknowledgment frame.

Structure of a Block Acknowledgment Request frame.

Structure of a Probe Request frame.

Structure of a Beacon or ProbeRsp frame.

Structure of Ethernet Header.

Structure of a 4-address QoS Data frame MAC header.

Structure of a 4-address Data frame MAC header.

Structure of a QoS Data + HTC frame MAC header.

Structure of a QoS Data frame MAC header.

Structure of a Data/Management frame MAC header.

Structure of a long control frame MAC header.

Definition at line 31 of file compiler.h.

Referenced by co_read32p(), co_read64p(), and co_write32p().

#define HE_MAC_CAPA_BIT_CLR | ( | he_cap,
|  | bit |  | ) |

Value:

    co_bit_clr((he_cap)->mac_cap_info,         \
                                                             HE_MAC_CAPA_##bit##_POS)

Clear a bit in the HE MAC capability element.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | bit | Bit to be cleared

Definition at line 308 of file mac.h.

#define HE_MAC_CAPA_BIT_IS_SET | ( | he_cap,
|  | bit |  | ) |

Value:

    co_bit_is_set((he_cap)->mac_cap_info,      \
                                                                HE_MAC_CAPA_##bit##_POS)

Test if a bit in the HE MAC capability element is set.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | bit | Bit to be set

Returns:
  true if set, false otherwise

Definition at line 288 of file mac.h.

#define HE_MAC_CAPA_BIT_SET | ( | he_cap,
|  | bit |  | ) |

Value:

    co_bit_set((he_cap)->mac_cap_info,         \
                                                              HE_MAC_CAPA_##bit##_POS)

Set a bit in the HE MAC capability element.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | bit | Bit to be set

Definition at line 298 of file mac.h.

#define HE_MAC_CAPA_VAL_GET | ( | he_cap,
|  | field |  | ) |

Value:

    co_val_get((he_cap)->mac_cap_info,         \
                                                             HE_MAC_CAPA_##field##_OFT,      \
                                                             HE_MAC_CAPA_##field##_WIDTH)

Get the value of a bit field in the HE MAC capability element.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | field | Bit field to be read

Returns:
  The value of the field

Definition at line 263 of file mac.h.

Referenced by me_get_ampdu_params().

#define HE_MAC_CAPA_VAL_SET | ( | he_cap,
|  | field,
|  | val |  | ) |

Value:

    co_val_set((he_cap)->mac_cap_info,       \
                                                               HE_MAC_CAPA_##field##_OFT,    \
                                                               HE_MAC_CAPA_##field##_WIDTH,  \
                                                               HE_MAC_CAPA_##field##_##val)

Set the value of a bit field in the HE MAC capability element.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | field | Bit field to be written
  `[in]` | val | The value of the field

Definition at line 275 of file mac.h.

#define HE_PHY_CAPA_BIT_CLR | ( | he_cap,
|  | bit |  | ) |

Value:

    co_bit_clr((he_cap)->phy_cap_info,         \
                                                             HE_PHY_CAPA_##bit##_POS)

Clear a bit in the HE PHY capability element.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | bit | Bit to be cleared

Definition at line 364 of file mac.h.

#define HE_PHY_CAPA_BIT_IS_SET | ( | he_cap,
|  | bit |  | ) |

Value:

    co_bit_is_set((he_cap)->phy_cap_info,      \
                                                                HE_PHY_CAPA_##bit##_POS)

Test if a bit in the HE PHY capability element is set.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | bit | Bit to be set

Returns:
  true if set, false otherwise

Definition at line 344 of file mac.h.

Referenced by me_config_req_handler(), and me_set_sta_ht_vht_param().

#define HE_PHY_CAPA_BIT_SET | ( | he_cap,
|  | bit |  | ) |

Value:

    co_bit_set((he_cap)->phy_cap_info,         \
                                                             HE_PHY_CAPA_##bit##_POS)

Set a bit in the HE PHY capability element.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | bit | Bit to be set

Definition at line 354 of file mac.h.

#define HE_PHY_CAPA_VAL_GET | ( | he_cap,
|  | field |  | ) |

Value:

    co_val_get((he_cap)->phy_cap_info,         \
                                                             HE_PHY_CAPA_##field##_OFT,      \
                                                             HE_PHY_CAPA_##field##_WIDTH)

Get the value of a bit field in the HE PHY capability element.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | field | Bit field to be read

Returns:
  The value of the field

Definition at line 319 of file mac.h.

Referenced by me_set_sta_ht_vht_param().

#define HE_PHY_CAPA_VAL_SET | ( | he_cap,
|  | field,
|  | val |  | ) |

Value:

    co_val_set((he_cap)->phy_cap_info,       \
                                                               HE_PHY_CAPA_##field##_OFT,    \
                                                               HE_PHY_CAPA_##field##_WIDTH,  \
                                                               HE_PHY_CAPA_##field##_##val)

Set the value of a bit field in the HE PHY capability element.

Parameters:

  `[in]` | he_cap | Pointer to the HE capability structure
  `[in]` | field | Bit field to be written
  `[in]` | val | The value of the field

Definition at line 331 of file mac.h.

#define MAC_ADDR_CMP | ( | addr1_ptr,
|  | addr2_ptr |  | ) |

Value:

    ((*(((uint16_t*)(addr1_ptr)) + 0) == *(((uint16_t*)(addr2_ptr)) + 0)) &&            \
         (*(((uint16_t*)(addr1_ptr)) + 1) == *(((uint16_t*)(addr2_ptr)) + 1)) &&            \
         (*(((uint16_t*)(addr1_ptr)) + 2) == *(((uint16_t*)(addr2_ptr)) + 2)))

Compare two MAC addresses.

The MAC addresses MUST be 16 bit aligned.

Parameters:

  `[in]` | addr1_ptr | Pointer to the first MAC address.
  `[in]` | addr2_ptr | Pointer to the second MAC address.

Returns:
  True if equal, false if not.

Definition at line 67 of file mac.h.

Referenced by rxu_cntrl_pm_mon_check(), rxu_mgt_frame_check(), rxu_mgt_search_rx_vif(), scanu_join_frame_handler(), scanu_scan_frame_handler(), tdls_check_tdls_channel_switch_response(), and tdls_check_tdls_peer_traffic_response().

#define MAC_ADDR_CMP_PACKED | ( | __a1,
|  | __a2 |  | ) | (memcmp(__a1, __a2, MAC_ADDR_LEN) == 0)

Compare two MAC addresses whose alignment is not known.

Parameters:

  `[in]` | __a1 | Pointer to the first MAC address.
  `[in]` | __a2 | Pointer to the second MAC address.

Returns:
  True if equal, false if not.

Definition at line 80 of file mac.h.

Referenced by rxu_cntrl_spurious_check().

#define MAC_ADDR_CPY | ( | addr1_ptr,
|  | addr2_ptr |  | ) |

Value:

    *(((uint16_t*)(addr1_ptr)) + 0) = *(((uint16_t*)(addr2_ptr)) + 0);                  \
        *(((uint16_t*)(addr1_ptr)) + 1) = *(((uint16_t*)(addr2_ptr)) + 1);                  \
        *(((uint16_t*)(addr1_ptr)) + 2) = *(((uint16_t*)(addr2_ptr)) + 2)

Copy a MAC address.

The MAC addresses MUST be 16 bit aligned.

Parameters:

  `[in]` | addr1_ptr | Pointer to the destination MAC address.
  `[in]` | addr2_ptr | Pointer to the source MAC address.

Definition at line 91 of file mac.h.

Referenced by me_build_associate_req(), rxu_cntrl_get_da_sa(), rxu_cntrl_mac2eth_update(), scanu_scan_frame_handler(), tdls_keep_alive_evt(), txl_frame_send_tdls_channel_switch_req_frame(), txl_frame_send_tdls_channel_switch_rsp_frame(), txl_frame_send_tdls_peer_traffic_ind_frame(), txu_cntrl_amsdu_hdr_append(), and txu_cntrl_mac_hdr_append().

#define MAC_ADDR_GROUP | ( | mac_addr_ptr |  | ) | ((*((uint8_t *)(mac_addr_ptr))) & 1)

Check if MAC address is a group address: test the multicast bit.

Parameters:

  `[in]` | mac_addr_ptr | Pointer to the MAC address to be checked.

Returns:
  0 if unicast address, 1 otherwise

Definition at line 115 of file mac.h.

Referenced by rxu_cntrl_machdr_read(), rxu_mgt_frame_check(), scanu_join_req_handler(), scanu_scan_frame_handler(), txl_frame_push(), and txl_hwdesc_config_post().

#define MAC_HE_CAPA_MAX_LEN

Value:

    (MAC_HE_MCS_INFO_OFT + 3 * MAC_HE_MCS_INFO_PER_BW_LEN +\
                                                    MAC_HE_PPE_THRES_MAX_LEN)

802.11 information element definition

Definition at line 1103 of file mac_frame.h.

#define MAC_HTC_HE | ( | a_control |  | ) | (MAC_HTC_TYPE_HE | ((a_control) << MAC_HTC_HE_A_CONTROL_OFT))

Format a +HTC HE Variant field.

The macro gets the A-Control subfield and format the corresponding +HTC HE field.

Parameters:

  `[in]` | a_control | A-Control subfield

Returns:
  The formatted +HTC HE Variant field

Definition at line 411 of file mac_frame.h.

#define MAC_HTC_HE_CTRL | ( | id,
|  | info |  | ) | (MAC_HTC_HE_CTRL_ID_##id | ((info) << MAC_HTC_HE_CTRL_INFO_OFT))

Format a control subfield for a +HTC HE.

The macro gets the control id and control information as parameter and group them to form the corresponding control subfield.

Parameters:

  `[in]` | id | Control ID (e.g. UPH, BSR, OM, etc.)
  `[in]` | info | Control information

Returns:
  The formatted control subfield

Definition at line 398 of file mac_frame.h.

#define MAC_PROT_ERP_STATUS_MASK

Value:

    (MAC_PROT_NONERP_PRESENT_BIT |                \
                                                MAC_PROT_USE_PROTECTION_BIT |                \
                                                MAC_PROT_BARKER_PREAMB_BIT)

ERP protection status mask.

Definition at line 227 of file mac.h.

Referenced by me_erp_prot_check().

#define MAC_QOSCTRL_HE_QUEUE_SIZE

Value:

    (MAC_QOSCTRL_QUEUE_SIZE_PRESENT |                \
                                             MAC_QOSCTRL_QUEUE_SIZE_UNKNOWN)

802.11 QoS control definition

Definition at line 313 of file mac_frame.h.

#define MAC_RAW_WME_INFO_ELMT_DEFAULT

Value:

    {                                                                             \
        MAC_ELTID_OUI, 0x07,                                                      \
        0x00, 0x50, 0xF2, MAC_OUI_TYPE_WME,         /* additionnal WPA OUI     */ \
        MAC_OUI_SUBTYPE_WME_INFORMATION, 0x01,      /* OUI subtype and version */ \
        0x00                                        /* QoS field               */ \
    }

Default WME information element format.

Definition at line 2130 of file mac_frame.h.

Referenced by me_build_associate_req().

#define MAC_SSID_CMP | ( | ssid1_ptr,
|  | ssid2_ptr |  | ) |

Value:

    (((ssid1_ptr)->length == (ssid2_ptr)->length) &&                                    \
         (memcmp((&(ssid1_ptr)->array[0]), (&(ssid2_ptr)->array[0]), (ssid1_ptr)->length) == 0))

Compare two SSID.

Parameters:

  `[in]` | ssid1_ptr | Pointer to the first SSID structure.
  `[in]` | ssid2_ptr | Pointer to the second SSID structure.

Returns:
  True if equal, false if not.

Definition at line 104 of file mac.h.

Referenced by scanu_is_scanned_ssid().

## Enumeration Type Documentation

enum mac_ac

Access Category enumeration.

Enumerator:

  AC_BK | Background.
  AC_BE | Best-effort.
  AC_VI | Video.
  AC_VO | Voice.
  AC_MAX | Number of access categories.

Definition at line 325 of file mac_types.h.

enum mac_akm_suite

Authentication and Key Management suite.

Enumerator:

  MAC_AKM_NONE | No security.
  MAC_AKM_PRE_RSN | Pre RSN (WEP or WPA).
  MAC_AKM_8021X | 00-0F-AC 1
  MAC_AKM_PSK | 00-0F-AC 2
  MAC_AKM_FT_8021X | 00-0F-AC 3
  MAC_AKM_FT_PSK | 00-0F-AC 4
  MAC_AKM_8021X_SHA256 | 00-0F-AC 5
  MAC_AKM_PSK_SHA256 | 00-0F-AC 6
  MAC_AKM_TDLS | 00-0F-AC 7
  MAC_AKM_SAE | 00-0F-AC 8
  MAC_AKM_FT_OVER_SAE | 00-0F-AC 9
  MAC_AKM_8021X_SUITE_B | 00-0F-AC 11
  MAC_AKM_8021X_SUITE_B_192 | 00-0F-AC 12
  MAC_AKM_FILS_SHA256 | 00-0F-AC 14
  MAC_AKM_FILS_SHA384 | 00-0F-AC 15
  MAC_AKM_FT_FILS_SHA256 | 00-0F-AC 16
  MAC_AKM_FT_FILS_SHA384 | 00-0F-AC 17
  MAC_AKM_OWE | 00-0F-AC 18
  MAC_AKM_WAPI_CERT | 00-14-72 1
  MAC_AKM_WAPI_PSK | 00-14-72 2

Definition at line 190 of file mac_types.h.

enum mac_bss_membership

BSS Membership Selector definitions.

Enumerator:

  MAC_BSS_MEMBERSHIP_HT_PHY | HT PHY.
  MAC_BSS_MEMBERSHIP_VHT_PHY | VHT PHY.

Definition at line 292 of file mac_types.h.

enum mac_chan_band

Channel Band.

Enumerator:

  PHY_BAND_2G4 | 2.4GHz Band
  PHY_BAND_5G | 5GHz band
  PHY_BAND_MAX | Number of bands.

Definition at line 80 of file mac_types.h.

enum mac_chan_bandwidth

Operating Channel Bandwidth.

Enumerator:

  PHY_CHNL_BW_20 | 20MHz BW
  PHY_CHNL_BW_40 | 40MHz BW
  PHY_CHNL_BW_80 | 80MHz BW
  PHY_CHNL_BW_160 | 160MHz BW
  PHY_CHNL_BW_80P80 | 80+80MHz BW
  PHY_CHNL_BW_OTHER | Reserved BW.

Definition at line 91 of file mac_types.h.

enum mac_chan_flags

Channel Flag.

Enumerator:

  CHAN_NO_IR | Cannot initiate radiation on this channel.
  CHAN_DISABLED | Channel is not allowed.
  CHAN_RADAR | Radar detection required on this channel.

Definition at line 114 of file mac_types.h.

enum mac_cipher_suite

Cipher suites (order is important as it is used by MACHW).

Enumerator:

  MAC_CIPHER_WEP40 | 00-0F-AC 1
  MAC_CIPHER_TKIP | 00-0F-AC 2
  MAC_CIPHER_CCMP | 00-0F-AC 4
  MAC_CIPHER_WEP104 | 00-0F-AC 5
  MAC_CIPHER_WPI_SMS4 | 00-14-72 1
  MAC_CIPHER_BIP_CMAC_128 | 00-0F-AC 6 (aka AES_CMAC)
  MAC_CIPHER_GCMP_128 | 00-0F-AC 08
  MAC_CIPHER_GCMP_256 | 00-0F-AC 09
  MAC_CIPHER_CCMP_256 | 00-0F-AC 10
  MAC_CIPHER_BIP_GMAC_128 | 00-0F-AC 11
  MAC_CIPHER_BIP_GMAC_256 | 00-0F-AC 12
  MAC_CIPHER_BIP_CMAC_256 | 00-0F-AC 13

Definition at line 157 of file mac_types.h.

enum mac_connection_flags

Connection flags.

Enumerator:

  CONTROL_PORT_HOST | Flag indicating whether the control port is controlled by host or not.
  CONTROL_PORT_NO_ENC | Flag indicating whether the control port frame shall be sent unencrypted.
  DISABLE_HT | Flag indicating whether HT and VHT shall be disabled or not.
  WPA_WPA2_IN_USE | Flag indicating whether WPA or WPA2 authentication is in use.
  MFP_IN_USE | Flag indicating whether MFP is in use.

Definition at line 454 of file mac_types.h.

enum mac_legacy_rates

Legacy rate 802.11 definitions.

Enumerator:

  MAC_RATE_1MBPS | DSSS/CCK 1Mbps.
  MAC_RATE_2MBPS | DSSS/CCK 2Mbps.
  MAC_RATE_5_5MBPS | DSSS/CCK 5.5Mbps.
  MAC_RATE_6MBPS | OFDM 6Mbps.
  MAC_RATE_9MBPS | OFDM 9Mbps.
  MAC_RATE_11MBPS | DSSS/CCK 11Mbps.
  MAC_RATE_12MBPS | OFDM 12Mbps.
  MAC_RATE_18MBPS | OFDM 18Mbps.
  MAC_RATE_24MBPS | OFDM 24Mbps.
  MAC_RATE_36MBPS | OFDM 36Mbps.
  MAC_RATE_48MBPS | OFDM 48Mbps.
  MAC_RATE_54MBPS | OFDM 54Mbps.

Definition at line 263 of file mac_types.h.

enum mac_sta_flags

Station flags.

Enumerator:

  STA_QOS_CAPA | Bit indicating that a STA has QoS (WMM) capability.
  STA_HT_CAPA | Bit indicating that a STA has HT capability.
  STA_VHT_CAPA | Bit indicating that a STA has VHT capability.
  STA_MFP_CAPA | Bit indicating that a STA has MFP capability.
  STA_OPMOD_NOTIF | Bit indicating that the STA included the Operation Notification IE.
  STA_HE_CAPA | Bit indicating that a STA has HE capability.

Definition at line 437 of file mac_types.h.

enum mac_tid

Traffic ID enumeration.

Enumerator:

  TID_0 | TID_0. Mapped to AC_BE as per 802.11 standard.
  TID_1 | TID_1. Mapped to AC_BK as per 802.11 standard.
  TID_2 | TID_2. Mapped to AC_BK as per 802.11 standard.
  TID_3 | TID_3. Mapped to AC_BE as per 802.11 standard.
  TID_4 | TID_4. Mapped to AC_VI as per 802.11 standard.
  TID_5 | TID_5. Mapped to AC_VI as per 802.11 standard.
  TID_6 | TID_6. Mapped to AC_VO as per 802.11 standard.
  TID_7 | TID_7. Mapped to AC_VO as per 802.11 standard.
  TID_MGT | Non standard Management TID used internally.
  TID_MAX | Number of TID supported.

Definition at line 340 of file mac_types.h.

enum mac_vif_type

Interface types.

Enumerator:

  VIF_STA | ESS STA interface.
  VIF_IBSS | IBSS STA interface.
  VIF_AP | AP interface.
  VIF_MESH_POINT | Mesh Point interface.
  VIF_MONITOR | Monitor interface.
  VIF_UNKNOWN | Unknown type.

Definition at line 33 of file mac_types.h.

## Function Documentation

enum mac_akm_suite mac_akm_suite_value | ( | uint32_t | akm_suite | ) |

Convert IEE802.11 AKM suite into enum mac_akm_suite.

Parameters:

  `[in]` | akm_suite | Ful AKM suite

Returns:
  The corresponding enum value and -1 if the suite is unknown

enum mac_cipher_suite mac_cipher_suite_value | ( | uint32_t | cipher_suite | ) |

Convert IEE802.11 Cipher suite into enum mac_cipher_suite.

Parameters:

  `[in]` | cipher_suite | Full Cipher suite

Returns:
  The corresponding enum value and -1 if the suite is unknown

static uint32_t mac_ext_ie_find | ( | uint32_t | addr,
|  | uint16_t | buflen,
|  | uint8_t | ext_ie_id,
|  | uint16_t * | len |
| ) |  |  | `[static]`

Find an extended information element in the variable part of a management frame body.

Parameters:

  `[in]` | addr | Address of the variable part of the management frame body to look for the IE into.
  `[in]` | buflen | Length of the frame body variable part.
  `[in]` | ext_ie_id | Identifier of the extended information element to look for.
  `[out]` | len | Length of the complete element

Returns:
  0 if the IE is not found otherwise the address of the first IE ID location in the frame passed as a parameter.

Definition at line 98 of file mac_ie.c.

References ASSERT_ERR, co_read8p(), MAC_ELTID_EXT, mac_ie_find(), MAC_INFOELT_EXT_ID_OFT, and MAC_INFOELT_EXT_INFO_OFT.

uint32_t mac_ie_country_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the Country element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_country_reg().

uint32_t mac_ie_csa_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the Channel Switch Announcement element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_csa().

uint32_t mac_ie_ds_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the DS element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scan_search_ds(), and scanu_scan_frame_handler().

uint32_t mac_ie_ecsa_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the Extended Channel Switch Announcement element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_csa().

uint32_t mac_ie_erp_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the ERP element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_beacon_check().

uint32_t mac_ie_ext_rates_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the Extended Supported Rates element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_rate_set().

static uint32_t mac_ie_find | ( | uint32_t | addr,
|  | uint16_t | buflen,
|  | uint8_t | ie_id,
|  | uint16_t * | len |
| ) |  |  | `[static]`

Find an information element in the variable part of a management frame body.

Parameters:

  `[in]` | addr | Address of the variable part of the management frame body to look for the IE into.
  `[in]` | buflen | Length of the frame body variable part.
  `[in]` | ie_id | Identifier of the information element to look for.
  `[out]` | len | Length of the complete element

Returns:
  0 if the IE is not found otherwise the address of the first IE ID location in the frame passed as a parameter.

Warning:
  To find a vendor specific information element, see mac_vsie_find. To find an extended information element, see mac_ext_ie_find

Definition at line 52 of file mac_ie.c.

References co_read8p(), mac_ie_len(), and MAC_INFOELT_LEN_OFT.

Referenced by mac_ext_ie_find(), and mac_vsie_find().

uint32_t mac_ie_he_capa_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the HE capability element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_he_oper_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the HE operation element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_ht_capa_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the HT capability element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_ht_capa().

uint32_t mac_ie_ht_oper_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the HT operation element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_beacon_check(), and scanu_join_frame_handler().

__INLINE uint16_t mac_ie_len | ( | uint32_t | addr | ) |

Compute the total length of an information element.

Parameters:

  `[in]` | addr | Address of the information element.

Returns:
  The length of the information element, including the two bytes (ID + Length) header

Definition at line 50 of file mac_ie.h.

References co_read8p(), MAC_INFOELT_INFO_OFT, and MAC_INFOELT_LEN_OFT.

Referenced by mac_ie_find(), scanu_check_ssid(), scanu_get_multi_bssid_info(), and scanu_new_bssid_set().

uint32_t mac_ie_mde_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the MDE element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_mobility_domain().

uint32_t mac_ie_mesh_awake_win_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the Mesh Awake Window element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_mesh_conf_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the Mesh Configuration element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_mesh_id_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the Mesh ID element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_mesh_peer_mgmt_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the Mesh Peering Management element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_mgmt_mic_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the Management MIC element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by mfp_check_mmic_ie().

uint32_t mac_ie_mu_edca_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the MU EDCA element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_multi_bssid_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the Multiple BSSID element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scanu_get_multi_bssid_info().

uint32_t mac_ie_multi_bssid_index_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the nonTransmitted BSSID index element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scanu_get_multi_bssid_info().

uint32_t mac_ie_non_txed_bssid_capa_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the nonTransmitted BSSID capability element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scanu_get_multi_bssid_info().

uint32_t mac_ie_op_mode_notif_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the Operating Mode Notification element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_beacon_check().

uint32_t mac_ie_power_constraint_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the Power Constraint element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_power_constraint().

uint32_t mac_ie_qos_capa_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the QoS Capability element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_rates_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the Supported Rates element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_rate_set().

uint32_t mac_ie_rsn_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the RSN element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scanu_get_security_info().

uint32_t mac_ie_sec_chnl_offset_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | bool * | valid_len |
| ) |  |  |

Search for the Secondary Channel Offset element in a frame buffer.

Note:
  For the IEs associated to Channel Switch Announcement, we return the address of the element even if its length is invalid, and we return an additional valid flag for the length. Indeed a channel switch might be announced using several IEs, and all of them need to be valid to ensure we have the complete information about the new channel.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | valid_len | Indicates whether the length of the element is valid or not

Returns:
  The address of the element if it is present, 0 otherwise

Referenced by me_extract_csa().

uint32_t mac_ie_ssid_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the SSID element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scanu_get_multi_bssid_info(), and scanu_scan_frame_handler().

uint32_t mac_ie_sub_non_txed_bssid_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the nonTransmitted BSSID profile sub-element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scanu_get_multi_bssid_info().

uint32_t mac_ie_tim_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the TIM element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by rxl_frame_handle().

uint32_t mac_ie_uora_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the UORA element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

uint32_t mac_ie_vht_capa_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the VHT capability element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_vht_capa().

uint32_t mac_ie_vht_oper_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the VHT operation element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_beacon_check(), and scanu_join_frame_handler().

uint32_t mac_ie_wapi_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the WAPI element in a frame buffer.

Not part of IEEE 802.11.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scanu_get_security_info().

uint32_t mac_ie_wide_bw_chnl_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | bool * | valid_len |
| ) |  |  |

Search for the Wide Bandwidth Channel sub-element in a frame buffer.

Note:
  For the IEs associated to Channel Switch Announcement, we return the address of the element even if its length is invalid, and we return an additional valid flag for the length. Indeed a channel switch might be announced using several IEs, and all of them need to be valid to ensure we have the complete information about the new channel.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | valid_len | Indicates whether the length of the element is valid or not

Returns:
  The address of the element if it is present, 0 otherwise

Referenced by me_extract_csa().

uint32_t mac_ie_wmm_param_find | ( | uint32_t | buffer,
|  | uint16_t | buflen |
| ) |  |  |

Search for the WMM parameter element in a frame buffer.

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by me_extract_edca_params().

uint32_t mac_ie_wpa_find | ( | uint32_t | buffer,
|  | uint16_t | buflen,
|  | uint8_t * | ie_len |
| ) |  |  |

Search for the WPA element in a frame buffer.

This is the depercated pre-RSN element

Parameters:

  `[in]` | buffer | Address of the frame buffer
  `[in]` | buflen | Buffer length
  `[out]` | ie_len | Length of the information part of the element

Returns:
  The address of the element if it is present and has a valid length, 0 otherwise

Referenced by scanu_get_security_info().

__INLINE bool mac_nontxed_bssid_get | ( | uint8_t | bssid_index,
|  | uint8_t | max_bssid_ind,
|  | struct mac_addr const * | ref_bssid,
|  | struct mac_addr * | bssid |
| ) |  |  |

Get the value of the nonTransmitted BSSID, based on the reference BSSID, the nonTransmitted BSSID index and the Maximum BSSID indicator.

Parameters:

  `[in]` | bssid_index | nonTransmitted BSSID index
  `[in]` | max_bssid_ind | Maximum BSSID indicator
  `[in]` | ref_bssid | Pointer to the reference BSSID
  `[out]` | bssid | nonTransmitted BSSID value

Returns:
  false if the BSSID index or Max BSSID indicator are outside our supported range

Definition at line 384 of file mac.h.

References mac_addr::array, and CO_BIT.

Referenced by scanu_new_bssid_set().

uint32_t mac_paid_gid_ap_compute | ( | struct mac_addr const * | mac_addr,
|  | uint16_t | aid |
| ) |  |  |

Compute the PAID/GID to be put in the THD for frames that need to be sent to a STA connected to an AP or a TDLS peer.

See also:
  802.11ac-2013, table 9-5b for details about the computation.

Parameters:

  `[in]` | mac_addr | Pointer to the BSSID of the AP
  `[in]` | aid | Association ID of the STA

Returns:
  The PAID/GID

Referenced by me_sta_add_req_handler().

uint32_t mac_paid_gid_sta_compute | ( | struct mac_addr const * | mac_addr | ) |

Compute the PAID/GID to be put in the THD for frames that need to be sent to an AP or a Mesh peer.

See also:
  802.11ac-2013, table 9-5b for details about the computation.

Parameters:

  `[in]` | mac_addr | Pointer to the BSSID of the AP or the MAC address of the mesh peer

Returns:
  The PAID/GID

Referenced by me_sta_add_req_handler(), and scanu_join_cfm_handler().

__INLINE void mac_ref_bssid_get | ( | uint8_t | bssid_index,
|  | uint8_t | max_bssid_ind,
|  | struct mac_addr const * | bssid,
|  | struct mac_addr * | ref_bssid |
| ) |  |  |

Get the value of the refernec BSSID, based on the nonTransmitted BSSID, the nonTransmitted BSSID index and the Maximum BSSID indicator.

Parameters:

  `[in]` | bssid_index | nonTransmitted BSSID index
  `[in]` | max_bssid_ind | Maximum BSSID indicator
  `[in]` | bssid | nonTransmitted BSSID value
  `[out]` | ref_bssid | Pointer to the reference BSSID

Definition at line 417 of file mac.h.

References mac_addr::array, and CO_BIT.

Referenced by scanu_join_req_handler().

static uint32_t mac_vsie_find | ( | uint32_t | addr,
|  | uint16_t | buflen,
|  | uint8_t const * | oui,
|  | uint8_t | ouilen,
|  | uint16_t * | len |
| ) |  |  | `[static]`

Find a vendor specific information element in the variable part of a management frame body.

Parameters:

  `[in]` | addr | Address of the variable part of the management frame body to look for the IE into.
  `[in]` | buflen | Length of the frame body variable part.
  `[in]` | oui | Pointer to the OUI identifier to look for.
  `[in]` | ouilen | Length of the OUI identifier.
  `[out]` | len | Length of the complete element

Returns:
  NULL if the VSIE is not found otherwise the pointer to the first VSIE ID location in the frame passed as a parameter.

Definition at line 148 of file mac_ie.c.

References ASSERT_ERR, co_cmp8p(), MAC_ELTID_OUI, mac_ie_find(), and MAC_INFOELT_INFO_OFT.

## Variable Documentation

struct he_trigger_base __PACKED

Structure of a short control frame MAC header.

Base structure of a HE Trigger frame.

Base part of the User Info field present in the HE trigger frames.

Structure of the User Info part of the HE Basic Trigger frame.

Structure of A-MSDU Header.

Structure of a Compressed Block Acknowledgment frame.

Multi-STA AID/TID info field.

Structure of BA SSC + 256-bit bitmap.

Structure of BA SSC + 128-bit bitmap.

Structure of BA SSC + 64-bit bitmap.

Structure of BA SSC + 32-bit bitmap.

Structure of generic BA SSC + bitmap.

Base structure of a Block Acknowledgment frame.

Structure of a Block Acknowledgment Request frame.

Structure of a Probe Request frame.

Structure of a Beacon or ProbeRsp frame.

Structure of Ethernet Header.

Structure of a 4-address QoS Data frame MAC header.

Structure of a 4-address Data frame MAC header.

Structure of a QoS Data + HTC frame MAC header.

Structure of a QoS Data frame MAC header.

Structure of a Data/Management frame MAC header.

Structure of a long control frame MAC header.

const uint8_t mac_ac2aci[AC_MAX]

Initial value:

    {
        [AC_BK] = 1,
        [AC_BE] = 0,
        [AC_VI] = 2,
        [AC_VO] = 3,
    }

Array converting an AC to its corresponding ACI. See Table 9-136 in 802.11-2016.

Definition at line 61 of file mac.c.

const uint8_t mac_ac2uapsd[AC_MAX]

Initial value:

    {
        [AC_BK] = MAC_QOS_INFO_STA_UAPSD_ENABLED_BK,
        [AC_BE] = MAC_QOS_INFO_STA_UAPSD_ENABLED_BE,
        [AC_VI] = MAC_QOS_INFO_STA_UAPSD_ENABLED_VI,
        [AC_VO] = MAC_QOS_INFO_STA_UAPSD_ENABLED_VO,
    }

Array converting an AC to its corresponding bit in the QoS Information field.

Definition at line 45 of file mac.c.

Referenced by rxl_pm_check().

const uint8_t mac_aci2ac[AC_MAX]

Initial value:

    {
        [0] = AC_BE,
        [1] = AC_BK,
        [2] = AC_VI,
        [3] = AC_VO,
    }

Array converting an ACI to its corresponding AC. See Table 9-136 in 802.11-2016.

Definition at line 53 of file mac.c.

const uint8_t mac_id2rate[MAC_RATESET_LEN]

Initial value:

    {
        MAC_RATE_1MBPS,
        MAC_RATE_2MBPS,
        MAC_RATE_5_5MBPS,
        MAC_RATE_11MBPS,
        MAC_RATE_6MBPS,
        MAC_RATE_9MBPS,
        MAC_RATE_12MBPS,
        MAC_RATE_18MBPS,
        MAC_RATE_24MBPS,
        MAC_RATE_36MBPS,
        MAC_RATE_48MBPS,
        MAC_RATE_54MBPS
    }

Array converting a MAC HW rate id into its corresponding standard rate value.

Definition at line 69 of file mac.c.

Referenced by scanu_build_ie().

const uint8_t mac_tid2ac[TID_MAX]

Initial value:

    {
        AC_BE,
        AC_BK,
        AC_BK,
        AC_BE,
        AC_VI,
        AC_VI,
        AC_VO,
        AC_VO,
        AC_VO
    }

Array converting a TID to its associated AC.

Definition at line 32 of file mac.c.

Referenced by bam_create_ba_agg(), mm_ba_add_req_handler(), rxl_pm_check(), txl_frame_send_tdls_channel_switch_req_frame(), and txl_frame_send_tdls_channel_switch_rsp_frame().