# mm_bcn_env_tag Struct Reference
[MM_BCN]

MM BCN environmenent structure. More...

`#include <mm_bcn.h>`

Collaboration diagram for mm_bcn_env_tag:
[legend]

## Data Fields
struct mm_bcn_change_req const * | param
| Pointer to the beacon parameter structure.
int | tx_cfm
| Number of beacon transmission confirmation still awaited.
bool | tx_pending
| Flag indicating if beacon transmission has to be programmed immediately after download.
bool | update_ongoing
| Flag indicating if beacon update is ongoing.
bool | update_pending
| Flag indicating if the beacon has to be updated immediately after the transmission.
struct hal_dma_desc_tag | dma
| Structure used for beacon download by the DMA.
struct co_list | tim_list
| List containing the TIM update requests.
uint8_t | p2p_noa_req [NX_VIRT_DEV_MAX]
| P2P NOA Change Request.

## Detailed Description

MM BCN environmenent structure.

Definition at line 53 of file mm_bcn.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_bcn.h