<map id="G" name="G">
<area shape="rect" id="node19" href="$structtxl__buffer__tag.html" title="Buffer header structure." alt="" coords="1125,1667,1259,1925"/>
<area shape="rect" id="node28" href="$structtx__agg__desc.html" title="Aggregation descriptor, containing AMPDU THD, BAR descriptor, BAR payload and Policy..." alt="" coords="508,1597,649,1995"/>
<area shape="rect" id="node2" href="$structhostdesc.html" title="Descriptor filled by the Host." alt="" coords="827,517,981,845"/>
<area shape="rect" id="node4" href="$structmac__addr.html" title="MAC address structure." alt="" coords="745,305,831,391"/>
<area shape="rect" id="node43" href="$structmac__hdr__ctrl.html" title="Structure of a long control frame MAC header." alt="" coords="693,613,803,750"/>
<area shape="rect" id="node6" href="$structumacdesc.html" title="Descriptor filled by the UMAC." alt="" coords="1005,526,1139,837"/>
<area shape="rect" id="node8" href="$structtxl__buffer__control.html" title="Control descriptor containing information about the transmission rates to use, the..." alt="" coords="997,262,1147,434"/>
<area shape="rect" id="node10" href="$structtx__policy__tbl.html" title="Policy Table Structure used to store Policy Table Information used by MAC HW to prepare..." alt="" coords="611,5,741,195"/>
<area shape="rect" id="node12" href="$structtx__compressed__policy__tbl.html" title="Compressed Policy Table Structure used to store Policy Table Information used by..." alt="" coords="975,49,1169,151"/>
<area shape="rect" id="node14" href="$structco__list__hdr.html" title="structure of a list element header" alt="" coords="156,639,249,724"/>
<area shape="rect" id="node30" href="$structco__list.html" title="structure of a list" alt="" coords="123,1093,187,1195"/>
<area shape="rect" id="node54" href="$structbfr__mem__node.html" title="Structure representing a piece of BFR memory." alt="" coords="5,1384,128,1573"/>
<area shape="rect" id="node17" href="$structlmacdesc.html" title="Descriptor filled by the LMAC." alt="" coords="1019,2062,1117,2199"/>
<area shape="rect" id="node22" href="$structdma__desc.html" title="Element in the pool of TX DMA bridge descriptors." alt="" coords="1503,1067,1593,1221"/>
<area shape="rect" id="node48" href="$structtx__hw__desc.html" title="Definition of a TX confirmation descriptor." alt="" coords="1340,1736,1444,1856"/>
<area shape="rect" id="node24" href="$structtx__pbd.html" title="Definition of a TX payload buffer descriptor." alt="" coords="1135,1067,1255,1221"/>
<area shape="rect" id="node34" href="$structtx__hd.html" title="Definition of a TX header descriptor." alt="" coords="841,928,1004,1360"/>
<area shape="rect" id="node36" href="$structba__ssc__bitmap.html" title="Structure of generic BA SSC + bitmap." alt="" coords="308,1093,428,1195"/>
<area shape="rect" id="node41" href="$structbar__frame.html" title="Structure of a Block Acknowledgment Request frame." alt="" coords="679,1084,817,1204"/>
<area shape="rect" id="node46" href="$structba__ssc__bitmap__256.html" title="Structure of BA SSC + 256&#45;bit bitmap." alt="" coords="503,1093,655,1195"/>
<area shape="rect" id="node52" href="$structtx__cfm__tag.html" title="Structure indicating the status and other information about the transmission." alt="" coords="1333,1049,1448,1239"/>
</map>
