# ba_agmt Struct Reference
[STA_MGMT]

BA agreement structure - one for every possible TID, valid if params non 0. More...

`#include <sta_mgmt.h>`

## Data Fields
uint16_t | ssn
| Starting sequence number - the one allowed as lowest in an A-MPDU - will change as MPDUs get Acked.
uint8_t | bufsz
| Buffer size - max number of MPDUs that can be held in recipient's buffer.

## Detailed Description

BA agreement structure - one for every possible TID, valid if params non 0.

Definition at line 289 of file sta_mgmt.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/sta/sta_mgmt.h