<map id="G" name="G">
<area shape="rect" id="node2" href="$structtxdesc.html" title="LMAC Tx Descriptor." alt="" coords="923,1075,1005,1213"/>
<area shape="rect" id="node21" href="$structtxl__buffer__tag.html" title="Buffer header structure." alt="" coords="1217,1667,1351,1925"/>
<area shape="rect" id="node30" href="$structtx__agg__desc.html" title="Aggregation descriptor, containing AMPDU THD, BAR descriptor, BAR payload and Policy..." alt="" coords="597,1597,739,1995"/>
<area shape="rect" id="node4" href="$structhostdesc.html" title="Descriptor filled by the Host." alt="" coords="873,517,1028,845"/>
<area shape="rect" id="node6" href="$structmac__addr.html" title="MAC address structure." alt="" coords="792,305,877,391"/>
<area shape="rect" id="node45" href="$structmac__hdr__ctrl.html" title="Structure of a long control frame MAC header." alt="" coords="740,613,849,750"/>
<area shape="rect" id="node8" href="$structumacdesc.html" title="Descriptor filled by the UMAC." alt="" coords="1052,526,1185,837"/>
<area shape="rect" id="node10" href="$structtxl__buffer__control.html" title="Control descriptor containing information about the transmission rates to use, the..." alt="" coords="1044,262,1193,434"/>
<area shape="rect" id="node12" href="$structtx__policy__tbl.html" title="Policy Table Structure used to store Policy Table Information used by MAC HW to prepare..." alt="" coords="475,5,605,195"/>
<area shape="rect" id="node14" href="$structtx__compressed__policy__tbl.html" title="Compressed Policy Table Structure used to store Policy Table Information used by..." alt="" coords="1021,49,1216,151"/>
<area shape="rect" id="node16" href="$structco__list__hdr.html" title="structure of a list element header" alt="" coords="405,639,499,724"/>
<area shape="rect" id="node32" href="$structco__list.html" title="structure of a list" alt="" coords="236,1093,300,1195"/>
<area shape="rect" id="node56" href="$structbfr__mem__node.html" title="Structure representing a piece of BFR memory." alt="" coords="5,1384,128,1573"/>
<area shape="rect" id="node19" href="$structlmacdesc.html" title="Descriptor filled by the LMAC." alt="" coords="932,2062,1031,2199"/>
<area shape="rect" id="node24" href="$structdma__desc.html" title="Element in the pool of TX DMA bridge descriptors." alt="" coords="1447,1067,1537,1221"/>
<area shape="rect" id="node50" href="$structtx__hw__desc.html" title="Definition of a TX confirmation descriptor." alt="" coords="1476,1736,1580,1856"/>
<area shape="rect" id="node26" href="$structtx__pbd.html" title="Definition of a TX payload buffer descriptor." alt="" coords="1561,1067,1681,1221"/>
<area shape="rect" id="node36" href="$structtx__hd.html" title="Definition of a TX header descriptor." alt="" coords="1260,928,1423,1360"/>
<area shape="rect" id="node38" href="$structba__ssc__bitmap.html" title="Structure of generic BA SSC + bitmap." alt="" coords="324,1093,444,1195"/>
<area shape="rect" id="node43" href="$structbar__frame.html" title="Structure of a Block Acknowledgment Request frame." alt="" coords="741,1084,880,1204"/>
<area shape="rect" id="node48" href="$structba__ssc__bitmap__256.html" title="Structure of BA SSC + 256&#45;bit bitmap." alt="" coords="468,1093,620,1195"/>
<area shape="rect" id="node54" href="$structtx__cfm__tag.html" title="Structure indicating the status and other information about the transmission." alt="" coords="1705,1049,1820,1239"/>
<area shape="rect" id="node59" href="$structtxl__frame__cfm__tag.html" title="TX frame confirmation descriptor." alt="" coords="1029,1093,1179,1195"/>
</map>
