# mm_set_vif_state_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_SET_VIF_STATE_REQ message. More...

`#include <mm_task.h>`

## Data Fields
uint16_t | aid
| Association Id received from the AP (valid only if the VIF is of STA type).
bool | active
| Flag indicating if the VIF is active or not.
uint8_t | inst_nbr
| Interface index.

## Detailed Description

Structure containing the parameters of the MM_SET_VIF_STATE_REQ message.

Definition at line 467 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h