# me_bss_info Struct Reference
[ME]

Information related to the BSS a VIF is linked to. More...

`#include <me.h>`

Collaboration diagram for me_bss_info:
[legend]

## Data Fields
struct mac_htcapability | ht_cap
| HT capabilities of the BSS.
struct mac_addr | bssid
| Network BSSID.
struct mac_ssid | ssid
| Network name.
uint8_t | bssid_index
| nonTransmitted BSSID index, in case the STA is connected to a nonTransmitted BSSID of a Multiple BSSID set.
uint8_t | max_bssid_ind
| Maximum BSSID indicator, in case the STA is connected to a nonTransmitted BSSID of a Multiple BSSID set.
uint16_t | bsstype
| Network type (IBSS or ESS).
struct mac_chan_op | chan
| Operating channel.
uint16_t | beacon_period
| Network beacon period.
struct mac_rateset | rate_set
| Legacy rate set.
struct mac_edca_param_set | edca_param
| EDCA parameter set.
int8_t | rssi
| RSSI of the beacons received from this BSS.
uint8_t | high_11b_rate
| Highest 11g rate that can be used.
uint16_t | prot_status
| Protection Status (Bit field).
uint8_t | power_constraint
| Power Constraint.
uint32_t | capa_flags
| Flags indicating which BSS capabilities are valid (HT/VHT/QoS/HE/etc.).
struct mobility_domain | mde
| Mobility Domain element.

## Detailed Description

Information related to the BSS a VIF is linked to.

Definition at line 134 of file me.h.

## Field Documentation

uint8_t me_bss_info::bssid_index

nonTransmitted BSSID index, in case the STA is connected to a nonTransmitted BSSID of a Multiple BSSID set.

Should be set to 0 otherwise

Definition at line 154 of file me.h.

Referenced by scanu_join_cfm_handler().

uint8_t me_bss_info::max_bssid_ind

Maximum BSSID indicator, in case the STA is connected to a nonTransmitted BSSID of a Multiple BSSID set.

Definition at line 157 of file me.h.

Referenced by scanu_join_cfm_handler().

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/me/me.h