# scanu_start_req Struct Reference
[TASK_SCANU]

Structure containing the parameters of the SCANU_START_REQ message. More...

`#include <scanu_task.h>`

Collaboration diagram for scanu_start_req:
[legend]

## Data Fields
struct mac_chan_def | chan [SCAN_CHANNEL_MAX]
| List of channel to be scanned.
struct mac_ssid | ssid [SCAN_SSID_MAX]
| List of SSIDs to be scanned.
struct mac_addr | bssid
| BSSID to be scanned (or WILDCARD BSSID if no BSSID is searched in particular).
uint32_t | add_ies
| Address (in host memory) of the additional IEs that need to be added to the ProbeReq (following the SSID element).
uint16_t | add_ie_len
| Length of the additional IEs.
uint8_t | vif_idx
| Index of the VIF that is scanning.
uint8_t | chan_cnt
| Number of channels to scan.
uint8_t | ssid_cnt
| Number of SSIDs to scan for.
bool | no_cck
| no CCK - For P2P frames not being sent at CCK rate in 2GHz band.

## Detailed Description

Structure containing the parameters of the SCANU_START_REQ message.

Definition at line 63 of file scanu_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/scanu/scanu_task.h