Start,
scramblerSeed,                	[ 1 0 0 1 1 0 1 ]
NTx,                          	[ 2 ] 
NRx,                          	[ 2 ] 
FrameFormat,                  	[ 'AC' ] 
PreambleType11b,              	[ 0 ] 
LegacyRate,                   	[ 11 ] 
MCS,                          	[ 0 ] 
ChanType,                     	[ 0 ] 
FrameBW,                      	[ 40 ] 
RxChannelBW,                  	[ 80 ] 
TxChannelBW,                  	[ 80 ] 
RxControlChannel,             	[ -1 ] 
TxControlChannel,             	[ -1 ] 
htLength,                     	[ 5500 ] 
CarrierFreq_GHz,              	[ 6 ] 
Smoothing,                    	[ 1 ] 
NESS,                         	[ 0 ] 
ShortGI,                      	[ 1 ] 
STBC,                         	[ 0 ] 
NSTS,                         	[ 1 ] 
NOTSOUNDING,                  	[ 1 ] 
LDPC,                         	[ 1 ] 
RxRFName,                     	[ 'KARST' ] 
AGC,                          	[ 'FXPT' ] 
StateDescription,             	[ 'FPGA_KARST' ] 
RxPAntdBm,                    	[ -40 ] 
DirName,                      	[ 'DUMP' ] 
TBEBias,                      	[ 5 ] 
Tx4044FilterShift,            	[ 0 ] 
TxFENegShiftDel,              	[ 7 ] 
Tx4044FilterInDel,            	[ 9 ] 
Tx4044FilterOutDel,           	[ 1 ] 
TxDigGainLin,                 	[ 32 ] 
EVM,                          	[ 1 ] 
debugEn,                      	[ 1 ] 
TxDump,                       	[ 1 ] 
RxDump,                       	[ 1 ] 
AGCDumpEn,                    	[ 1 ] 
TXFRONTENDDumpEn,             	[ 0 ] 
HTSTFAGCEn,                   	[ 1 ] 
Aggregation,                  	[ 1 ] 
DozeNotAllow,                 	[ 0 ] 
TxIQPhase_deg,                	[ 0 ] 
TxIQGain_dB,                  	[ 0 ] 
RxIQPhase_deg,                	[ 0 ] 
RxIQGain_dB,                  	[ 0 ] 
RxDC_mv,                      	[ 0 ] 
TxDC_mv,                      	[ 0 ] 
CarrierLostStartUs,           	[ 0 ] 
CarrierLostStopUs,            	[ 0 ] 
packetStartUs,                	[ 16 ] 
ACIRxPAntdBm,                 	[ 0 ] 
ACIStartUs,                   	[ 0 ] 
ACIStopUs,                    	[ 0 ] 
ACIFcMHz,                     	[ 0 ] 
ACIOperatingMode,             	[ 'NON' ] 
RampUpFreqkHz,                	[ 0 ] 
RampUpLength_us,              	[ 0 ] 
RampUpType,                   	[ 1 ] 
RampUpRatio,                  	[ 0.5 ] 
RampUpPowDeltadB,             	[ -15 ] 
LSIGParityErrForce,           	[ 0 ] 
HTSIGCRCErrForce,             	[ 0 ] 
smmIdx,                       	[ 0 ] 
FixRandomSeed,                	[ 1 ] 
RNGSeed,                      	[ 1 ] 
AGCPrint,                     	[ 0 ] 
ClockOffset_ppm,              	[ 0 ] 
FrequencyOffset_ppm,          	[ 0 ] 
PartialAID,                   	[ 0 1 0 0 1 1 0 1 1 ]
GroupID,                      	[ 1 1 1 1 1 1 ]
BFDump,                       	[ 0 ] 
BFEn,                         	[ 0 ] 
AGCDelay_us,                  	[ 4 ] 
SMFFilterSet,                 	[ 0 ] 
FrameBWDet,                   	[ 'FXPT' ] 
RxSmoothing,                  	[ 'FXPT' ] 
TDDCCompInit,                 	[ 'FXPT' ] 
TDDCTracking,                 	[ 'FXPT' ] 
TDCyclicRotateValUs20MHz,     	[ 0.3 ] 
TDCyclicRotateValUs40MHz,     	[ 0.3 ] 
ShiftSBEn,                    	[ 1 ] 
dcTrigOff,                    	[ 0 ] 
dcTrigOff,                       [ 0 ]
dcRelockHTTrigOff,             [ -1 ]
foHTTrigOff2020,               [ 3 ]
foHTTrigOff2040,               [ 1 ]
foHTTrigOff4020,               [ 3 ]
foHTTrigOff4040,               [ 5 ]
dcHTTrigOff20,                 [ 60 ]
dcVHTTrigOff20,                [ 235 ]
dcHTTrigOff40,                 [ 53 ]
dcVHTTrigOff40,                [ 190 ]
foHTTrigOff2080,               [ 1 ]
foHTTrigOff4080,               [ 10 ]
RxPhaseNoiseFc_kHz,           	[ 0 ] 
RxPhaseNoisePow_degrms,       	[ 0 ] 
TxPhaseNoiseFc_kHz,           	[ 0 ] 
TxPhaseNoisePow_degrms,       	[ 0 ] 
End,
