# apm_start_req Struct Reference
[TASK_APM]

Structure containing the parameters of the APM_START_REQ message. More...

`#include <apm_task.h>`

Collaboration diagram for apm_start_req:
[legend]

## Data Fields
struct mac_rateset | basic_rates
| Basic rate set.
struct mac_chan_op | chan
| Operating channel on which we have to enable the AP.
uint32_t | bcn_addr
| Address, in host memory, to the beacon template.
uint16_t | bcn_len
| Length of the beacon template.
uint16_t | tim_oft
| Offset of the TIM IE in the beacon.
uint16_t | bcn_int
| Beacon interval.
uint32_t | flags
| Flags (mac_connection_flags).
uint16_t | ctrl_port_ethertype
| Control port Ethertype.
uint8_t | tim_len
| Length of the TIM IE.
uint8_t | vif_idx
| Index of the VIF for which the AP is started.

## Detailed Description

Structure containing the parameters of the APM_START_REQ message.

Definition at line 76 of file apm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/apm/apm_task.h