# p2p_noa_info_tag Struct Reference
[P2P]

Structure containing all information linked with NoA. More...

`#include <p2p.h>`

Collaboration diagram for p2p_noa_info_tag:
[legend]

## Data Fields
struct mm_timer_tag | noa_timer
| Timer used for P2P Notice of Absence management.
uint8_t | noa_status
| Status of the NOA timer.
uint8_t | p2p_index
| Index of the linked P2P information structure.
uint8_t | noa_inst
| NOA Instance.
uint8_t | noa_counter
| NOA Counter Indicate the remaining number of absence (current one included) - 255 for continuous.
uint8_t | noa_init_counter
| Initial NOA Counter value.
uint32_t | noa_dur_us
| NOA - Absence Duration (in us).
uint32_t | noa_intv_us
| NOA - Absence Interval (in us).
uint8_t | noa_type
| Type of NoA (due to Concurrent Mode or required by Host for GO) - relevant for GO only.
bool | dyn_noa
| Indicate if NoA can be paused for traffic reasons.
uint32_t | noa_start_time
| NOA - Start Time - GO only.
uint32_t | noa_time_upd_cnt
| Counter used to know when we can update the start time inside the beacon - GO only.
uint32_t | peer_next_noa_time
| Next NOA time (absence or end of absence) in peer TSF (valid only for CLI connection).

## Detailed Description

Structure containing all information linked with NoA.

Definition at line 228 of file p2p.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/p2p/p2p.h