# RD
[LMAC]

Management of the radar pulses received from PHY. More...

Collaboration diagram for RD:

## Data Structures
struct | rd_env_tag
| RX control environment declaration. More...
## Functions
void | rd_init (void)
| This function initializes the radar pulse manager.
void | rd_event_ind (int rd_idx)
| Indicate to the RD module that a radar event has been detected by the PHY.
## Variables
struct rd_env_tag | rd_env
| Radar environment variable.

## Detailed Description

Management of the radar pulses received from PHY.

## Function Documentation

void rd_event_ind | ( | int | rd_idx | ) |

Indicate to the RD module that a radar event has been detected by the PHY.

Parameters:

  `[in]` | rd_idx | Index of the radar detection chain on which pulses have been detected

Referenced by phy_rc_isr().

void rd_init | ( | void |  | ) |

This function initializes the radar pulse manager.