# /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/sm/sm_task.c File Reference

The UMAC's STA Manager (SM) module implementation. More...

`#include "sm_task.h"`
`#include "co_endian.h"`
`#include "scanu_task.h"`
`#include "scanu.h"`
`#include "sm.h"`
`#include "me_utils.h"`
`#include "mac_frame.h"`
`#include "ke_timer.h"`
`#include "mac.h"`
`#include "mm_task.h"`
`#include "me.h"`
`#include "me_mgmtframe.h"`
`#include "mm.h"`
`#include "vif_mgmt.h"`
`#include "sta_mgmt.h"`
`#include "rxu_task.h"`
`#include "ps.h"`

Go to the source code of this file.

## Functions
static int | sm_connect_req_handler (ke_msg_id_t const msgid, struct sm_connect_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| SM_CONNECT_REQ message handler.
static int | sm_disconnect_req_handler (ke_msg_id_t const msgid, struct sm_disconnect_req const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| SM_DISCONNECT_REQ message handler.
static int | mm_connection_loss_ind_handler (ke_msg_id_t const msgid, struct mm_connection_loss_ind const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| MM_CONNECTION_LOSS_IND message handler.
static int | sm_rsp_timeout_ind_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| SM_RSP_TIMEOUT_IND message handler.
static int | scanu_start_cfm_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| SCANU_START_CFM message handler.
static int | scanu_join_cfm_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| SCANU_JOIN_CFM message handler.
static int | mm_sta_add_cfm_handler (ke_msg_id_t const msgid, struct mm_sta_add_cfm const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| MM_STA_ADD_CFM message handler.
static int | me_set_ps_disable_cfm_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME_SET_PS_DISABLE_CFM message handler.
static int | mm_bss_param_setting_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| BSS parameter setting message handler.
static int | me_set_active_cfm_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| ME_SET_ACTIVE_CFM message handler.
static int | mm_set_vif_state_cfm_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| MM_SET_VIF_STATE_CFM message handler.
static int | mm_sta_del_cfm_handler (ke_msg_id_t const msgid, struct mm_sta_del_cfm const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| MM_STA_DEL_CFM message handler.
static int | mm_chan_ctxt_unlink_cfm_handler (ke_msg_id_t const msgid, void const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| MM_CHAN_CTXT_UNLINK_CFM message handler.
static int | rxu_mgt_ind_handler (ke_msg_id_t const msgid, struct rxu_mgt_ind const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| RXU_MGT_IND message handler.
static int | sm_external_auth_required_rsp_handler (ke_msg_id_t const msgid, struct sm_external_auth_required_rsp const *param, ke_task_id_t const dest_id, ke_task_id_t const src_id)
| SM_EXTERNAL_AUTH_REQUIRED_RSP message handler.
## Variables
struct ke_msg_handler | sm_default_state []
| DEFAULT handler definition.
struct ke_state_handler | sm_default_handler
| Specifies the message handlers that are common to all states.
ke_state_t | sm_state [SM_IDX_MAX]
| Defines the placeholder for the states of all the task instances.

## Detailed Description

The UMAC's STA Manager (SM) module implementation.

Copyright (C) RivieraWaves 2011-2019

Definition in file sm_task.c.