# rxu_cntrl_env_tag Struct Reference
[RXU]

The context structure of the UMAC's Rx module. More...

`#include <rxu_cntrl.h>`

Collaboration diagram for rxu_cntrl_env_tag:
[legend]

## Data Fields
struct rx_cntrl_rx_status | rx_status
| Information related to the currently received packet.
struct co_list | rxdesc_ready
| List of RX Descriptor elements that are ready for DMA transfer.
uint32_t | hostid_current
| HostId of the buffer currently involved in the packet reception.
uint8_t | rxdesc_idx
| Index of the next rxu_stat_desc structure to use.
struct co_list | rxu_reord_free
| List of free RX Reordering structures.
struct co_list | rxu_defrag_free
| List of free Reassembly structures.
struct co_list | rxu_defrag_used
| List of used Reassembly structures.
struct rx_cntrl_dupli | rxu_dupli
| Unknown STA duplicate filtering information.
struct mac_addr * | mac_addr_ptr
| Pointer to this stations MAC Address.
struct rx_cntrl_pm_mon | pm_mon
| PM bit monitoring.
uint32_t | ttr
| Time to run parameter used.

## Detailed Description

The context structure of the UMAC's Rx module.

Definition at line 312 of file rxu_cntrl.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/rxu/rxu_cntrl.h