# mm_set_channel_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_SET_CHANNEL_REQ message. More...

`#include <mm_task.h>`

Collaboration diagram for mm_set_channel_req:
[legend]

## Data Fields
struct mac_chan_op | chan
| Channel information.
uint8_t | index
| Index of the RF for which the channel has to be set (0: operating (primary), 1: secondary RF (used for additional radar detection).

## Detailed Description

Structure containing the parameters of the MM_SET_CHANNEL_REQ message.

Definition at line 316 of file mm_task.h.

## Field Documentation

uint8_t mm_set_channel_req::index

Index of the RF for which the channel has to be set (0: operating (primary), 1: secondary RF (used for additional radar detection).

This parameter is reserved if no secondary RF is available in the system

Definition at line 323 of file mm_task.h.

Referenced by mm_set_channel_req_handler().

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h