# sm_connect_ind Struct Reference
[TASK_SM]

Structure containing the parameters of the SM_CONNECT_IND message. More...

`#include <sm_task.h>`

Collaboration diagram for sm_connect_ind:
[legend]

## Data Fields
uint16_t | status_code
| Status code of the connection procedure.
struct mac_addr | bssid
| BSSID.
bool | roamed
| Flag indicating if the indication refers to an internal roaming or from a host request.
uint8_t | vif_idx
| Index of the VIF for which the association process is complete.
uint8_t | ap_idx
| Index of the STA entry allocated for the AP.
uint8_t | ch_idx
| Index of the LMAC channel context the connection is attached to.
bool | qos
| Flag indicating if the AP is supporting QoS.
uint8_t | acm
| ACM bits set in the AP WMM parameter element.
uint16_t | assoc_req_ie_len
| Length of the AssocReq IEs.
uint16_t | assoc_rsp_ie_len
| Length of the AssocRsp IEs.
uint32_t | assoc_ie_buf [SM_ASSOC_IE_LEN/4]
| IE buffer.
uint16_t | aid
| Association Id allocated by the AP for this connection.
struct mac_chan_op | chan
| AP operating channel.
uint32_t | ac_param [AC_MAX]
| EDCA parameters.

## Detailed Description

Structure containing the parameters of the SM_CONNECT_IND message.

Definition at line 127 of file sm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/sm/sm_task.h