<map id="G" name="G">
<area shape="rect" id="node2" href="$structtxdesc.html" title="LMAC Tx Descriptor." alt="" coords="112,1075,195,1213"/>
<area shape="rect" id="node21" href="$structtxl__buffer__tag.html" title="Buffer header structure." alt="" coords="941,1667,1075,1925"/>
<area shape="rect" id="node30" href="$structtx__agg__desc.html" title="Aggregation descriptor, containing AMPDU THD, BAR descriptor, BAR payload and Policy..." alt="" coords="537,1597,679,1995"/>
<area shape="rect" id="node4" href="$structhostdesc.html" title="Descriptor filled by the Host." alt="" coords="5,517,160,845"/>
<area shape="rect" id="node6" href="$structmac__addr.html" title="MAC address structure." alt="" coords="175,305,260,391"/>
<area shape="rect" id="node45" href="$structmac__hdr__ctrl.html" title="Structure of a long control frame MAC header." alt="" coords="341,613,451,750"/>
<area shape="rect" id="node8" href="$structumacdesc.html" title="Descriptor filled by the UMAC." alt="" coords="184,526,317,837"/>
<area shape="rect" id="node10" href="$structtxl__buffer__control.html" title="Control descriptor containing information about the transmission rates to use, the..." alt="" coords="857,262,1007,434"/>
<area shape="rect" id="node12" href="$structtx__policy__tbl.html" title="Policy Table Structure used to store Policy Table Information used by MAC HW to prepare..." alt="" coords="1043,5,1173,195"/>
<area shape="rect" id="node14" href="$structtx__compressed__policy__tbl.html" title="Compressed Policy Table Structure used to store Policy Table Information used by..." alt="" coords="816,49,1011,151"/>
<area shape="rect" id="node16" href="$structco__list__hdr.html" title="structure of a list element header" alt="" coords="561,639,655,724"/>
<area shape="rect" id="node32" href="$structco__list.html" title="structure of a list" alt="" coords="655,1093,719,1195"/>
<area shape="rect" id="node56" href="$structbfr__mem__node.html" title="Structure representing a piece of BFR memory." alt="" coords="1524,1384,1647,1573"/>
<area shape="rect" id="node19" href="$structlmacdesc.html" title="Descriptor filled by the LMAC." alt="" coords="959,2114,1057,2251"/>
<area shape="rect" id="node24" href="$structdma__desc.html" title="Element in the pool of TX DMA bridge descriptors." alt="" coords="1319,1067,1409,1221"/>
<area shape="rect" id="node50" href="$structtx__hw__desc.html" title="Definition of a TX confirmation descriptor." alt="" coords="1215,1736,1319,1856"/>
<area shape="rect" id="node26" href="$structtx__pbd.html" title="Definition of a TX payload buffer descriptor." alt="" coords="988,1067,1108,1221"/>
<area shape="rect" id="node36" href="$structtx__hd.html" title="Definition of a TX header descriptor." alt="" coords="1132,928,1295,1360"/>
<area shape="rect" id="node38" href="$structba__ssc__bitmap.html" title="Structure of generic BA SSC + bitmap." alt="" coords="743,1093,863,1195"/>
<area shape="rect" id="node43" href="$structbar__frame.html" title="Structure of a Block Acknowledgment Request frame." alt="" coords="219,1084,357,1204"/>
<area shape="rect" id="node48" href="$structba__ssc__bitmap__256.html" title="Structure of BA SSC + 256&#45;bit bitmap." alt="" coords="381,1093,533,1195"/>
<area shape="rect" id="node54" href="$structtx__cfm__tag.html" title="Structure indicating the status and other information about the transmission." alt="" coords="1433,1049,1548,1239"/>
</map>
