# mm_sta_add_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_STA_ADD_REQ message. More...

`#include <mm_task.h>`

Collaboration diagram for mm_sta_add_req:
[legend]

## Data Fields
uint32_t | ampdu_size_max_he
| Maximum A-MPDU size, in bytes, for HE frames.
uint32_t | ampdu_size_max_vht
| Maximum A-MPDU size, in bytes, for VHT frames.
uint32_t | paid_gid
| PAID/GID.
uint16_t | ampdu_size_max_ht
| Maximum A-MPDU size, in bytes, for HT frames.
struct mac_addr | mac_addr
| MAC address of the station to be added.
uint8_t | ampdu_spacing_min
| A-MPDU spacing, in us.
uint8_t | inst_nbr
| Interface index.
bool | tdls_sta
| TDLS station.
bool | tdls_initiator
| TDLS link initiator.
bool | tdls_chsw_allowed
| Flag to indicate if TDLS Channel Switch is allowed.
uint8_t | bssid_index
| nonTransmitted BSSID index, set to the BSSID index in case the STA added is an AP that is a nonTransmitted BSSID.
uint8_t | max_bssid_ind
| Maximum BSSID indicator, valid if the STA added is an AP that is a nonTransmitted BSSID.

## Detailed Description

Structure containing the parameters of the MM_STA_ADD_REQ message.

Definition at line 515 of file mm_task.h.

## Field Documentation

uint8_t mm_sta_add_req::bssid_index

nonTransmitted BSSID index, set to the BSSID index in case the STA added is an AP that is a nonTransmitted BSSID.

Should be set to 0 otherwise

Definition at line 539 of file mm_task.h.

Referenced by me_sta_add_req_handler(), and scanu_join_cfm_handler().

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h