# bam_baw Struct Reference
[BAM]

Per RA/TID Data for AMPDU TX. More...

`#include <bam.h>`

## Data Fields
bam_baw_index_func_ptr | idx_compute
| Pointer to the function computing the BaW index.
uint16_t | fsn
| Starting Seq Num of BlockAck window.
uint8_t | states [BAM_MAX_TX_WIN_SIZE]
| State of each element of the BA window BAW_{FREE,PENDING,CONFIRMED}.
uint8_t | fsn_idx
| Index in the state table corresponding to the fsn value.
uint8_t | buf_size
| Size of the receiver reordering window.
uint8_t | mask
| BaW wrapping mask.

## Detailed Description

Per RA/TID Data for AMPDU TX.

Definition at line 287 of file bam.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/bam/bam.h