# apm_start_cfm Struct Reference
[TASK_APM]

Structure containing the parameters of the APM_START_CFM message. More...

`#include <apm_task.h>`

## Data Fields
uint8_t | status
| Status of the AP starting procedure.
uint8_t | vif_idx
| Index of the VIF for which the AP is started.
uint8_t | ch_idx
| Index of the channel context attached to the VIF.
uint8_t | bcmc_idx
| Index of the STA used for BC/MC traffic.

## Detailed Description

Structure containing the parameters of the APM_START_CFM message.

Definition at line 101 of file apm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/apm/apm_task.h