# txl_agg_build_tag Struct Reference
[TX_CNTRL]

Structure containing the information about the current A-MPDU being built. More...

`#include <txl_cntrl.h>`

Collaboration diagram for txl_agg_build_tag:
[legend]

## Data Fields
struct tx_agg_desc * | desc
| Pointer to the allocated aggregation descriptor.
struct txdesc * | txdesc_first
| Pointer to the first TX descriptor of the A-MPDU.
struct txdesc * | txdesc_last
| Pointer to the last TX descriptor of the A-MPDU.
uint32_t | max_len [NX_BW_LEN_STEPS]
| Maximum length of the A-MPDU.
uint16_t | mmss_bytes
| Minimum number of bytes per A-MPDU sub frame (to fulfill the spacing requirement).
uint16_t | nb_delims
| Number of blank delimiters set in current desc to ensure minimal spacing from previous MPDU.
uint8_t | max_cnt
| Maximum number of MPDUs inside the A-MPDU.
uint8_t | curr_cnt
| Current number of MPDUs inside the A-MPDU.
uint8_t | bw
| BW of transmission of the A-MPDU.
uint8_t | bw_idx
| Current step of per-bandwidth length.

## Detailed Description

Structure containing the information about the current A-MPDU being built.

Definition at line 162 of file txl_cntrl.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/tx/txl/txl_cntrl.h