<map id="G" name="G">
<area shape="rect" id="node2" href="$structtxl__list.html" title="Structure of a per&#45;AC Tx list." alt="" coords="1077,2779,1232,3090"/>
<area shape="rect" id="node4" href="$structco__list.html" title="structure of a list" alt="" coords="1608,853,1672,955"/>
<area shape="rect" id="node11" href="$structtxl__mumimo__build__info__tag.html" title="Structure containing the information about the MU&#45;MIMO PPDU being built." alt="" coords="1192,2462,1395,2703"/>
<area shape="rect" id="node40" href="$structtx__agg__desc.html" title="Aggregation descriptor, containing AMPDU THD, BAR descriptor, BAR payload and Policy..." alt="" coords="852,1357,993,1755"/>
<area shape="rect" id="node6" href="$structco__list__hdr.html" title="structure of a list element header" alt="" coords="721,200,815,285"/>
<area shape="rect" id="node14" href="$structtxdesc.html" title="LMAC Tx Descriptor." alt="" coords="657,2225,740,2362"/>
<area shape="rect" id="node63" href="$structbfr__mem__node.html" title="Structure representing a piece of BFR memory." alt="" coords="5,1144,128,1333"/>
<area shape="rect" id="node9" href="$structtx__hd.html" title="Definition of a TX header descriptor." alt="" coords="841,688,1004,1120"/>
<area shape="rect" id="node57" href="$structtx__hw__desc.html" title="Definition of a TX confirmation descriptor." alt="" coords="256,1496,360,1616"/>
<area shape="rect" id="node31" href="$structtxl__buffer__tag.html" title="Buffer header structure." alt="" coords="347,2453,480,2712"/>
<area shape="rect" id="node68" href="$structtxl__agg__build__tag.html" title="Structure containing the information about the current A&#45;MPDU being built." alt="" coords="853,2462,992,2703"/>
<area shape="rect" id="node16" href="$structhostdesc.html" title="Descriptor filled by the Host." alt="" coords="475,336,629,664"/>
<area shape="rect" id="node18" href="$structmac__addr.html" title="MAC address structure." alt="" coords="677,5,763,91"/>
<area shape="rect" id="node52" href="$structmac__hdr__ctrl.html" title="Structure of a long control frame MAC header." alt="" coords="1132,174,1241,311"/>
<area shape="rect" id="node20" href="$structumacdesc.html" title="Descriptor filled by the UMAC." alt="" coords="477,1822,611,2133"/>
<area shape="rect" id="node22" href="$structtxl__buffer__control.html" title="Control descriptor containing information about the transmission rates to use, the..." alt="" coords="401,1470,551,1642"/>
<area shape="rect" id="node24" href="$structtx__policy__tbl.html" title="Policy Table Structure used to store Policy Table Information used by MAC HW to prepare..." alt="" coords="687,809,817,999"/>
<area shape="rect" id="node26" href="$structtx__compressed__policy__tbl.html" title="Compressed Policy Table Structure used to store Policy Table Information used by..." alt="" coords="367,853,561,955"/>
<area shape="rect" id="node29" href="$structlmacdesc.html" title="Descriptor filled by the LMAC." alt="" coords="277,1909,376,2046"/>
<area shape="rect" id="node34" href="$structdma__desc.html" title="Element in the pool of TX DMA bridge descriptors." alt="" coords="113,827,204,981"/>
<area shape="rect" id="node36" href="$structtx__pbd.html" title="Definition of a TX payload buffer descriptor." alt="" coords="467,2216,587,2371"/>
<area shape="rect" id="node45" href="$structba__ssc__bitmap.html" title="Structure of generic BA SSC + bitmap." alt="" coords="1301,853,1421,955"/>
<area shape="rect" id="node50" href="$structbar__frame.html" title="Structure of a Block Acknowledgment Request frame." alt="" coords="1445,844,1584,964"/>
<area shape="rect" id="node55" href="$structba__ssc__bitmap__256.html" title="Structure of BA SSC + 256&#45;bit bitmap." alt="" coords="1125,853,1277,955"/>
<area shape="rect" id="node61" href="$structtx__cfm__tag.html" title="Structure indicating the status and other information about the transmission." alt="" coords="228,809,343,999"/>
</map>
