# tx_cfm_tag Struct Reference
[HWDESC]

Structure indicating the status and other information about the transmission. More...

`#include <hal_desc.h>`

## Data Fields
uint16_t | pn [4]
| PN that was used for the transmission.
uint16_t | sn
| Sequence number of the packet.
uint16_t | timestamp
| Timestamp of first transmission of this MPDU.
int8_t | credits
| Number of flow control credits allocated.
uint8_t | ampdu_size
| Size (in mdpu) of the A-MPDU in which this frame as been transmitted.
uint16_t | amsdu_size
| Size allowed for AMSDU.
uint32_t | status
| TX status.

## Detailed Description

Structure indicating the status and other information about the transmission.

Definition at line 1012 of file hal_desc.h.

## Field Documentation

uint8_t tx_cfm_tag::ampdu_size

Size (in mdpu) of the A-MPDU in which this frame as been transmitted.

Valid only for singleton (=1) or last frame of the A-MPDU

Definition at line 1027 of file hal_desc.h.

Referenced by txl_mumimo_ampdu_finish().

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/hal/hal_desc.h