- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

# /space/home/slher/rel/Beken/v6_4_5/macsw/modules/dbg/src/dbg_profiling.c

Go to the documentation of this file.

    00001
    00020 /*
    00021  * INCLUDE FILES
    00022  ****************************************************************************************
    00023  */
    00024 #include "dbg_profiling.h"
    00025
    00026 /*
    00027  * GLOBAL VARIABLES
    00028  ****************************************************************************************
    00029  */
    00030 #if NX_PROFILING_ON
    00031 const char * const dbg_prof_conf[DBG_PROF_MAX] =
    00032 {
    00033     #ifdef TX_IPC_IRQ_DEF
    00034     [TX_IPC_IRQ] = "TX_IPC_IRQ",
    00035     #endif
    00036     #ifdef TX_MACIF_EVT_DEF
    00037     [TX_MACIF_EVT] = "TX_MACIF_EVT",
    00038     #endif
    00039     #ifdef TX_DMA_IRQ_DEF
    00040     [TX_DMA_IRQ] = "TX_DMA_IRQ",
    00041     #endif
    00042     #ifdef TX_NEW_TAIL_DEF
    00043     [TX_NEW_TAIL] = "TX_NEW_TAIL",
    00044     #endif
    00045     #ifdef TX_MAC_IRQ_DEF
    00046     [TX_MAC_IRQ] = "TX_MAC_IRQ",
    00047     #endif
    00048     #ifdef TX_HE_TRIG_IRQ_DEF
    00049     [TX_HE_TRIG_IRQ] = "TX_HE_TRIG_IRQ",
    00050     #endif
    00051     #ifdef TX_BUF_FREE_DEF
    00052     [TX_BUF_FREE]= "TX_BUF_FREE",
    00053     #endif
    00054     #ifdef TX_BUF_ALLOC_DEF
    00055     [TX_BUF_ALLOC] = "TX_BUF_ALLOC",
    00056     #endif
    00057     #ifdef TX_PAYL_HDL_DEF
    00058     [TX_PAYL_HDL] = "TX_PAYL_HDL",
    00059     #endif
    00060     #ifdef TX_CFM_EVT_DEF
    00061     [TX_CFM_EVT] = "TX_CFM_EVT",
    00062     #endif
    00063     #ifdef TX_CFM_DMA_IRQ_DEF
    00064     [TX_CFM_DMA_IRQ] = "TX_CFM_DMA_IRQ",
    00065     #endif
    00066     #ifdef MSG_BASIC_PROF_DEF
    00067     [MSG_IRQ]     = "MSG_IRQ",
    00068     [MSG_FWD]     = "MSG_FWD",
    00069     [MSG_IPC_IND] = "MSG_IPC_IND",
    00070     #endif
    00071     #ifdef RX_MAC_IRQ_DEF
    00072     [RX_MAC_IRQ] = "RX_MAC_IRQ",
    00073     #endif
    00074     #ifdef RX_DMA_IRQ_DEF
    00075     [RX_DMA_IRQ] = "RX_DMA_IRQ",
    00076     #endif
    00077     #ifdef RX_DMA_EVT_DEF
    00078     [RX_DMA_EVT] = "RX_DMA_EVT",
    00079     #endif
    00080     #ifdef RX_IPC_IND_DEF
    00081     [RX_IPC_IND] = "RX_IPC_IND",
    00082     #endif
    00083     #ifdef RX_MPDU_XFER_DEF
    00084     [RX_MPDU_XFER] = "RX_MPDU_XFER",
    00085     #endif
    00086     #ifdef RX_MPDU_FREE_DEF
    00087     [RX_MPDU_FREE] = "RX_MPDU_FREE",
    00088     #endif
    00089     #ifdef RX_CNTRL_EVT_DEF
    00090     [RX_CNTRL_EVT] = "RX_CNTRL_EVT",
    00091     #endif
    00092     #ifdef MM_HW_IDLE_DEF
    00093     [MM_HW_IDLE] = "MM_HW_IDLE",
    00094     #endif
    00095     #ifdef MM_SET_CHANNEL_DEF
    00096     [MM_SET_CHANNEL] = "MM_SET_CHANNEL",
    00097     #endif
    00098     #ifdef AGG_FIRST_MPDU_DWNLD_DEF
    00099     [AGG_FIRST_MPDU_DWNLD] = "AGG_FIRST_MPDU_DWNLD",
    00100     #endif
    00101     #ifdef AGG_START_AMPDU_DEF
    00102     [AGG_START_AMPDU] = "AGG_START_AMPDU",
    00103     #endif
    00104     #ifdef AGG_ADD_MPDU_DEF
    00105     [AGG_ADD_MPDU] = "AGG_ADD_MPDU",
    00106     #endif
    00107     #ifdef AGG_SMPDU_DONETX_DEF
    00108     [AGG_SMPDU_DONETX] = "AGG_SMPDU_DONETX",
    00109     #endif
    00110     #ifdef AGG_FINISH_AMPDU_DEF
    00111     [AGG_FINISH_AMPDU] = "AGG_FINISH_AMPDU",
    00112     #endif
    00113     #ifdef AGG_BAR_DONETX_DEF
    00114     [AGG_BAR_DONETX] = "AGG_BAR_DONETX",
    00115     #endif
    00116     #ifdef AGG_BA_RXED_DEF
    00117     [AGG_BA_RXED] = "AGG_BA_RXED",
    00118     #endif
    00119
    00120     #ifdef MU_SEC_USER_IRQ_DEF
    00121     [MU_SEC_USER_IRQ] = "MU_SEC_USER_IRQ",
    00122     #endif
    00123     #ifdef MU_PPDU_START_DEF
    00124     [MU_PPDU_START] = "MU_PPDU_START",
    00125     #endif
    00126     #ifdef MU_MPDU_ADD_DEF
    00127     [MU_MPDU_ADD] = "MU_MPDU_ADD",
    00128     #endif
    00129     #ifdef MU_PPDU_CLOSE_DEF
    00130     [MU_PPDU_CLOSE] = "MU_PPDU_CLOSE",
    00131     #endif
    00132     #ifdef MU_USER_POS_DEF
    00133     [MU_USER_POS] = "MU_USER_POS[0]",
    00134     [MU_USER_POS + 1] = "MU_USER_POS[1]",
    00135     #endif
    00136     #ifdef MU_USER_POS_IRQ_DEF
    00137     [MU_USER_POS_IRQ] = "MU_USER_POS_IRQ[0]",
    00138     [MU_USER_POS_IRQ + 1] = "MU_USER_POS_IRQ[1]",
    00139     #endif
    00140
    00141     #ifdef CHAN_CTXT_CDE_EVT_PROF_DEF
    00142     [CHAN_CTXT_CDE_EVT] = "CHAN_CTXT_CDE_EVT",
    00143     #endif
    00144     #ifdef CHAN_CTXT_TBTT_SWITCH_PROF_DEF
    00145     [CHAN_CTXT_TBTT_SWITCH] = "CHAN_CTXT_TBTT_SWITCH",
    00146     #endif
    00147     #ifdef CHAN_CTXT_IDX_PROF_DEF
    00148     [CHAN_CTXT_IDX_PROF]     = "CHAN_CTXT_IDX_PROF[0]",
    00149     [CHAN_CTXT_IDX_PROF + 1] = "CHAN_CTXT_IDX_PROF[1]",
    00150     [CHAN_CTXT_IDX_PROF + 2] = "CHAN_CTXT_IDX_PROF[2]",
    00151     #endif
    00152     #ifdef CHAN_CTXT_TX_DISCARD_PROF_DEF
    00153     [CHAN_CTXT_TX_DISCARD]  = "CHAN_CTXT_TX_DISCARD",
    00154     #endif
    00155     #ifdef CHAN_CTXT_WAIT_END_PROF_DEF
    00156     [CHAN_CTXT_WAIT_END]    = "CHAN_CTXT_WAIT_END",
    00157     #endif
    00158     #ifdef CHAN_CTXT_SWITCH_PROF_DEF
    00159     [CHAN_CTXT_SWITCH] = "CHAN_CTXT_SWITCH",
    00160     #endif
    00161     #ifdef CHAN_CTXT_TBTT_PRES_PROF_DEF
    00162     [CHAN_CTXT_TBTT_PRES] = "CHAN_CTXT_TBTT_PRES",
    00163     #endif
    00164
    00165     #ifdef P2P_NOA_ABS_DEF
    00166     [P2P_NOA_0_ABS]  = "P2P_NOA_0_ABS",
    00167     [P2P_NOA_1_ABS]  = "P2P_NOA_1_ABS",
    00168     #endif
    00169     #ifdef P2P_CTW_DEF
    00170     [P2P_CTW]        = "P2P_CTW",
    00171     #endif
    00172     #ifdef P2P_WAIT_BCN_DEF
    00173     [P2P_WAIT_BCN]   = "P2P_WAIT_BCN",
    00174     #endif
    00175     #ifdef P2P_ABSENCE_DEF
    00176     [P2P_ABSENCE]    = "P2P_ABSENCE",
    00177     #endif
    00178     #ifdef P2P_PS_PAUSED_DEF
    00179     [P2P_PS_PAUSED]  = "P2P_PS_PAUSED",
    00180     #endif
    00181
    00182     #ifdef RADAR_IRQ_DEF
    00183     [RADAR_IRQ] = "RADAR_IRQ",
    00184     #endif
    00185     #ifdef TX_FRAME_PUSH_DEF
    00186     [TX_FRAME_PUSH] = "TX_FRAME_PUSH",
    00187     #endif
    00188     #ifdef TX_FRAME_CFM_DEF
    00189     [TX_FRAME_CFM] = "TX_FRAME_CFM",
    00190     #endif
    00191     #ifdef TX_AC_BG_DEF
    00192     [TX_AC_BG]      = "TX_AC_BG[0]",
    00193     [TX_AC_BG + 1]  = "TX_AC_BG[1]",
    00194     #endif
    00195     #ifdef TX_AC_IRQ_DEF
    00196     [TX_AC_IRQ]      = "TX_AC_IRQ[0]",
    00197     [TX_AC_IRQ + 1]  = "TX_AC_IRQ[1]",
    00198     #endif
    00199     #ifdef BCN_PRIM_TBTT_IRQ_DEF
    00200     [BCN_PRIM_TBTT_IRQ] = "BCN_PRIM_TBTT_IRQ",
    00201     #endif
    00202     #ifdef BCN_SEC_TBTT_IRQ_DEF
    00203     [BCN_SEC_TBTT_IRQ] = "BCN_SEC_TBTT_IRQ",
    00204     #endif
    00205     #ifdef HW_TBTT_EVT_DEF
    00206     [HW_TBTT_EVT] = "HW_TBTT_EVT",
    00207     #endif
    00208     #ifdef AP_TBTT_DEF
    00209     [AP_TBTT] = "AP_TBTT",
    00210     #endif
    00211     #ifdef STA_TBTT_DEF
    00212     [STA_TBTT] = "STA_TBTT",
    00213     #endif
    00214     #ifdef TBTT_IDX_DEF
    00215     [TBTT_IDX_PROF]     = "TBTT_IDX_PROF[0]",
    00216     [TBTT_IDX_PROF + 1] = "TBTT_IDX_PROF[1]",
    00217     [TBTT_IDX_PROF + 2] = "TBTT_IDX_PROF[2]",
    00218     #endif
    00219
    00220     #ifdef PS_SLEEP_DEF
    00221     [PS_SLEEP]          = "PS_SLEEP",
    00222     #endif
    00223     #ifdef PS_PAUSE_DEF
    00224     [PS_PAUSE]          = "PS_PAUSE",
    00225     #endif
    00226     #ifdef PS_DPSM_UPDATE_DEF
    00227     [PS_DPSM_UPDATE]    = "PS_DPSM_UPDATE",
    00228     #endif
    00229     #ifdef PS_CHECK_RX_DEF
    00230     [PS_CHECK_RX]       = "PS_CHECK_RX",
    00231     #endif
    00232     #ifdef PS_CHECK_TX_DEF
    00233     [PS_CHECK_TX]       = "PS_CHECK_TX",
    00234     #endif
    00235     #ifdef PS_CHECK_BCN_DEF
    00236     [PS_CHECK_BCN]      = "PS_CHECK_BCN",
    00237     #endif
    00238
    00239     #ifdef TD_CHECK_RX_DEF
    00240     [TD_CHECK_RX]       = "TD_CHECK_RX",
    00241     #endif
    00242     #ifdef TD_CHECK_TX_DEF
    00243     [TD_CHECK_TX]       = "TD_CHECK_TX",
    00244     #endif
    00245     #ifdef TD_CHECK_RX_PS_DEF
    00246     [TD_CHECK_RX_PS]    = "TD_CHECK_RX_PS",
    00247     #endif
    00248     #ifdef TD_CHECK_TX_PS_DEF
    00249     [TD_CHECK_TX_PS]    = "TD_CHECK_TX_PS",
    00250     #endif
    00251     #ifdef TD_TIMER_END_DEF
    00252     [TD_TIMER_END]      = "TD_TIMER_END",
    00253     #endif
    00254
    00255     #ifdef BFR_MU_CALIB_DEF
    00256     [BFR_MU_CALIB]      = "BFR_MU_CALIB",
    00257     #endif //(BFR_MU_CALIB_DEF)
    00258     #ifdef BFR_SU_CALIB_DEF
    00259     [BFR_SU_CALIB]      = "BFR_SU_CALIB",
    00260     #endif //(BFR_SU_CALIB_DEF)
    00261     #ifdef BFR_RX_BFR_DEF
    00262     [BFR_RX_BFR]        = "BFR_RX_BFR",
    00263     #endif //(BFR_RX_BFR_DEF)
    00264     #ifdef BFR_UPLOAD_DEF
    00265     [BFR_UPLOAD]        = "BFR_UPLOAD",
    00266     #endif //(BFR_UPLOAD_DEF)
    00267     #ifdef BFR_DOWNLOAD_DEF
    00268     [BFR_DOWNLOAD]      = "BFR_DOWNLOAD",
    00269     #endif //(BFR_DOWNLOAD_DEF)
    00270     #ifdef BFR_TX_IND_DEF
    00271     [BFR_TX_IND]        = "BFR_TX_IND",
    00272     #endif //(BFR_TX_IND_DEF)
    00273     #ifdef BFR_TX_CFM_DEF
    00274     [BFR_TX_CFM]        = "BFR_TX_CFM",
    00275     #endif //(BFR_TX_CFM_DEF)
    00276     #ifdef BFR_SMM_IDX_DEF
    00277     [BFR_SMM_IDX_0]     = "BFR_SMM_IDX[0]",
    00278     [BFR_SMM_IDX_1]     = "BFR_SMM_IDX[1]",
    00279     [BFR_SMM_IDX_2]     = "BFR_SMM_IDX[2]",
    00280     [BFR_SMM_IDX_LAST]  = "BFR_SMM_IDX[3]",
    00281     #endif //(BFR_SMM_IDX_DEF)
    00282
    00283     #ifdef RX_DUPLI_CHECK_DEF
    00284     [RX_DUPLI_CHECK]      = "RX_DUPLI_CHECK",
    00285     #endif
    00286     #ifdef RX_DUPLI_NSTA_CHECK_DEF
    00287     [RX_DUPLI_NSTA_CHECK] = "RX_DUPLI_NSTA_CHECK",
    00288     #endif
    00289
    00290     #ifdef IPCDESC_PREPARE_DEF
    00291     [IPCDESC_PREPARE]     = "IPCDESC_PREPARE",
    00292     #endif
    00293     #ifdef IPCDESC_TRANSFER_DEF
    00294     [IPCDESC_TRANSFER]    = "IPCDESC_TRANSFER",
    00295     #endif
    00296
    00297     #ifdef DEFRAG_CHECK_DEF
    00298     [DEFRAG_CHECK]        = "DEFRAG_CHECK",
    00299     #endif
    00300     #ifdef DEFRAG_TRANSFER_DEF
    00301     [DEFRAG_TRANSFER]     = "DEFRAG_TRANSFER",
    00302     #endif
    00303     #ifdef DEFRAG_UPD_LENGTH_DEF
    00304     [DEFRAG_UPD_LENGTH]   = "DEFRAG_UPD_LENGTH",
    00305     #endif
    00306
    00307     #ifdef REORD_CHECK_DEF
    00308     [REORD_CHECK]         = "REORD_CHECK",
    00309     #endif
    00310     #ifdef REORD_BAR_CHECK_DEF
    00311     [REORD_BAR_CHECK]     = "REORD_BAR_CHECK",
    00312     #endif
    00313     #ifdef REORD_FLUSH_DEF
    00314     [REORD_FLUSH]         = "REORD_FLUSH",
    00315     #endif
    00316     #ifdef REORD_FWD_DEF
    00317     [REORD_FWD]           = "REORD_FWD",
    00318     #endif
    00319
    00320     #ifdef MAC2ETH_UPDATE_DEF
    00321     [MAC2ETH_UPDATE]      = "MAC2ETH_UPDATE",
    00322     #endif
    00323
    00324     #ifdef PS_PEER_STATE_DEF
    00325     [PS_PEER_STATE]       = "PS_PEER_STATE",
    00326     #endif
    00327     #ifdef PS_BCMC_STATE_DEF
    00328     [PS_BCMC_STATE]       = "PS_BCMC_STATE",
    00329     #endif
    00330     #ifdef PS_STATE_VAL_DEF
    00331     [PS_STATE_VAL]        = "PS_STATE_VAL[0]",
    00332     [PS_STATE_VAL + 1]    = "PS_STATE_VAL[1]",
    00333     #endif
    00334     #ifdef PS_PSPOLL_RX_DEF
    00335     [PS_PSPOLL_RX]        = "PS_PSPOLL_RX",
    00336     #endif
    00337     #ifdef PS_TRAFFIC_REQ_DEF
    00338     [PS_TRAFFIC_REQ]      = "PS_TRAFFIC_REQ",
    00339     #endif
    00340     #ifdef BW_DROP_IRQ_DEF
    00341     [BW_DROP_IRQ]         = "BW_DROP_IRQ",
    00342     #endif
    00343     #ifdef BW_DROP_STEP_DEF
    00344     [BW_DROP_STEP]        = "BW_DROP_STEP",
    00345     #endif
    00346     #ifdef RC_UPD_COUNTERS_DEF
    00347     [RC_UPD_COUNTERS]     = "RC_UPD_COUNTERS",
    00348     #endif
    00349     #ifdef RC_UPD_COUNTERS_TRIAL_DEF
    00350     [RC_UPD_COUNTERS_TRIAL]     = "RC_UPD_COUNTERS_TRIAL",
    00351     #endif
    00352     #ifdef RC_STATS_CALC_DEF
    00353     [RC_STATS_CALC]       = "RC_STATS_CALC",
    00354     #endif
    00355     #ifdef RC_UPD_RETRY_CHAIN_DEF
    00356     [RC_UPD_RETRY_CHAIN]  = "RC_UPD_RETRY_CHAIN",
    00357     #endif
    00358     #ifdef RC_UPD_RETRY_CHAIN_TRIAL_DEF
    00359     [RC_UPD_RETRY_CHAIN_TRIAL] = "RC_UPD_RETRY_CHAIN_TRIAL",
    00360     #endif
    00361     #ifdef RC_SET_TRIAL_BUFFER_DEF
    00362     [RC_SET_TRIAL_BUFFER] = "RC_SET_TRIAL_BUFFER",
    00363     #endif
    00364     #ifdef RC_LOOKAROUND_TX_DEF
    00365     [RC_LOOKAROUND_TX]    = "RC_LOOKAROUND_TX",
    00366     #endif
    00367     #ifdef RC_SW_RETRY_DEF
    00368     [RC_SW_RETRY]         = "RC_SW_RETRY",
    00369     #endif
    00370
    00371     #ifdef FT_OVER_DS_REQ_DEF
    00372     [FT_OVER_DS_REQ]      = "FT_OVER_DS_REQ",
    00373     #endif
    00374     #ifdef FT_REASSOC_DEF
    00375     [FT_REASSOC]          = "FT_REASSOC",
    00376     #endif
    00377
    00378     #ifdef MESH_PS_ENABLE_DEF
    00379     [MESH_PS_ENABLE]      = "MESH_PS_ENABLE",
    00380     #endif //(MESH_PS_ENABLE_DEF)
    00381     #ifdef MESH_PS_SP_OWNER_DEF
    00382     [MESH_PS_SP_OWNER]    = "MESH_PS_SP_OWNER",
    00383     #endif //(MESH_PS_SP_OWNER_DEF)
    00384     #ifdef MESH_PS_SP_RECIP_DEF
    00385     [MESH_PS_SP_RECIP]    = "MESH_PS_SP_RECIP",
    00386     #endif //(MESH_PS_SP_RECIP_DEF)
    00387     #ifdef MESH_PS_WAIT_BCMC_DEF
    00388     [MESH_PS_WAIT_BCMC]   = "MESH_PS_WAIT_BCMC",
    00389     #endif //(MESH_PS_WAIT_BCMC_DEF)
    00390     #ifdef MESH_PS_WAIT_BCN_DEF
    00391     [MESH_PS_WAIT_BCN]    = "MESH_PS_WAIT_BCN",
    00392     #endif //(MESH_PS_WAIT_BCN_DEF)
    00393     #ifdef MESH_PS_LOCAL_MAW_DEF
    00394     [MESH_PS_LOCAL_MAW]   = "MESH_PS_LOCAL_MAW",
    00395     #endif //(MESH_PS_LOCAL_MAW_DEF)
    00396     #ifdef MESH_PS_PEER_MAW_DEF
    00397     [MESH_PS_PEER_MAW]    = "MESH_PS_PEER_MAW",
    00398     #endif //(MESH_PS_PEER_MAW_DEF)
    00399
    00400     #ifdef CPU_SLEEP_DEF
    00401     [CPU_SLEEP]           = "CPU_SLEEP",
    00402     #endif //CPU_SLEEP_DEF
    00403     #ifdef DEEP_SLEEP_DEF
    00404     [DEEP_SLEEP]           = "DEEP_SLEEP",
    00405     #endif //DEEP_SLEEP_DEF
    00406
    00407     #ifdef TDLS_CHSW_REQ_RX_DEF
    00408     [TDLS_RX_CHSW_REQ] = "TDLS_RX_CHSW_REQ",
    00409     #endif
    00410     #ifdef TDLS_CHSW_RESP_RX_DEF
    00411     [TDLS_RX_CHSW_RESP] = "TDLS_RX_CHSW_RESP",
    00412     #endif
    00413     #ifdef TDLS_CHSW_REQ_TX_DEF
    00414     [TDLS_TX_CHSW_REQ] = "TDLS_TX_CHSW_REQ",
    00415     #endif
    00416     #ifdef TDLS_CHSW_RESP_TX_DEF
    00417     [TDLS_TX_CHSW_RESP] = "TDLS_TX_CHSW_RESP",
    00418     #endif
    00419     #ifdef TDLS_SWITCH_TO_OFFCH_DEF
    00420     [TDLS_SWITCH_TO_OFFCH] = "TDLS_SWITCH_TO_OFFCH",
    00421     #endif
    00422     #ifdef TDLS_SWITCH_TO_BASECH_DEF
    00423     [TDLS_SWITCH_TO_BASECH]= "TDLS_SWITCH_TO_BASECH",
    00424     #endif
    00425     #ifdef TDLS_CHSW_TIME_TIMER_DEF
    00426     [TDLS_CHSW_TIME_TIMER]  = "TDLS_CHSW_TIME_TIMER",
    00427     #endif
    00428     #ifdef TDLS_CHSW_TIMEOUT_TIMER_DEF
    00429     [TDLS_CHSW_TIMEOUT_TIMER]= "TDLS_CHSW_TIMEOUT_TIMER",
    00430     #endif
    00431     #ifdef TDLS_CHSW_END_TIMER_DEF
    00432     [TDLS_CHSW_END_TIMER]= "TDLS_CHSW_END_TIMER",
    00433     #endif
    00434     #ifdef TDLS_CHSW_REQ_TX_TIMER_DEF
    00435     [TDLS_CHSW_REQ_TX_TIMER]= "TDLS_CHSW_REQ_TX_TIMER",
    00436     #endif
    00437     #ifdef TDLS_DELAY_CHSW_DEF
    00438     [TDLS_DELAY_CHSW]= "TDLS_DELAY_CHSW",
    00439     #endif
    00440     #ifdef TDLS_CHSW_NULL_FRAME_TX_DEF
    00441     [TDLS_TX_CHSW_NULL_FRAME]= "TDLS_TX_CHSW_NULL_FRAME",
    00442     #endif
    00443     #ifdef RTOS_TASK_DEF
    00444     [RTOS_TASK]     = "RTOS_TASK[0]",
    00445     [RTOS_TASK + 1] = "RTOS_TASK[1]",
    00446     [RTOS_TASK + 2] = "RTOS_TASK[2]",
    00447     [RTOS_TASK + 3] = "RTOS_TASK[3]",
    00448     #endif
    00449     #ifdef ANT_DIV_SWITCH_DEF
    00450     [ANT_DIV_SWITCH]= "ANT_DIV_SWITCH",
    00451     #endif
    00452
    00453 };
    00454 #endif
    00455
    00457