# sta_capa_info Struct Reference
[STA_MGMT]

Station capability information. More...

`#include <sta_mgmt.h>`

Collaboration diagram for sta_capa_info:
[legend]

## Data Fields
struct mac_rateset | rate_set
| Legacy rate set supported by the STA.
struct mac_htcapability | ht_cap
| HT capabilities.
uint32_t | capa_flags
| Bitfield showing some capabilities of the STA (STA_QOS_CAPA, STA_HT_CAPA, STA_VHT_CAPA, STA_MFP_CAPA).
uint8_t | phy_bw_max
| Maximum PHY channel bandwidth supported by the STA.
uint8_t | bw_cur
| Current channel bandwidth for the STA.
uint8_t | uapsd_queues
| Bit field indicating which queues have to be delivered upon U-APSD trigger.
uint8_t | max_sp_len
| Maximum size, in frames, of a APSD service period.
uint8_t | stbc_nss
| Maximum number of spatial streams supported for STBC reception.

## Detailed Description

Station capability information.

Definition at line 198 of file sta_mgmt.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/sta/sta_mgmt.h