# mm_p2p_noa_upd_ind Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_P2P_NOA_UPD_IND message. More...

`#include <mm_task.h>`

## Data Fields
uint8_t | vif_index
| VIF Index.
uint8_t | noa_inst_nb
| NOA Instance Number.
uint8_t | noa_type
| NoA Type.
uint8_t | count
| Count.
uint32_t | duration_us
| Duration (in us).
uint32_t | interval_us
| Interval (in us).
uint32_t | start_time
| Start Time.

## Detailed Description

Structure containing the parameters of the MM_P2P_NOA_UPD_IND message.

Definition at line 1029 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h