# mm_bcn_change_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_BCN_CHANGE_REQ message. More...

`#include <mm_task.h>`

## Data Fields
uint32_t | bcn_ptr
| Pointer, in host memory, to the new beacon template.
uint16_t | bcn_len
| Length of the beacon template.
uint16_t | tim_oft
| Offset of the TIM IE in the beacon.
uint8_t | tim_len
| Length of the TIM IE.
uint8_t | inst_nbr
| Index of the VIF for which the beacon is updated.
uint8_t | csa_oft [BCN_MAX_CSA_CPT]
| Offset of CSA (channel switch announcement) counters (0 means no counter).

## Detailed Description

Structure containing the parameters of the MM_BCN_CHANGE_REQ message.

Definition at line 772 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h