# mm_traffic_req_ind Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_TRAFFIC_REQ_IND message. More...

`#include <mm_task.h>`

## Data Fields
uint8_t | sta_idx
| Index of the peer device that needs traffic.
uint8_t | pkt_cnt
| Number of packets that need to be sent (if 0, all buffered traffic shall be sent and if set to PS_SP_INTERRUPTED, it means that current service period has been interrupted).
bool | uapsd
| Flag indicating if the traffic request concerns U-APSD queues or not.

## Detailed Description

Structure containing the parameters of the MM_TRAFFIC_REQ_IND message.

Definition at line 818 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h