# bam_addba_rsp Struct Reference
[BAM]

ADDBA Response frame Action field format (see IEEE 802.11-2012, section 8.5.5.3). More...

`#include <bam.h>`

## Data Fields
uint8_t | category
| Category - Set to 3 (representing Block Ack).
uint8_t | action
| Block Ack Action - Set to 1 (representing ADDBA response).
uint8_t | dialog_token
| Dialog Token - Copied from received ADDBA Request frame.
uint16_t | status_code
| Status Code.
uint16_t | ba_param_set
| Block Ack Parameter Set (from LSB to MSB) --------------------------------------------------------------- | A-MSDU Supported | Block Ack Policy | TID | Buffer Size | | 1 bit | 1 bit | 4 bits | 10 bits | ---------------------------------------------------------------.
uint16_t | ba_timeout
| Block Ack Timeout Value - In TUs. A value of 0 disables the timeout.

## Detailed Description

ADDBA Response frame Action field format (see IEEE 802.11-2012, section 8.5.5.3).

Definition at line 239 of file bam.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/bam/bam.h