# mm_version_cfm Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_VERSION_CFM message. More...

`#include <mm_task.h>`

## Data Fields
uint32_t | version_lmac
| Version of the LMAC FW.
uint32_t | version_machw_1
| Version1 of the MAC HW (as encoded in version1Reg MAC HW register).
uint32_t | version_machw_2
| Version2 of the MAC HW (as encoded in version2Reg MAC HW register).
uint32_t | version_phy_1
| Version1 of the PHY (depends on actual PHY).
uint32_t | version_phy_2
| Version2 of the PHY (depends on actual PHY).
uint32_t | features
| Supported Features.
uint16_t | max_sta_nb
| Maximum number of supported stations.
uint8_t | max_vif_nb
| Maximum number of supported virtual interfaces.

## Detailed Description

Structure containing the parameters of the MM_VERSION_CFM message.

Definition at line 494 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h