# mm_set_p2p_noa_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_SET_P2P_NOA_REQ message. More...

`#include <mm_task.h>`

## Data Fields
uint8_t | vif_index
| VIF Index.
uint8_t | noa_inst_nb
| Allocated NOA Instance Number - Valid only if count = 0.
uint8_t | count
| Count.
bool | dyn_noa
| Indicate if NoA can be paused for traffic reason.
uint32_t | duration_us
| Duration (in us).
uint32_t | interval_us
| Interval (in us).
uint32_t | start_offset
| Start Time offset from next TBTT (in us).

## Detailed Description

Structure containing the parameters of the MM_SET_P2P_NOA_REQ message.

Definition at line 987 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h