# sta_pol_tbl_cntl Struct Reference
[STA_MGMT]

Information related to the used policy table. More...

`#include <sta_mgmt.h>`

Collaboration diagram for sta_pol_tbl_cntl:
[legend]

## Data Fields
struct txl_buffer_control * | buf_ctrl
| Pointer to the buffer control structure.
struct rc_sta_stats * | sta_stats
| Pointer to the rate control algorithm structure.
uint32_t | prot_cfg
| Protection Configuration Mapped on Rate Control entry in policy table provided to the HW (see MAC HW USer Manual) Bit 28:26 - Format and Modulation of Protection frame for Transmission Bit 25:24 - Bandwidth of Protection Frame for Transmission Bit 23:17 - MCS Index of Protection Frame for Transmission Bit 16:14 - NAV Protection Frame Exchange Pushed inside Policy Table if Update Protection bit set to 1 in upd_field.
uint16_t | ppdu_tx_cfg
| PPDU Transmission Configuration Mapped on Rate Control entry in policy table provided to the HW (see MAC HW USer Manual) Bit 10 - Preamble Type of PPDU for Transmission -> Bit 10 Pushed inside Policy Table if Update PPDU TX bit set to 1 in upd_field.
uint8_t | upd_field
| Bit field indicating update to be done in the Policy Table.

## Detailed Description

Information related to the used policy table.

Definition at line 244 of file sta_mgmt.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/sta/sta_mgmt.h