<map id="G" name="G">
<area shape="rect" id="node2" href="$structco__list.html" title="structure of a list" alt="" coords="1251,853,1315,955"/>
<area shape="rect" id="node24" href="$structvif__info__tag.html" title="VIF Info Table." alt="" coords="957,3229,1128,4459"/>
<area shape="rect" id="node76" href="$structtx__agg__desc.html" title="Aggregation descriptor, containing AMPDU THD, BAR descriptor, BAR payload and Policy..." alt="" coords="1797,1357,1939,1755"/>
<area shape="rect" id="node4" href="$structco__list__hdr.html" title="structure of a list element header" alt="" coords="983,200,1076,285"/>
<area shape="rect" id="node21" href="$structke__msg.html" title="Message structure." alt="" coords="564,1153,668,1325"/>
<area shape="rect" id="node29" href="$structmm__timer__tag.html" title="Structure defining the properties of a timer." alt="" coords="988,1779,1111,1917"/>
<area shape="rect" id="node32" href="$structchan__tbtt__tag.html" title="Structure containing TBTT switch information." alt="" coords="571,2277,752,2501"/>
<area shape="rect" id="node51" href="$structtxdesc.html" title="LMAC Tx Descriptor." alt="" coords="2207,2551,2289,2689"/>
<area shape="rect" id="node100" href="$structbfr__mem__node.html" title="Structure representing a piece of BFR memory." alt="" coords="1349,1144,1472,1333"/>
<area shape="rect" id="node107" href="$structchan__ctxt__tag.html" title="Structure describing a channel context." alt="" coords="733,2843,875,3067"/>
<area shape="rect" id="node7" href="$structsm__connect__ind.html" title="Structure containing the parameters of the SM_CONNECT_IND message." alt="" coords="461,2799,611,3110"/>
<area shape="rect" id="node9" href="$structmac__addr.html" title="MAC address structure." alt="" coords="408,5,493,91"/>
<area shape="rect" id="node14" href="$structsm__connect__req.html" title="Structure containing the parameters of SM_CONNECT_REQ message." alt="" coords="73,2817,244,3093"/>
<area shape="rect" id="node36" href="$structme__bss__info.html" title="Information related to the BSS a VIF is linked to." alt="" coords="1547,2782,1699,3127"/>
<area shape="rect" id="node53" href="$structhostdesc.html" title="Descriptor filled by the Host." alt="" coords="1431,336,1585,664"/>
<area shape="rect" id="node89" href="$structmac__hdr__ctrl.html" title="Structure of a long control frame MAC header." alt="" coords="1551,174,1660,311"/>
<area shape="rect" id="node11" href="$structmac__chan__op.html" title="Operating Channel." alt="" coords="819,2525,941,2715"/>
<area shape="rect" id="node16" href="$structmac__ssid.html" title="SSID." alt="" coords="461,2569,544,2671"/>
<area shape="rect" id="node19" href="$structmac__chan__def.html" title="Primary Channel definition." alt="" coords="69,2551,187,2689"/>
<area shape="rect" id="node27" href="$structkey__info__tag.html" title="Structure containing the information about a key." alt="" coords="1193,2817,1305,3093"/>
<area shape="rect" id="node39" href="$structmac__rateset.html" title="Structure containing the legacy rateset of a station." alt="" coords="1769,2569,1879,2671"/>
<area shape="rect" id="node42" href="$structmobility__domain.html" title="Mobility Domain IE." alt="" coords="1903,2569,2065,2671"/>
<area shape="rect" id="node44" href="$structmac__htcapability.html" title="MAC HT capability information element." alt="" coords="1367,2534,1551,2706"/>
<area shape="rect" id="node47" href="$structmac__edca__param__set.html" title="EDCA Parameter Set Element." alt="" coords="1575,2551,1745,2689"/>
<area shape="rect" id="node49" href="$structtxl__frame__desc__tag.html" title="TX frame descriptor." alt="" coords="1331,2877,1485,3032"/>
<area shape="rect" id="node67" href="$structtxl__buffer__tag.html" title="Buffer header structure." alt="" coords="2400,2825,2533,3084"/>
<area shape="rect" id="node56" href="$structumacdesc.html" title="Descriptor filled by the UMAC." alt="" coords="2296,1942,2429,2253"/>
<area shape="rect" id="node58" href="$structtxl__buffer__control.html" title="Control descriptor containing information about the transmission rates to use, the..." alt="" coords="2324,1470,2473,1642"/>
<area shape="rect" id="node60" href="$structtx__policy__tbl.html" title="Policy Table Structure used to store Policy Table Information used by MAC HW to prepare..." alt="" coords="2111,809,2241,999"/>
<area shape="rect" id="node62" href="$structtx__compressed__policy__tbl.html" title="Compressed Policy Table Structure used to store Policy Table Information used by..." alt="" coords="2404,853,2599,955"/>
<area shape="rect" id="node65" href="$structlmacdesc.html" title="Descriptor filled by the LMAC." alt="" coords="2173,2029,2272,2166"/>
<area shape="rect" id="node70" href="$structdma__desc.html" title="Element in the pool of TX DMA bridge descriptors." alt="" coords="2623,827,2713,981"/>
<area shape="rect" id="node94" href="$structtx__hw__desc.html" title="Definition of a TX confirmation descriptor." alt="" coords="2184,1496,2288,1616"/>
<area shape="rect" id="node72" href="$structtx__pbd.html" title="Definition of a TX payload buffer descriptor." alt="" coords="2652,2543,2772,2697"/>
<area shape="rect" id="node80" href="$structtx__hd.html" title="Definition of a TX header descriptor." alt="" coords="1924,688,2087,1120"/>
<area shape="rect" id="node82" href="$structba__ssc__bitmap.html" title="Structure of generic BA SSC + bitmap." alt="" coords="1441,853,1561,955"/>
<area shape="rect" id="node87" href="$structbar__frame.html" title="Structure of a Block Acknowledgment Request frame." alt="" coords="1761,844,1900,964"/>
<area shape="rect" id="node92" href="$structba__ssc__bitmap__256.html" title="Structure of BA SSC + 256&#45;bit bitmap." alt="" coords="1585,853,1737,955"/>
<area shape="rect" id="node98" href="$structtx__cfm__tag.html" title="Structure indicating the status and other information about the transmission." alt="" coords="2265,809,2380,999"/>
<area shape="rect" id="node103" href="$structtxl__frame__cfm__tag.html" title="TX frame confirmation descriptor." alt="" coords="1193,2569,1343,2671"/>
</map>
