# mac_he_mcs_nss_supp Struct Reference
[MAC]

Structure listing the per-NSS, per-BW supported MCS combinations. More...

`#include <mac_types.h>`

## Data Fields
uint16_t | rx_mcs_80
| per-NSS supported MCS in RX, for BW <= 80MHz
uint16_t | tx_mcs_80
| per-NSS supported MCS in TX, for BW <= 80MHz
uint16_t | rx_mcs_160
| per-NSS supported MCS in RX, for BW = 160MHz
uint16_t | tx_mcs_160
| per-NSS supported MCS in TX, for BW = 160MHz
uint16_t | rx_mcs_80p80
| per-NSS supported MCS in RX, for BW = 80+80MHz
uint16_t | tx_mcs_80p80
| per-NSS supported MCS in TX, for BW = 80+80MHz

## Detailed Description

Structure listing the per-NSS, per-BW supported MCS combinations.

Definition at line 407 of file mac_types.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/modules/mac/src/mac_types.h