# me_env_tag Struct Reference
[ME]

ME environment structure. More...

`#include <me.h>`

Collaboration diagram for me_env_tag:
[legend]

## Data Fields
uint32_t | active_vifs
| Bitfield containing the ACTIVE state request of the different VIFs.
uint32_t | ps_disable_vifs
| Bitfield containing the PS state of the different VIFs.
ke_task_id_t | requester_id
| TaskID of the task requesting the last command.
struct mac_htcapability | ht_cap
| HT capabilities of the device.
uint16_t | tx_lft
| Lifetime of packets sent under a BlockAck agreement (expressed in TUs).
struct me_chan_config_req | chan
| List of supported channels.
uint8_t | stbc_nss
| Maximum number of Spatial Streams supported for a HT/VHT STBC transmission.
uint8_t | phy_bw_max
| Maximum supported BW.
uint8_t | capa_flags
| Local capability flags.
bool | ps_on
| Boolean indicating if PS mode shall be enabled or not.
uint8_t | ps_mode
| Mode that should be used when PS is enabled (PS_MODE_ON or PS_MODE_ON_DYN).

## Detailed Description

ME environment structure.

Definition at line 86 of file me.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/me/me.h