# tx_policy_tbl Struct Reference
[HWDESC]

Policy Table Structure used to store Policy Table Information used by MAC HW to prepare transmit vector to used by PHY. More...

`#include <hal_desc.h>`

## Data Fields
uint32_t | upatterntx
| Unique Pattern at the start of Policy Table.
uint32_t | phycntrlinfo1
| PHY Control Information 1 used by MAC HW.
uint32_t | phycntrlinfo2
| PHY Control Information 2 used by MAC HW.
uint32_t | maccntrlinfo1
| MAC Control Information 1 used by MAC HW.
uint32_t | maccntrlinfo2
| MAC Control Information 2 used by MAC HW.
uint32_t | ratecntrlinfo [RATE_CONTROL_STEPS]
| Rate Control Information used by MAC HW.
uint32_t | powercntrlinfo [RATE_CONTROL_STEPS]
| Power Control Information used by MAC HW.

## Detailed Description

Policy Table Structure used to store Policy Table Information used by MAC HW to prepare transmit vector to used by PHY.

Definition at line 784 of file hal_desc.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/hal/hal_desc.h