# mm_ps_change_ind Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_PS_CHANGE_IND message. More...

`#include <mm_task.h>`

## Data Fields
uint8_t | sta_idx
| Index of the peer device that is switching its PS state.
uint8_t | ps_state
| New PS state of the peer device (0: active, 1: sleeping).

## Detailed Description

Structure containing the parameters of the MM_PS_CHANGE_IND message.

Definition at line 800 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h