# me_set_active_req Struct Reference
[TASK_ME]

Structure containing the parameters of the ME_SET_ACTIVE_REQ message. More...

`#include <me_task.h>`

## Data Fields
bool | active
| Boolean indicating whether the VIF requests the HW to be passed in ACTIVE or IDLE.
uint8_t | vif_idx
| VIF index.

## Detailed Description

Structure containing the parameters of the ME_SET_ACTIVE_REQ message.

Definition at line 236 of file me_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/me/me_task.h