# rxl_hwdesc_env_tag Struct Reference
[RX_HWDESC]

Buffer Management control structure. More...

Collaboration diagram for rxl_hwdesc_env_tag:
[legend]

## Data Fields
struct co_list | ready
| Frames waiting for upload.
struct rx_dmadesc * | first_dmadesc
| First DMA descriptor the SW has to process.
struct rx_dmadesc * | last_dmadesc
| The last DMA descriptor in the HW list.
struct rx_dmadesc * | free_dmadesc
| The first free DMA descriptor in the HW list.
struct rx_pbd * | first
| First RX payload buffer descriptor chained to HW.
struct rx_pbd * | last
| Last RX payload buffer descriptor chained to HW.
struct rx_pbd * | free
| Free (spare) RX payload buffer descriptor (not chained to HW).
bool | monitor_en
| Flag indicating whether monitor mode is enabled or not.
struct rxl_buffer_tag | buf [2]
| Buffer parameters.

## Detailed Description

Buffer Management control structure.

Definition at line 47 of file rxl_hwdesc.c.

The documentation for this struct was generated from the following files:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/rx/rxl/v10/rxl_hwdesc.c
- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/rx/rxl/v20/rxl_hwdesc.c