# bam_delba Struct Reference
[BAM]

DELBA frame Action field format (see IEEE 802.11-2012, section 8.5.5.4). More...

`#include <bam.h>`

## Data Fields
uint8_t | category
| Category - Set to 3 (representing Block Ack).
uint8_t | action
| Block Ack Action - Set to 2 (representing DELBA).
uint16_t | delba_param
| DELBA Parameter Set (from LSB to MSB) ------------------------------------ | Reserved | Initiator | TID | | 11 bits | 1 bit | 4 bits | ------------------------------------.
uint16_t | reason_code
| Reason Code.

## Detailed Description

DELBA frame Action field format (see IEEE 802.11-2012, section 8.5.5.4).

Definition at line 262 of file bam.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/bam/bam.h