# mm_bfmer_enable_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_BFMER_ENABLE_REQ message. More...

`#include <mm_task.h>`

## Data Fields
uint32_t | host_bfr_addr
| Address of the beamforming report space allocated in host memory.
uint16_t | host_bfr_size
| Size of the beamforming report space allocated in host memory.
uint16_t | aid
| AID.
uint8_t | sta_idx
| STA Index.
uint8_t | rx_nss
| Maximum number of spatial streams the station can receive.
bool | vht_mu_bfmee
| Indicate if peer STA is MU Beamformee (VHT) capable.

## Detailed Description

Structure containing the parameters of the MM_BFMER_ENABLE_REQ message.

Definition at line 897 of file mm_task.h.

## Field Documentation

uint16_t mm_bfmer_enable_req::host_bfr_size

Size of the beamforming report space allocated in host memory.

This space should be twice the maximum size of the expected beamforming reports as the FW will divide it in two in order to be able to upload a new report while another one is used in transmission

Definition at line 905 of file mm_task.h.

Referenced by mm_bfmer_enable_req_handler().

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h