# rxu_cntrl_reord Struct Reference
[RXU]

RX reordering environment declaration. More...

`#include <rxu_cntrl.h>`

Collaboration diagram for rxu_cntrl_reord:
[legend]

## Data Fields
struct co_list_hdr | list_hdr
| Pointer to the next element in the queue.
uint32_t | sn_rx_time
| Time at which last waited SN has been received.
struct key_info_tag * | key
| Pointer to the key structure used for PN check.
uint16_t | win_start
| Lowest expected to be received (from 0 to 4096) = WinStartB IEEE Std 802.11-2012 section 9.21.7.6.1.
uint8_t | rx_status_pos
| Current position in the RX packet status array.
uint8_t | ooo_pkt_cnt
| Number of packet received out of order and waiting for next sn.
uint8_t | tid
| TID of the reordering structure.
struct rxu_cntrl_reord_elt | elt [RX_CNTRL_REORD_WIN_SIZE]
| Reordering buffer elements.
struct mm_timer_tag | timer
| MM timer structure used for flushing the reordering buffer.
bool | active
| Flag indicating if the reordering agreement is active or not.

## Detailed Description

RX reordering environment declaration.

Definition at line 212 of file rxu_cntrl.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/rxu/rxu_cntrl.h