# mm_ba_add_req Struct Reference
[MM_TASK]

Structure containing the parameters of the MM_BA_ADD_REQ message. More...

`#include <mm_task.h>`

## Data Fields
uint8_t | type
| Type of agreement (0: TX, 1: RX).
uint8_t | sta_idx
| Index of peer station with which the agreement is made.
uint8_t | tid
| TID for which the agreement is made with peer station.
uint8_t | bufsz
| Buffer size - number of MPDUs that can be held in its buffer per TID.
uint16_t | ssn
| Start sequence number negotiated during BA setup - the one in first aggregated MPDU counts more.

## Detailed Description

Structure containing the parameters of the MM_BA_ADD_REQ message.

Definition at line 613 of file mm_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/lmac/src/mm/mm_task.h