# bam_env_tag Struct Reference
[BAM]

Declaration of BAM environment. More...

`#include <bam.h>`

Collaboration diagram for bam_env_tag:
[legend]

## Data Fields
uint32_t | pkt_cnt
| Packet Counter.
uint32_t | last_activity_time
| Last activity time (TX or RX) on this BA agreement.
uint16_t | ssn
| Start sequence Number of BA.
uint16_t | ba_timeout
| BA Setup timeout value.
uint8_t | sta_idx
| Index of the station.
uint8_t | dev_type
| BA Device Type Originator/Responder (bam_ba_type).
uint8_t | ba_policy
| Block-Ack Policy Setup Immediate/Delayed (bam_ba_policy).
uint8_t | buffer_size
| Number of buffers available for this BA.
uint8_t | tid
| TID for block ack setting.
uint8_t | dialog_token
| Dialog token.
uint8_t | amsdu
| Is AMSDU allowed.
uint8_t | delba_count
| Number of time DELBA has been sent.
struct bam_baw * | baw
| Transmit window control structure.

## Detailed Description

Declaration of BAM environment.

Definition at line 303 of file bam.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/bam/bam.h