<map id="G" name="G">
<area shape="rect" id="node2" href="$structco__list.html" title="structure of a list" alt="" coords="1325,853,1389,955"/>
<area shape="rect" id="node59" href="$structtx__agg__desc.html" title="Aggregation descriptor, containing AMPDU THD, BAR descriptor, BAR payload and Policy..." alt="" coords="679,1357,820,1755"/>
<area shape="rect" id="node4" href="$structco__list__hdr.html" title="structure of a list element header" alt="" coords="1515,200,1608,285"/>
<area shape="rect" id="node9" href="$structmm__timer__tag.html" title="Structure defining the properties of a timer." alt="" coords="1684,1170,1807,1307"/>
<area shape="rect" id="node12" href="$structchan__tbtt__tag.html" title="Structure containing TBTT switch information." alt="" coords="1736,1779,1917,2003"/>
<area shape="rect" id="node34" href="$structtxdesc.html" title="LMAC Tx Descriptor." alt="" coords="708,2447,791,2585"/>
<area shape="rect" id="node83" href="$structbfr__mem__node.html" title="Structure representing a piece of BFR memory." alt="" coords="1365,1144,1488,1333"/>
<area shape="rect" id="node90" href="$structchan__ctxt__tag.html" title="Structure describing a channel context." alt="" coords="1864,2739,2005,2963"/>
<area shape="rect" id="node7" href="$structkey__info__tag.html" title="Structure containing the information about a key." alt="" coords="2387,2713,2499,2989"/>
<area shape="rect" id="node15" href="$structmac__addr.html" title="MAC address structure." alt="" coords="1729,5,1815,91"/>
<area shape="rect" id="node17" href="$structme__bss__info.html" title="Information related to the BSS a VIF is linked to." alt="" coords="2211,2678,2363,3023"/>
<area shape="rect" id="node36" href="$structhostdesc.html" title="Descriptor filled by the Host." alt="" coords="5,336,160,664"/>
<area shape="rect" id="node72" href="$structmac__hdr__ctrl.html" title="Structure of a long control frame MAC header." alt="" coords="711,174,820,311"/>
<area shape="rect" id="node19" href="$structmac__ssid.html" title="SSID." alt="" coords="2244,2465,2327,2567"/>
<area shape="rect" id="node21" href="$structmac__rateset.html" title="Structure containing the legacy rateset of a station." alt="" coords="2351,2465,2460,2567"/>
<area shape="rect" id="node24" href="$structmobility__domain.html" title="Mobility Domain IE." alt="" coords="2484,2465,2647,2567"/>
<area shape="rect" id="node26" href="$structmac__htcapability.html" title="MAC HT capability information element." alt="" coords="2671,2430,2855,2602"/>
<area shape="rect" id="node28" href="$structmac__chan__op.html" title="Operating Channel." alt="" coords="1992,2421,2115,2611"/>
<area shape="rect" id="node30" href="$structmac__edca__param__set.html" title="EDCA Parameter Set Element." alt="" coords="2879,2447,3049,2585"/>
<area shape="rect" id="node32" href="$structtxl__frame__desc__tag.html" title="TX frame descriptor." alt="" coords="665,2773,820,2928"/>
<area shape="rect" id="node50" href="$structtxl__buffer__tag.html" title="Buffer header structure." alt="" coords="844,2721,977,2980"/>
<area shape="rect" id="node39" href="$structumacdesc.html" title="Descriptor filled by the UMAC." alt="" coords="1092,2027,1225,2338"/>
<area shape="rect" id="node41" href="$structtxl__buffer__control.html" title="Control descriptor containing information about the transmission rates to use, the..." alt="" coords="1209,1470,1359,1642"/>
<area shape="rect" id="node43" href="$structtx__policy__tbl.html" title="Policy Table Structure used to store Policy Table Information used by MAC HW to prepare..." alt="" coords="1171,809,1301,999"/>
<area shape="rect" id="node45" href="$structtx__compressed__policy__tbl.html" title="Compressed Policy Table Structure used to store Policy Table Information used by..." alt="" coords="1464,853,1659,955"/>
<area shape="rect" id="node48" href="$structlmacdesc.html" title="Descriptor filled by the LMAC." alt="" coords="968,2114,1067,2251"/>
<area shape="rect" id="node53" href="$structdma__desc.html" title="Element in the pool of TX DMA bridge descriptors." alt="" coords="457,827,548,981"/>
<area shape="rect" id="node77" href="$structtx__hw__desc.html" title="Definition of a TX confirmation descriptor." alt="" coords="968,1496,1072,1616"/>
<area shape="rect" id="node55" href="$structtx__pbd.html" title="Definition of a TX payload buffer descriptor." alt="" coords="849,2439,969,2593"/>
<area shape="rect" id="node63" href="$structtx__hd.html" title="Definition of a TX header descriptor." alt="" coords="748,688,911,1120"/>
<area shape="rect" id="node65" href="$structba__ssc__bitmap.html" title="Structure of generic BA SSC + bitmap." alt="" coords="313,853,433,955"/>
<area shape="rect" id="node70" href="$structbar__frame.html" title="Structure of a Block Acknowledgment Request frame." alt="" coords="100,844,239,964"/>
<area shape="rect" id="node75" href="$structba__ssc__bitmap__256.html" title="Structure of BA SSC + 256&#45;bit bitmap." alt="" coords="572,853,724,955"/>
<area shape="rect" id="node81" href="$structtx__cfm__tag.html" title="Structure indicating the status and other information about the transmission." alt="" coords="1032,809,1147,999"/>
<area shape="rect" id="node86" href="$structtxl__frame__cfm__tag.html" title="TX frame confirmation descriptor." alt="" coords="376,2465,525,2567"/>
</map>
