# me_config_req Struct Reference
[TASK_ME]

Structure containing the parameters of the ME_CONFIG_REQ message. More...

`#include <me_task.h>`

Collaboration diagram for me_config_req:
[legend]

## Data Fields
struct mac_htcapability | ht_cap
| HT Capabilities.
struct mac_vhtcapability | vht_cap
| VHT Capabilities.
struct mac_hecapability | he_cap
| HE capabilities.
uint16_t | tx_lft
| Lifetime of packets sent under a BlockAck agreement (expressed in TUs).
uint8_t | phy_bw_max
| Maximum supported BW.
bool | ht_supp
| Boolean indicating if HT is supported or not.
bool | vht_supp
| Boolean indicating if VHT is supported or not.
bool | he_supp
| Boolean indicating if HE is supported or not.
bool | he_ul_on
| Boolean indicating if HE OFDMA UL is enabled or not.
bool | ps_on
| Boolean indicating if PS mode shall be enabled or not.
bool | ant_div_on
| Boolean indicating if Antenna Diversity shall be enabled or not.
bool | dpsm
| Boolean indicating if Dynamic PS mode shall be used or not.

## Detailed Description

Structure containing the parameters of the ME_CONFIG_REQ message.

Definition at line 105 of file me_task.h.

The documentation for this struct was generated from the following file:

- /space/home/slher/rel/Beken/v6_4_5/macsw/ip/umac/src/me/me_task.h